// SPDX-License-Identifier: GPL-2.0
//
// Copyright 2014 Freescale Semiconductor, Inc.

#include <dt-bindings/clock/imx6sx-clock.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include "imx6sx-pinfunc.h"

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	/*
	 * The decompressor and also some bootloaders rely on a
	 * pre-existing /chosen node to be available to insert the
	 * command line and merge other ATAGS info.
	 */
	chosen {};

	aliases {
		can0 = &flexcan1;
		can1 = &flexcan2;
		ethernet0 = &fec1;
		ethernet1 = &fec2;
		gpio0 = &gpio1;
		gpio1 = &gpio2;
		gpio2 = &gpio3;
		gpio3 = &gpio4;
		gpio4 = &gpio5;
		gpio5 = &gpio6;
		gpio6 = &gpio7;
		i2c0 = &i2c1;
		i2c1 = &i2c2;
		i2c2 = &i2c3;
		i2c3 = &i2c4;
		mmc0 = &usdhc1;
		mmc1 = &usdhc2;
		mmc2 = &usdhc3;
		mmc3 = &usdhc4;
		serial0 = &uart1;
		serial1 = &uart2;
		serial2 = &uart3;
		serial3 = &uart4;
		serial4 = &uart5;
		serial5 = &uart6;
		spi0 = &ecspi1;
		spi1 = &ecspi2;
		spi2 = &ecspi3;
		spi3 = &ecspi4;
		spi4 = &ecspi5;
		usb0 = &usbotg1;
		usb1 = &usbotg2;
		usb2 = &usbh;
		usbphy0 = &usbphy1;
		usbphy1 = &usbphy2;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			operating-points = <
				/* kHz    uV */
				996000  1250000
				792000  1175000
				396000  1075000
				198000	975000
			>;
			fsl,soc-operating-points = <
				/* ARM kHz  SOC uV */
				996000      1175000
				792000      1175000
				396000      1175000
				198000	    1175000
			>;
			clock-latency = <61036>; /* two CLK32 periods */
			#cooling-cells = <2>;
			clocks = <&clks IMX6SX_CLK_ARM>,
				 <&clks IMX6SX_CLK_PLL2_PFD2>,
				 <&clks IMX6SX_CLK_STEP>,
				 <&clks IMX6SX_CLK_PLL1_SW>,
				 <&clks IMX6SX_CLK_PLL1_SYS>;
			clock-names = "arm", "pll2_pfd2_396m", "step",
				      "pll1_sw", "pll1_sys";
			arm-supply = <&reg_arm>;
			soc-supply = <&reg_soc>;
			nvmem-cells = <&cpu_speed_grade>;
			nvmem-cell-names = "speed_grade";
		};
	};

	ckil: clock-ckil {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "ckil";
	};

	osc: clock-osc {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
		clock-output-names = "osc";
	};

	ipp_di0: clock-ipp-di0 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
		clock-output-names = "ipp_di0";
	};

	ipp_di1: clock-ipp-di1 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
		clock-output-names = "ipp_di1";
	};

	anaclk1: clock-anaclk1 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
		clock-output-names = "anaclk1";
	};

	anaclk2: clock-anaclk2 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
		clock-output-names = "anaclk2";
	};

	mqs: mqs {
		compatible = "fsl,imx6sx-mqs";
		gpr = <&gpr>;
		status = "disabled";
	};

	pmu {
		compatible = "arm,cortex-a9-pmu";
		interrupt-parent = <&gpc>;
		interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
	};

	usbphynop1: usbphynop1 {
		compatible = "usb-nop-xceiv";
		#phy-cells = <0>;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		interrupt-parent = <&gpc>;
		ranges;

		ocram_s: sram@8f8000 {
			compatible = "mmio-sram";
			reg = <0x008f8000 0x4000>;
			ranges = <0 0x008f8000 0x4000>;
			#address-cells = <1>;
			#size-cells = <1>;
			clocks = <&clks IMX6SX_CLK_OCRAM_S>;
		};

		ocram: sram@900000 {
			compatible = "mmio-sram";
			reg = <0x00900000 0x20000>;
			ranges = <0 0x00900000 0x20000>;
			#address-cells = <1>;
			#size-cells = <1>;
			clocks = <&clks IMX6SX_CLK_OCRAM>;
		};

		intc: interrupt-controller@a01000 {
			compatible = "arm,cortex-a9-gic";
			#interrupt-cells = <3>;
			interrupt-controller;
			reg = <0x00a01000 0x1000>,
			      <0x00a00100 0x100>;
			interrupt-parent = <&intc>;
		};

		L2: cache-controller@a02000 {
			compatible = "arm,pl310-cache";
			reg = <0x00a02000 0x1000>;
			interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
			cache-unified;
			cache-level = <2>;
			arm,tag-latency = <4 2 3>;
			arm,data-latency = <4 2 3>;
		};

		gpu: gpu@1800000 {
			compatible = "vivante,gc";
			reg = <0x01800000 0x4000>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clks IMX6SX_CLK_GPU>,
				 <&clks IMX6SX_CLK_GPU>,
				 <&clks IMX6SX_CLK_GPU>;
			clock-names = "bus", "core", "shader";
			power-domains = <&pd_pu>;
		};

		dma_apbh: dma-controller@1804000 {
			compatible = "fsl,imx6sx-dma-apbh", "fsl,imx28-dma-apbh";
			reg = <0x01804000 0x2000>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			#dma-cells = <1>;
			dma-channels = <4>;
			clocks = <&clks IMX6SX_CLK_APBH_DMA>;
		};

		gpmi: nand-controller@1806000 {
			compatible = "fsl,imx6sx-gpmi-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x01806000 0x2000>, <0x01808000 0x4000>;
			reg-names = "gpmi-nand", "bch";
			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "bch";
			clocks = <&clks IMX6SX_CLK_GPMI_IO>,
				 <&clks IMX6SX_CLK_GPMI_APB>,
				 <&clks IMX6SX_CLK_GPMI_BCH>,
				 <&clks IMX6SX_CLK_GPMI_BCH_APB>,
				 <&clks IMX6SX_CLK_PER1_BCH>;
			clock-names = "gpmi_io", "gpmi_apb", "gpmi_bch",
				      "gpmi_bch_apb", "per1_bch";
			dmas = <&dma_apbh 0>;
			dma-names = "rx-tx";
			status = "disabled";
		};

		aips1: bus@2000000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02000000 0x100000>;
			ranges;

			spba-bus@2000000 {
				compatible = "fsl,spba-bus", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x02000000 0x40000>;
				ranges;

				spdif: spdif@2004000 {
					compatible = "fsl,imx6sx-spdif", "fsl,imx35-spdif";
					reg = <0x02004000 0x4000>;
					interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>;
					dmas = <&sdma 14 18 0>,
					       <&sdma 15 18 0>;
					dma-names = "rx", "tx";
					clocks = <&clks IMX6SX_CLK_SPDIF_GCLK>,
						 <&clks IMX6SX_CLK_OSC>,
						 <&clks IMX6SX_CLK_SPDIF>,
						 <&clks 0>, <&clks 0>, <&clks 0>,
						 <&clks IMX6SX_CLK_IPG>,
						 <&clks 0>, <&clks 0>,
						 <&clks IMX6SX_CLK_SPBA>;
					clock-names = "core", "rxtx0",
						      "rxtx1", "rxtx2",
						      "rxtx3", "rxtx4",
						      "rxtx5", "rxtx6",
						      "rxtx7", "spba";
					status = "disabled";
				};

				ecspi1: spi@2008000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02008000 0x4000>;
					interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI1>,
						 <&clks IMX6SX_CLK_ECSPI1>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi2: spi@200c000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x0200c000 0x4000>;
					interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI2>,
						 <&clks IMX6SX_CLK_ECSPI2>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi3: spi@2010000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02010000 0x4000>;
					interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI3>,
						 <&clks IMX6SX_CLK_ECSPI3>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi4: spi@2014000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02014000 0x4000>;
					interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI4>,
						 <&clks IMX6SX_CLK_ECSPI4>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				uart1: serial@2020000 {
					compatible = "fsl,imx6sx-uart",
						     "fsl,imx6q-uart", "fsl,imx21-uart";
					reg = <0x02020000 0x4000>;
					interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_UART_IPG>,
						 <&clks IMX6SX_CLK_UART_SERIAL>;
					clock-names = "ipg", "per";
					dmas = <&sdma 25 4 0>, <&sdma 26 4 0>;
					dma-names = "rx", "tx";
					status = "disabled";
				};

				esai: esai@2024000 {
					compatible = "fsl,imx35-esai";
					reg = <0x02024000 0x4000>;
					interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ESAI_IPG>,
						 <&clks IMX6SX_CLK_ESAI_EXTAL>,
						 <&clks IMX6SX_CLK_ESAI_IPG>,
						 <&clks IMX6SX_CLK_SPBA>;
					clock-names = "core", "extal",
						      "fsys", "spba";
					dmas = <&sdma 23 21 0>,
					       <&sdma 24 21 0>;
					dma-names = "rx", "tx";
					status = "disabled";
				};

				ssi1: ssi@2028000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x02028000 0x4000>;
					interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI1_IPG>,
						 <&clks IMX6SX_CLK_SSI1>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 37 1 0>, <&sdma 38 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				ssi2: ssi@202c000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x0202c000 0x4000>;
					interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI2_IPG>,
						 <&clks IMX6SX_CLK_SSI2>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 41 1 0>, <&sdma 42 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				ssi3: ssi@2030000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x02030000 0x4000>;
					interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI3_IPG>,
						 <&clks IMX6SX_CLK_SSI3>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 45 1 0>, <&sdma 46 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				asrc: asrc@2034000 {
					compatible = "fsl,imx6sx-asrc", "fsl,imx53-asrc";
					reg = <0x02034000 0x4000>;
					interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ASRC_IPG>,
						<&clks IMX6SX_CLK_ASRC_MEM>, <&clks 0>,
						<&clks 0>, <&clks 0>, <&clks 0>, <&clks 0>,
						<&clks 0>, <&clks 0>, <&clks 0>, <&clks 0>,
						<&clks 0>, <&clks 0>, <&clks 0>, <&clks 0>,
						<&clks IMX6SX_CLK_SPDIF>, <&clks 0>, <&clks 0>,
						<&clks IMX6SX_CLK_SPBA>;
					clock-names = "mem", "ipg", "asrck_0",
						"asrck_1", "asrck_2", "asrck_3", "asrck_4",
						"asrck_5", "asrck_6", "asrck_7", "asrck_8",
						"asrck_9", "asrck_a", "asrck_b", "asrck_c",
						"asrck_d", "asrck_e", "asrck_f", "spba";
					dmas = <&sdma 17 23 1>, <&sdma 18 23 1>,
					       <&sdma 19 23 1>, <&sdma 20 23 1>,
					       <&sdma 21 23 1>, <&sdma 22 23 1>;
					dma-names = "rxa", "rxb", "rxc",
						    "txa", "txb", "txc";
					fsl,asrc-rate = <48000>;
					fsl,asrc-width = <16>;
					status = "okay";
				};
			};

			pwm1: pwm@2080000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02080000 0x4000>;
				interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM1>,
					 <&clks IMX6SX_CLK_PWM1>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm2: pwm@2084000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02084000 0x4000>;
				interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM2>,
					 <&clks IMX6SX_CLK_PWM2>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm3: pwm@2088000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02088000 0x4000>;
				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM3>,
					 <&clks IMX6SX_CLK_PWM3>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm4: pwm@208c000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x0208c000 0x4000>;
				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM4>,
					 <&clks IMX6SX_CLK_PWM4>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			flexcan1: can@2090000 {
				compatible = "fsl,imx6sx-flexcan", "fsl,imx6q-flexcan";
				reg = <0x02090000 0x4000>;
				interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_CAN1_IPG>,
					 <&clks IMX6SX_CLK_CAN1_SERIAL>;
				clock-names = "ipg", "per";
				fsl,stop-mode = <&gpr 0x10 1>;
				status = "disabled";
			};

			flexcan2: can@2094000 {
				compatible = "fsl,imx6sx-flexcan", "fsl,imx6q-flexcan";
				reg = <0x02094000 0x4000>;
				interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_CAN2_IPG>,
					 <&clks IMX6SX_CLK_CAN2_SERIAL>;
				clock-names = "ipg", "per";
				fsl,stop-mode = <&gpr 0x10 2>;
				status = "disabled";
			};

			gpt: timer@2098000 {
				compatible = "fsl,imx6sx-gpt", "fsl,imx6dl-gpt";
				reg = <0x02098000 0x4000>;
				interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_GPT_BUS>,
					 <&clks IMX6SX_CLK_GPT_3M>;
				clock-names = "ipg", "per";
			};

			gpio1: gpio@209c000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x0209c000 0x4000>;
				interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 5 26>;
			};

			gpio2: gpio@20a0000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a0000 0x4000>;
				interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 31 20>;
			};

			gpio3: gpio@20a4000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a4000 0x4000>;
				interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 51 29>;
			};

			gpio4: gpio@20a8000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a8000 0x4000>;
				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 80 32>;
			};

			gpio5: gpio@20ac000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020ac000 0x4000>;
				interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 112 24>;
			};

			gpio6: gpio@20b0000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020b0000 0x4000>;
				interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 136 12>, <&iomuxc 12 158 11>;
			};

			gpio7: gpio@20b4000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020b4000 0x4000>;
				interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 148 10>, <&iomuxc 10 169 2>;
			};

			kpp: keypad@20b8000 {
				compatible = "fsl,imx6sx-kpp", "fsl,imx21-kpp";
				reg = <0x020b8000 0x4000>;
				interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				status = "disabled";
			};

			wdog1: watchdog@20bc000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x020bc000 0x4000>;
				interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
			};

			wdog2: watchdog@20c0000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x020c0000 0x4000>;
				interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				status = "disabled";
			};

			clks: clock-controller@20c4000 {
				compatible = "fsl,imx6sx-ccm";
				reg = <0x020c4000 0x4000>;
				interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
				#clock-cells = <1>;
				clocks = <&ckil>, <&osc>, <&ipp_di0>, <&ipp_di1>, <&anaclk1>, <&anaclk2>;
				clock-names = "ckil", "osc", "ipp_di0", "ipp_di1", "anaclk1", "anaclk2";
			};

			anatop: anatop@20c8000 {
				compatible = "fsl,imx6sx-anatop", "fsl,imx6q-anatop",
					     "syscon", "simple-mfd";
				reg = <0x020c8000 0x1000>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;

				reg_vdd1p1: regulator-1p1 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd1p1";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
					anatop-reg-offset = <0x110>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <4>;
					anatop-min-voltage = <800000>;
					anatop-max-voltage = <1375000>;
					anatop-enable-bit = <0>;
				};

				reg_vdd3p0: regulator-3p0 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd3p0";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <3150000>;
					regulator-always-on;
					anatop-reg-offset = <0x120>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2625000>;
					anatop-max-voltage = <3400000>;
					anatop-enable-bit = <0>;
				};

				reg_vdd2p5: regulator-2p5 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd2p5";
					regulator-min-microvolt = <2250000>;
					regulator-max-microvolt = <2750000>;
					regulator-always-on;
					anatop-reg-offset = <0x130>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2100000>;
					anatop-max-voltage = <2875000>;
					anatop-enable-bit = <0>;
				};

				reg_arm: regulator-vddcore {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddarm";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <0>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <24>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_pcie: regulator-vddpcie {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddpcie";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <9>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <26>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_soc: regulator-vddsoc {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddsoc";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <18>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <28>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				tempmon: tempmon {
					compatible = "fsl,imx6sx-tempmon", "fsl,imx6q-tempmon";
					interrupt-parent = <&gpc>;
					interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
					fsl,tempmon = <&anatop>;
					nvmem-cells = <&tempmon_calib>, <&tempmon_temp_grade>;
					nvmem-cell-names = "calib", "temp_grade";
					clocks = <&clks IMX6SX_CLK_PLL3_USB_OTG>;
				};
			};

			usbphy1: usbphy@20c9000 {
				compatible = "fsl,imx6sx-usbphy", "fsl,imx23-usbphy";
				reg = <0x020c9000 0x1000>;
				interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBPHY1>;
				fsl,anatop = <&anatop>;
			};

			usbphy2: usbphy@20ca000 {
				compatible = "fsl,imx6sx-usbphy", "fsl,imx23-usbphy";
				reg = <0x020ca000 0x1000>;
				interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBPHY2>;
				fsl,anatop = <&anatop>;
			};

			snvs: snvs@20cc000 {
				compatible = "fsl,sec-v4.0-mon", "syscon", "simple-mfd";
				reg = <0x020cc000 0x4000>;

				snvs_rtc: snvs-rtc-lp {
					compatible = "fsl,sec-v4.0-mon-rtc-lp";
					regmap = <&snvs>;
					offset = <0x34>;
					interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
				};

				snvs_poweroff: snvs-poweroff {
					compatible = "syscon-poweroff";
					regmap = <&snvs>;
					offset = <0x38>;
					value = <0x60>;
					mask = <0x60>;
					status = "disabled";
				};

				snvs_pwrkey: snvs-powerkey {
					compatible = "fsl,sec-v4.0-pwrkey";
					regmap = <&snvs>;
					interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
					linux,keycode = <KEY_POWER>;
					wakeup-source;
					status = "disabled";
				};
			};

			epit1: epit@20d0000 {
				reg = <0x020d0000 0x4000>;
				interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
			};

			epit2: epit@20d4000 {
				reg = <0x020d4000 0x4000>;
				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
			};

			src: reset-controller@20d8000 {
				compatible = "fsl,imx6sx-src", "fsl,imx51-src";
				reg = <0x020d8000 0x4000>;
				interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
				#reset-cells = <1>;
			};

			gpc: gpc@20dc000 {
				compatible = "fsl,imx6sx-gpc", "fsl,imx6q-gpc";
				reg = <0x020dc000 0x4000>;
				interrupt-controller;
				#interrupt-cells = <3>;
				interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-parent = <&intc>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				clock-names = "ipg";

				pgc {
					#address-cells = <1>;
					#size-cells = <0>;

					power-domain@0 {
						reg = <0>;
						#power-domain-cells = <0>;
					};

					pd_pu: power-domain@1 {
						reg = <1>;
						#power-domain-cells = <0>;
						power-supply = <&reg_soc>;
						clocks = <&clks IMX6SX_CLK_GPU>;
					};

					pd_disp: power-domain@2 {
						reg = <2>;
						#power-domain-cells = <0>;
						clocks = <&clks IMX6SX_CLK_PXP_AXI>,
							 <&clks IMX6SX_CLK_DISPLAY_AXI>,
							 <&clks IMX6SX_CLK_LCDIF1_PIX>,
							 <&clks IMX6SX_CLK_LCDIF_APB>,
							 <&clks IMX6SX_CLK_LCDIF2_PIX>,
							 <&clks IMX6SX_CLK_CSI>,
							 <&clks IMX6SX_CLK_VADC>;
					};

					pd_pci: power-domain@3 {
						reg = <3>;
						#power-domain-cells = <0>;
						power-supply = <&reg_pcie>;
					};
				};
			};

			iomuxc: pinctrl@20e0000 {
				compatible = "fsl,imx6sx-iomuxc";
				reg = <0x020e0000 0x4000>;
			};

			gpr: syscon@20e4000 {
				compatible = "fsl,imx6sx-iomuxc-gpr",
					     "fsl,imx6q-iomuxc-gpr", "syscon", "simple-mfd";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x020e4000 0x4000>;

				lvds_bridge: bridge@18 {
					compatible = "fsl,imx6sx-ldb";
					reg = <0x18 0x4>;
					clocks = <&clks IMX6SX_CLK_LDB_DI0>;
					clock-names = "ldb";
					status = "disabled";

					ports {
						#address-cells = <1>;
						#size-cells = <0>;

						port@0 {
							reg = <0>;

							ldb_from_lcdif1: endpoint {
							};
						};

						port@1 {
							reg = <1>;

							ldb_lvds_ch0: endpoint {
							};
						};
					};
				};
			};

			sdma: dma-controller@20ec000 {
				compatible = "fsl,imx6sx-sdma", "fsl,imx6q-sdma";
				reg = <0x020ec000 0x4000>;
				interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>,
					 <&clks IMX6SX_CLK_SDMA>;
				clock-names = "ipg", "ahb";
				#dma-cells = <3>;
				/* imx6sx reuses imx6q sdma firmware */
				fsl,sdma-ram-script-name = "imx/sdma/sdma-imx6q.bin";
			};
		};

		aips2: bus@2100000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02100000 0x100000>;
			ranges;

			crypto: crypto@2100000 {
				compatible = "fsl,sec-v4.0";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x2100000 0x10000>;
				ranges = <0 0x2100000 0x10000>;
				interrupt-parent = <&intc>;
				clocks = <&clks IMX6SX_CLK_CAAM_MEM>,
					 <&clks IMX6SX_CLK_CAAM_ACLK>,
					 <&clks IMX6SX_CLK_CAAM_IPG>,
					 <&clks IMX6SX_CLK_EIM_SLOW>;
				clock-names = "mem", "aclk", "ipg", "emi_slow";

				sec_jr0: jr@1000 {
					compatible = "fsl,sec-v4.0-job-ring";
					reg = <0x1000 0x1000>;
					interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
				};

				sec_jr1: jr@2000 {
					compatible = "fsl,sec-v4.0-job-ring";
					reg = <0x2000 0x1000>;
					interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
				};
			};

			usbotg1: usb@2184000 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184000 0x200>;
				interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbphy = <&usbphy1>;
				fsl,usbmisc = <&usbmisc 0>;
				ahb-burst-config = <0x0>;
				tx-burst-size-dword = <0x10>;
				rx-burst-size-dword = <0x10>;
				status = "disabled";
			};

			usbotg2: usb@2184200 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184200 0x200>;
				interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbphy = <&usbphy2>;
				fsl,usbmisc = <&usbmisc 1>;
				ahb-burst-config = <0x0>;
				tx-burst-size-dword = <0x10>;
				rx-burst-size-dword = <0x10>;
				status = "disabled";
			};

			usbh: usb@2184400 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184400 0x200>;
				interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbphy = <&usbphynop1>;
				fsl,usbmisc = <&usbmisc 2>;
				phy_type = "hsic";
				dr_mode = "host";
				ahb-burst-config = <0x0>;
				tx-burst-size-dword = <0x10>;
				rx-burst-size-dword = <0x10>;
				status = "disabled";
			};

			usbmisc: usbmisc@2184800 {
				#index-cells = <1>;
				compatible = "fsl,imx6sx-usbmisc", "fsl,imx6q-usbmisc";
				reg = <0x02184800 0x200>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
			};

			fec1: ethernet@2188000 {
				compatible = "fsl,imx6sx-fec", "fsl,imx6q-fec";
				reg = <0x02188000 0x4000>;
				interrupt-names = "int0", "pps";
				interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ENET>,
					 <&clks IMX6SX_CLK_ENET_AHB>,
					 <&clks IMX6SX_CLK_ENET_PTP>,
					 <&clks IMX6SX_CLK_ENET_REF>,
					 <&clks IMX6SX_CLK_ENET_PTP>;
				clock-names = "ipg", "ahb", "ptp",
					      "enet_clk_ref", "enet_out";
				fsl,num-tx-queues = <3>;
				fsl,num-rx-queues = <3>;
				fsl,stop-mode = <&gpr 0x10 3>;
				status = "disabled";
			};

			mlb: mlb@218c000 {
				reg = <0x0218c000 0x4000>;
				interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_MLB>;
				status = "disabled";
			};

			usdhc1: mmc@2190000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02190000 0x4000>;
				interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC1>,
					 <&clks IMX6SX_CLK_USDHC1>,
					 <&clks IMX6SX_CLK_USDHC1>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				fsl,tuning-start-tap = <20>;
				fsl,tuning-step = <2>;
				status = "disabled";
			};

			usdhc2: mmc@2194000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02194000 0x4000>;
				interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC2>,
					 <&clks IMX6SX_CLK_USDHC2>,
					 <&clks IMX6SX_CLK_USDHC2>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				fsl,tuning-start-tap = <20>;
				fsl,tuning-step = <2>;
				status = "disabled";
			};

			usdhc3: mmc@2198000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02198000 0x4000>;
				interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC3>,
					 <&clks IMX6SX_CLK_USDHC3>,
					 <&clks IMX6SX_CLK_USDHC3>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				fsl,tuning-start-tap = <20>;
				fsl,tuning-step = <2>;
				status = "disabled";
			};

			usdhc4: mmc@219c000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x0219c000 0x4000>;
				interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC4>,
					 <&clks IMX6SX_CLK_USDHC4>,
					 <&clks IMX6SX_CLK_USDHC4>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			i2c1: i2c@21a0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a0000 0x4000>;
				interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C1>;
				status = "disabled";
			};

			i2c2: i2c@21a4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a4000 0x4000>;
				interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C2>;
				status = "disabled";
			};

			i2c3: i2c@21a8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a8000 0x4000>;
				interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C3>;
				status = "disabled";
			};

			memory-controller@21b0000 {
				compatible = "fsl,imx6sx-mmdc", "fsl,imx6q-mmdc";
				reg = <0x021b0000 0x4000>;
				clocks = <&clks IMX6SX_CLK_MMDC_P0_IPG>;
			};

			fec2: ethernet@21b4000 {
				compatible = "fsl,imx6sx-fec", "fsl,imx6q-fec";
				reg = <0x021b4000 0x4000>;
				interrupt-names = "int0", "pps";
				interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ENET>,
					 <&clks IMX6SX_CLK_ENET_AHB>,
					 <&clks IMX6SX_CLK_ENET_PTP>,
					 <&clks IMX6SX_CLK_ENET2_REF_125M>,
					 <&clks IMX6SX_CLK_ENET_PTP>;
				clock-names = "ipg", "ahb", "ptp",
					      "enet_clk_ref", "enet_out";
				fsl,stop-mode = <&gpr 0x10 4>;
				status = "disabled";
			};

			weim: memory-controller@21b8000 {
				#address-cells = <2>;
				#size-cells = <1>;
				compatible = "fsl,imx6sx-weim", "fsl,imx6q-weim";
				reg = <0x021b8000 0x4000>;
				interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_EIM_SLOW>;
				fsl,weim-cs-gpr = <&gpr>;
				status = "disabled";
			};

			ocotp: efuse@21bc000 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "fsl,imx6sx-ocotp", "syscon";
				reg = <0x021bc000 0x4000>;
				clocks = <&clks IMX6SX_CLK_OCOTP>;

				cpu_speed_grade: speed-grade@10 {
					reg = <0x10 4>;
				};

				tempmon_calib: calib@38 {
					reg = <0x38 4>;
				};

				tempmon_temp_grade: temp-grade@20 {
					reg = <0x20 4>;
				};
			};

			sai1: sai@21d4000 {
				compatible = "fsl,imx6sx-sai";
				reg = <0x021d4000 0x4000>;
				interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_SAI1_IPG>,
					 <&clks IMX6SX_CLK_SAI1>,
					 <&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&sdma 31 24 0>, <&sdma 32 24 0>;
				status = "disabled";
			};

			audmux: audmux@21d8000 {
				compatible = "fsl,imx6sx-audmux", "fsl,imx31-audmux";
				reg = <0x021d8000 0x4000>;
				status = "disabled";
			};

			sai2: sai@21dc000 {
				compatible = "fsl,imx6sx-sai";
				reg = <0x021dc000 0x4000>;
				interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_SAI2_IPG>,
					 <&clks IMX6SX_CLK_SAI2>,
					 <&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&sdma 33 24 0>, <&sdma 34 24 0>;
				status = "disabled";
			};

			qspi1: spi@21e0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-qspi";
				reg = <0x021e0000 0x4000>, <0x60000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_QSPI1>,
					 <&clks IMX6SX_CLK_QSPI1>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			qspi2: spi@21e4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-qspi";
				reg = <0x021e4000 0x4000>, <0x70000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_QSPI2>,
					 <&clks IMX6SX_CLK_QSPI2>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			uart2: serial@21e8000 {
				compatible = "fsl,imx6sx-uart",
					     "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021e8000 0x4000>;
				interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 27 4 0>, <&sdma 28 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart3: serial@21ec000 {
				compatible = "fsl,imx6sx-uart",
					     "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021ec000 0x4000>;
				interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 29 4 0>, <&sdma 30 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart4: serial@21f0000 {
				compatible = "fsl,imx6sx-uart",
					     "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021f0000 0x4000>;
				interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 31 4 0>, <&sdma 32 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart5: serial@21f4000 {
				compatible = "fsl,imx6sx-uart",
					     "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021f4000 0x4000>;
				interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 33 4 0>, <&sdma 34 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			i2c4: i2c@21f8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021f8000 0x4000>;
				interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C4>;
				status = "disabled";
			};
		};

		aips3: bus@2200000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02200000 0x100000>;
			ranges;

			spba-bus@2240000 {
				compatible = "fsl,spba-bus", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x02240000 0x40000>;
				ranges;

				csi1: csi@2214000 {
					reg = <0x02214000 0x4000>;
					interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_DISPLAY_AXI>,
						 <&clks IMX6SX_CLK_CSI>,
						 <&clks IMX6SX_CLK_DCIC1>;
					clock-names = "disp-axi", "csi_mclk", "dcic";
					status = "disabled";
				};

				pxp: pxp@2218000 {
					compatible = "fsl,imx6sx-pxp", "fsl,imx6ull-pxp";
					reg = <0x02218000 0x4000>;
					interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_PXP_AXI>;
					clock-names = "axi";
					power-domains = <&pd_disp>;
					status = "disabled";
				};

				csi2: csi@221c000 {
					reg = <0x0221c000 0x4000>;
					interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_DISPLAY_AXI>,
						 <&clks IMX6SX_CLK_CSI>,
						 <&clks IMX6SX_CLK_DCIC2>;
					clock-names = "disp-axi", "csi_mclk", "dcic";
					status = "disabled";
				};

				lcdif1: lcdif@2220000 {
					compatible = "fsl,imx6sx-lcdif", "fsl,imx28-lcdif";
					reg = <0x02220000 0x4000>;
					interrupts = <GIC_SPI 5 IRQ_TYPE_EDGE_RISING>;
					clocks = <&clks IMX6SX_CLK_LCDIF1_PIX>,
						 <&clks IMX6SX_CLK_LCDIF_APB>,
						 <&clks IMX6SX_CLK_DISPLAY_AXI>;
					clock-names = "pix", "axi", "disp_axi";
					assigned-clocks = <&clks IMX6SX_CLK_LCDIF1_PRE_SEL>,
							  <&clks IMX6SX_CLK_LCDIF1_SEL>;
					assigned-clock-parents = <&clks IMX6SX_CLK_PLL5_VIDEO_DIV>,
								 <&clks IMX6SX_CLK_LCDIF1_PODF>;
					power-domains = <&pd_disp>;
					status = "disabled";

					port {
						lcdif1_to_ldb: endpoint {
						};
					};
				};

				lcdif2: lcdif@2224000 {
					compatible = "fsl,imx6sx-lcdif", "fsl,imx28-lcdif";
					reg = <0x02224000 0x4000>;
					interrupts = <GIC_SPI 6 IRQ_TYPE_EDGE_RISING>;
					clocks = <&clks IMX6SX_CLK_LCDIF2_PIX>,
						 <&clks IMX6SX_CLK_LCDIF_APB>,
						 <&clks IMX6SX_CLK_DISPLAY_AXI>;
					clock-names = "pix", "axi", "disp_axi";
					power-domains = <&pd_disp>;
					status = "disabled";
				};

				vadc: vadc@2228000 {
					reg = <0x02228000 0x4000>, <0x0222c000 0x4000>;
					reg-names = "vadc-vafe", "vadc-vdec";
					clocks = <&clks IMX6SX_CLK_VADC>,
						 <&clks IMX6SX_CLK_CSI>;
					clock-names = "vadc", "csi";
					power-domains = <&pd_disp>;
					status = "disabled";
				};
			};

			adc1: adc@2280000 {
				compatible = "fsl,imx6sx-adc", "fsl,vf610-adc";
				reg = <0x02280000 0x4000>;
				interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				clock-names = "adc";
				fsl,adck-max-frequency = <30000000>, <40000000>,
							 <20000000>;
				status = "disabled";
			};

			adc2: adc@2284000 {
				compatible = "fsl,imx6sx-adc", "fsl,vf610-adc";
				reg = <0x02284000 0x4000>;
				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				clock-names = "adc";
				fsl,adck-max-frequency = <30000000>, <40000000>,
							 <20000000>;
				status = "disabled";
			};

			wdog3: watchdog@2288000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x02288000 0x4000>;
				interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				status = "disabled";
			};

			ecspi5: spi@228c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
				reg = <0x0228c000 0x4000>;
				interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ECSPI5>,
					 <&clks IMX6SX_CLK_ECSPI5>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart6: serial@22a0000 {
				compatible = "fsl,imx6sx-uart",
					     "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x022a0000 0x4000>;
				interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 0 4 0>, <&sdma 47 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			pwm5: pwm@22a4000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022a4000 0x4000>;
				interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM5>,
					 <&clks IMX6SX_CLK_PWM5>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm6: pwm@22a8000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022a8000 0x4000>;
				interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM6>,
					 <&clks IMX6SX_CLK_PWM6>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm7: pwm@22ac000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022ac000 0x4000>;
				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM7>,
					 <&clks IMX6SX_CLK_PWM7>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};

			pwm8: pwm@22b0000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022b0000 0x4000>;
				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM8>,
					 <&clks IMX6SX_CLK_PWM8>;
				clock-names = "ipg", "per";
				#pwm-cells = <3>;
			};
		};

		pcie: pcie@8ffc000 {
			compatible = "fsl,imx6sx-pcie";
			reg = <0x08ffc000 0x04000>, <0x08f00000 0x80000>;
			reg-names = "dbi", "config";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			bus-range = <0x00 0xff>;
			ranges = <0x81000000 0 0          0x08f80000 0 0x00010000>, /* downstream I/O */
				 <0x82000000 0 0x08000000 0x08000000 0 0x00f00000>; /* non-prefetchable memory */
			num-lanes = <1>;
			interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &gpc GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>,
					<0 0 0 2 &gpc GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>,
					<0 0 0 3 &gpc GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
					<0 0 0 4 &gpc GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clks IMX6SX_CLK_PCIE_AXI>,
				 <&clks IMX6SX_CLK_LVDS1_OUT>,
				 <&clks IMX6SX_CLK_PCIE_REF_125M>,
				 <&clks IMX6SX_CLK_DISPLAY_AXI>;
			clock-names = "pcie", "pcie_bus", "pcie_phy", "pcie_inbound_axi";
			power-domains = <&pd_disp>, <&pd_pci>;
			power-domain-names = "pcie", "pcie_phy";
			status = "disabled";
		};
	};
};
