// SPDX-License-Identifier: GPL-2.0+ OR MIT
//
// Copyright (C) 2015 Freescale Semiconductor, Inc.

/dts-v1/;

#include "imx7d.dtsi"

/ {
	model = "Freescale i.MX7 SabreSD Board";
	compatible = "fsl,imx7d-sdb", "fsl,imx7d";

	aliases {
		ethernet0 = &fec1;
		ethernet1 = &fec2;
	};

	chosen {
		stdout-path = &uart1;
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0x80000000>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_gpio_keys>;

		key-volume-up {
			label = "Volume Up";
			gpios = <&gpio5 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEUP>;
			wakeup-source;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio5 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEDOWN>;
			wakeup-source;
		};
	};

	spi-4 {
		compatible = "spi-gpio";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_spi4>;
		sck-gpios = <&gpio1 13 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio1 9 GPIO_ACTIVE_HIGH>;
		cs-gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
		num-chipselects = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		extended_io: gpio-expander@0 {
			compatible = "fairchild,74hc595";
			gpio-controller;
			#gpio-cells = <2>;
			reg = <0>;
			registers-number = <1>;
			spi-max-frequency = <100000>;
		};
	};

	reg_sd1_vmmc: regulator-sd1-vmmc {
		compatible = "regulator-fixed";
		regulator-name = "VDD_SD1";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio5 2 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		startup-delay-us = <200000>;
		off-on-delay-us = <20000>;
	};

	reg_usb_otg1_vbus: regulator-usb-otg1-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_otg1_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio1 5 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	reg_usb_otg2_vbus: regulator-usb-otg2-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_otg2_vbus";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_usb_otg2_vbus_reg>;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio1 7 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	reg_vref_1v8: regulator-vref-1v8 {
		compatible = "regulator-fixed";
		regulator-name = "vref-1v8";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	reg_brcm: regulator-brcm {
		compatible = "regulator-fixed";
		gpio = <&gpio4 21 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-name = "brcm_reg";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_brcm_reg>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <200000>;
	};

	reg_lcd_3v3: regulator-lcd-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "lcd-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&extended_io 7 GPIO_ACTIVE_LOW>;
	};

	reg_can2_3v3: regulator-can2-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "can2-3v3";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_flexcan2_reg>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio2 14 GPIO_ACTIVE_LOW>;
	};

	reg_fec2_3v3: regulator-fec2-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "fec2-3v3";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_enet2_reg>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio1 4 GPIO_ACTIVE_LOW>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 5000000 0>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <6>;
		status = "okay";
	};

	panel {
		compatible = "innolux,at043tn24";
		backlight = <&backlight>;
		power-supply = <&reg_lcd_3v3>;

		port {
			panel_in: endpoint {
				remote-endpoint = <&display_out>;
			};
		};
	};

	sound {
		compatible = "fsl,imx7d-evk-wm8960",
			     "fsl,imx-audio-wm8960";
		model = "wm8960-audio";
		audio-cpu = <&sai1>;
		audio-codec = <&codec>;
		hp-det-gpio = <&gpio2 28 GPIO_ACTIVE_HIGH>;
		audio-routing =
			"Headphone Jack", "HP_L",
			"Headphone Jack", "HP_R",
			"Ext Spk", "SPK_LP",
			"Ext Spk", "SPK_LN",
			"Ext Spk", "SPK_RP",
			"Ext Spk", "SPK_RN",
			"LINPUT1", "AMIC",
			"AMIC", "MICB";
	};

	sound-hdmi {
		compatible = "fsl,imx-audio-sii902x";
		model = "sii902x-audio";
		audio-cpu = <&sai3>;
		hdmi-out;
	};
};

&adc1 {
	vref-supply = <&reg_vref_1v8>;
	status = "okay";
};

&adc2 {
	vref-supply = <&reg_vref_1v8>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&sw1a_reg>;
};

&cpu1 {
	cpu-supply = <&sw1a_reg>;
};

&ecspi3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi3>;
	cs-gpios = <&gpio5 9 GPIO_ACTIVE_LOW>;
	status = "okay";

	tsc2046@0 {
		compatible = "ti,tsc2046";
		reg = <0>;
		spi-max-frequency = <1000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tsc2046_pendown>;
		interrupt-parent = <&gpio2>;
		interrupts = <29 0>;
		pendown-gpio = <&gpio2 29 GPIO_ACTIVE_LOW>;
		touchscreen-max-pressure = <255>;
		wakeup-source;
	};
};

&fec1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet1>;
	assigned-clocks = <&clks IMX7D_ENET1_TIME_ROOT_SRC>,
			  <&clks IMX7D_ENET1_TIME_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_ENET_MAIN_100M_CLK>;
	assigned-clock-rates = <0>, <100000000>;
	phy-mode = "rgmii";
	phy-handle = <&ethphy0>;
	fsl,magic-packet;
	phy-reset-gpios = <&extended_io 5 GPIO_ACTIVE_LOW>;
	status = "okay";

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;

		ethphy0: ethernet-phy@0 {
			reg = <0>;
		};

		ethphy1: ethernet-phy@1 {
			reg = <1>;
		};
	};
};

&fec2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet2>;
	assigned-clocks = <&clks IMX7D_ENET2_TIME_ROOT_SRC>,
			  <&clks IMX7D_ENET2_TIME_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_ENET_MAIN_100M_CLK>;
	assigned-clock-rates = <0>, <100000000>;
	phy-mode = "rgmii";
	phy-handle = <&ethphy1>;
	phy-supply = <&reg_fec2_3v3>;
	fsl,magic-packet;
	status = "okay";
};

&flexcan2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan2>;
	xceiver-supply = <&reg_can2_3v3>;
	status = "okay";
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	pmic: pmic@8 {
		compatible = "fsl,pfuze3000";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1a {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			/* use sw1c_reg to align with pfuze100/pfuze200 */
			sw1c_reg: sw1b {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3 {
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1650000>;
				regulator-boot-on;
				regulator-always-on;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vldo1 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen2_reg: vldo2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vccsd {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen4_reg: v33 {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vldo3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vldo4 {
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
				regulator-always-on;
			};
		};
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	mpl3115@60 {
		compatible = "fsl,mpl3115";
		reg = <0x60>;
	};
};

&i2c3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";
};

&i2c4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c4>;
	status = "okay";

	codec: wm8960@1a {
		compatible = "wlf,wm8960";
		reg = <0x1a>;
		clocks = <&clks IMX7D_AUDIO_MCLK_ROOT_DIV>;
		clock-names = "mclk";
		wlf,shared-lrclk;
		wlf,hp-cfg = <2 2 3>;
		wlf,gpio-cfg = <1 3>;
		assigned-clocks = <&clks IMX7D_AUDIO_MCLK_ROOT_SRC>,
				  <&clks IMX7D_PLL_AUDIO_POST_DIV>,
				  <&clks IMX7D_AUDIO_MCLK_ROOT_DIV>;
		assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
		assigned-clock-rates = <0>, <884736000>, <12288000>;
	};
};

&lcdif {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_lcdif>;
	status = "okay";

	port {
		display_out: endpoint {
			remote-endpoint = <&panel_in>;
		};
	};
};

&pcie {
	reset-gpio = <&extended_io 1 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&reg_1p0d {
	vin-supply = <&sw2_reg>;
};

&reg_1p2 {
	vin-supply = <&sw2_reg>;
};

&sai1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai1>;
	assigned-clocks = <&clks IMX7D_SAI1_ROOT_SRC>,
			  <&clks IMX7D_PLL_AUDIO_POST_DIV>,
			  <&clks IMX7D_SAI1_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <0>, <884736000>, <36864000>;
	status = "okay";
};

&sai3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai3 &pinctrl_sai3_mclk>;
	assigned-clocks = <&clks IMX7D_SAI3_ROOT_SRC>,
			  <&clks IMX7D_PLL_AUDIO_POST_DIV>,
			  <&clks IMX7D_SAI3_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <0>, <884736000>, <36864000>;
	status = "okay";
};

&snvs_pwrkey {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	assigned-clocks = <&clks IMX7D_UART1_ROOT_SRC>;
	assigned-clock-parents = <&clks IMX7D_PLL_SYS_MAIN_240M_CLK>;
	status = "okay";
};

&uart6 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart6>;
	assigned-clocks = <&clks IMX7D_UART6_ROOT_SRC>;
	assigned-clock-parents = <&clks IMX7D_PLL_SYS_MAIN_240M_CLK>;
	uart-has-rtscts;
	status = "okay";
};

&usbotg1 {
	vbus-supply = <&reg_usb_otg1_vbus>;
	status = "okay";
};

&usbotg2 {
	vbus-supply = <&reg_usb_otg2_vbus>;
	dr_mode = "host";
	status = "okay";
};

&usdhc1 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc1>, <&pinctrl_usdhc1_gpio>;
	pinctrl-1 = <&pinctrl_usdhc1_100mhz>, <&pinctrl_usdhc1_gpio>;
	pinctrl-2 = <&pinctrl_usdhc1_200mhz>, <&pinctrl_usdhc1_gpio>;
	cd-gpios = <&gpio5 0 GPIO_ACTIVE_LOW>;
	wp-gpios = <&gpio5 1 GPIO_ACTIVE_HIGH>;
	vmmc-supply = <&reg_sd1_vmmc>;
	wakeup-source;
	keep-power-in-suspend;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc2>;
	pinctrl-1 = <&pinctrl_usdhc2_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc2_200mhz>;
	wakeup-source;
	keep-power-in-suspend;
	non-removable;
	vmmc-supply = <&reg_brcm>;
	fsl,tuning-step = <2>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc3>;
	pinctrl-1 = <&pinctrl_usdhc3_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc3_200mhz>;
	assigned-clocks = <&clks IMX7D_USDHC3_ROOT_CLK>;
	assigned-clock-rates = <400000000>;
	bus-width = <8>;
	fsl,tuning-step = <2>;
	non-removable;
	status = "okay";
};

&wdog1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_wdog>;
	fsl,ext-reset-output;
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	pinctrl_brcm_reg: brcmreggrp {
		fsl,pins = <
			MX7D_PAD_ECSPI2_MOSI__GPIO4_IO21	0x14
		>;
	};

	pinctrl_ecspi3: ecspi3grp {
		fsl,pins = <
			MX7D_PAD_SAI2_TX_SYNC__ECSPI3_MISO	0x2
			MX7D_PAD_SAI2_TX_BCLK__ECSPI3_MOSI	0x2
			MX7D_PAD_SAI2_RX_DATA__ECSPI3_SCLK	0x2
			MX7D_PAD_SD2_CD_B__GPIO5_IO9		0x59
		>;
	};

	pinctrl_enet1: enet1grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO10__ENET1_MDIO			0x3
			MX7D_PAD_GPIO1_IO11__ENET1_MDC			0x3
			MX7D_PAD_ENET1_RGMII_TXC__ENET1_RGMII_TXC	0x1
			MX7D_PAD_ENET1_RGMII_TD0__ENET1_RGMII_TD0	0x1
			MX7D_PAD_ENET1_RGMII_TD1__ENET1_RGMII_TD1	0x1
			MX7D_PAD_ENET1_RGMII_TD2__ENET1_RGMII_TD2	0x1
			MX7D_PAD_ENET1_RGMII_TD3__ENET1_RGMII_TD3	0x1
			MX7D_PAD_ENET1_RGMII_TX_CTL__ENET1_RGMII_TX_CTL	0x1
			MX7D_PAD_ENET1_RGMII_RXC__ENET1_RGMII_RXC	0x1
			MX7D_PAD_ENET1_RGMII_RD0__ENET1_RGMII_RD0	0x1
			MX7D_PAD_ENET1_RGMII_RD1__ENET1_RGMII_RD1	0x1
			MX7D_PAD_ENET1_RGMII_RD2__ENET1_RGMII_RD2	0x1
			MX7D_PAD_ENET1_RGMII_RD3__ENET1_RGMII_RD3	0x1
			MX7D_PAD_ENET1_RGMII_RX_CTL__ENET1_RGMII_RX_CTL	0x1
		>;
	};

	pinctrl_enet2: enet2grp {
		fsl,pins = <
			MX7D_PAD_EPDC_GDSP__ENET2_RGMII_TXC		0x1
			MX7D_PAD_EPDC_SDCE2__ENET2_RGMII_TD0		0x1
			MX7D_PAD_EPDC_SDCE3__ENET2_RGMII_TD1		0x1
			MX7D_PAD_EPDC_GDCLK__ENET2_RGMII_TD2		0x1
			MX7D_PAD_EPDC_GDOE__ENET2_RGMII_TD3		0x1
			MX7D_PAD_EPDC_GDRL__ENET2_RGMII_TX_CTL		0x1
			MX7D_PAD_EPDC_SDCE1__ENET2_RGMII_RXC		0x1
			MX7D_PAD_EPDC_SDCLK__ENET2_RGMII_RD0		0x1
			MX7D_PAD_EPDC_SDLE__ENET2_RGMII_RD1		0x1
			MX7D_PAD_EPDC_SDOE__ENET2_RGMII_RD2		0x1
			MX7D_PAD_EPDC_SDSHR__ENET2_RGMII_RD3		0x1
			MX7D_PAD_EPDC_SDCE0__ENET2_RGMII_RX_CTL		0x1
		>;
	};

	pinctrl_enet2_reg: enet2reggrp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO04__GPIO1_IO4	0x14
		>;
	};

	pinctrl_flexcan2: flexcan2grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO14__FLEXCAN2_RX	0x59
			MX7D_PAD_GPIO1_IO15__FLEXCAN2_TX	0x59
		>;
	};

	pinctrl_flexcan2_reg: flexcan2reggrp {
		fsl,pins = <
			MX7D_PAD_EPDC_DATA14__GPIO2_IO14	0x59	/* CAN_STBY */
		>;
	};

	pinctrl_gpio_keys: gpio-keysgrp {
		fsl,pins = <
			MX7D_PAD_SD2_RESET_B__GPIO5_IO11	0x59
			MX7D_PAD_SD2_WP__GPIO5_IO10		0x59
		>;
	};

	pinctrl_hog: hoggrp {
		fsl,pins = <
			MX7D_PAD_ECSPI2_SS0__GPIO4_IO23		0x34  /* bt reg on */
			MX7D_PAD_EPDC_BDR0__GPIO2_IO28		0x59  /* headphone detect */
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX7D_PAD_I2C1_SDA__I2C1_SDA		0x4000007f
			MX7D_PAD_I2C1_SCL__I2C1_SCL		0x4000007f
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX7D_PAD_I2C2_SDA__I2C2_SDA		0x4000007f
			MX7D_PAD_I2C2_SCL__I2C2_SCL		0x4000007f
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX7D_PAD_I2C3_SDA__I2C3_SDA		0x4000007f
			MX7D_PAD_I2C3_SCL__I2C3_SCL		0x4000007f
		>;
	};

	pinctrl_i2c4: i2c4grp {
		fsl,pins = <
			MX7D_PAD_SAI1_RX_BCLK__I2C4_SDA		0x4000007f
			MX7D_PAD_SAI1_RX_SYNC__I2C4_SCL		0x4000007f
		>;
	};

	pinctrl_lcdif: lcdifgrp {
		fsl,pins = <
			MX7D_PAD_LCD_DATA00__LCD_DATA0		0x79
			MX7D_PAD_LCD_DATA01__LCD_DATA1		0x79
			MX7D_PAD_LCD_DATA02__LCD_DATA2		0x79
			MX7D_PAD_LCD_DATA03__LCD_DATA3		0x79
			MX7D_PAD_LCD_DATA04__LCD_DATA4		0x79
			MX7D_PAD_LCD_DATA05__LCD_DATA5		0x79
			MX7D_PAD_LCD_DATA06__LCD_DATA6		0x79
			MX7D_PAD_LCD_DATA07__LCD_DATA7		0x79
			MX7D_PAD_LCD_DATA08__LCD_DATA8		0x79
			MX7D_PAD_LCD_DATA09__LCD_DATA9		0x79
			MX7D_PAD_LCD_DATA10__LCD_DATA10		0x79
			MX7D_PAD_LCD_DATA11__LCD_DATA11		0x79
			MX7D_PAD_LCD_DATA12__LCD_DATA12		0x79
			MX7D_PAD_LCD_DATA13__LCD_DATA13		0x79
			MX7D_PAD_LCD_DATA14__LCD_DATA14		0x79
			MX7D_PAD_LCD_DATA15__LCD_DATA15		0x79
			MX7D_PAD_LCD_DATA16__LCD_DATA16		0x79
			MX7D_PAD_LCD_DATA17__LCD_DATA17		0x79
			MX7D_PAD_LCD_DATA18__LCD_DATA18		0x79
			MX7D_PAD_LCD_DATA19__LCD_DATA19		0x79
			MX7D_PAD_LCD_DATA20__LCD_DATA20		0x79
			MX7D_PAD_LCD_DATA21__LCD_DATA21		0x79
			MX7D_PAD_LCD_DATA22__LCD_DATA22		0x79
			MX7D_PAD_LCD_DATA23__LCD_DATA23		0x79
			MX7D_PAD_LCD_CLK__LCD_CLK		0x79
			MX7D_PAD_LCD_ENABLE__LCD_ENABLE		0x79
			MX7D_PAD_LCD_VSYNC__LCD_VSYNC		0x79
			MX7D_PAD_LCD_HSYNC__LCD_HSYNC		0x79
			MX7D_PAD_LCD_RESET__LCD_RESET		0x79
		>;
	};

	pinctrl_sai1: sai1grp {
		fsl,pins = <
			MX7D_PAD_SAI1_MCLK__SAI1_MCLK           0x1f
			MX7D_PAD_ENET1_RX_CLK__SAI1_TX_BCLK     0x1f
			MX7D_PAD_ENET1_CRS__SAI1_TX_SYNC	0x1f
			MX7D_PAD_ENET1_COL__SAI1_TX_DATA0	0x30
			MX7D_PAD_ENET1_TX_CLK__SAI1_RX_DATA0	0x1f
		>;
	};

	pinctrl_sai2: sai2grp {
		fsl,pins = <
			MX7D_PAD_SAI2_TX_BCLK__SAI2_TX_BCLK     0x1f
			MX7D_PAD_SAI2_TX_SYNC__SAI2_TX_SYNC     0x1f
			MX7D_PAD_SAI2_TX_DATA__SAI2_TX_DATA0    0x30
			MX7D_PAD_SAI2_RX_DATA__SAI2_RX_DATA0    0x1f
		>;
	};

	pinctrl_sai3: sai3grp {
		fsl,pins = <
			MX7D_PAD_UART3_TX_DATA__SAI3_TX_BCLK   0x1f
			MX7D_PAD_UART3_CTS_B__SAI3_TX_SYNC     0x1f
			MX7D_PAD_UART3_RTS_B__SAI3_TX_DATA0    0x30
		>;
	};

	pinctrl_spi4: spi4grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO09__GPIO1_IO9	0x59
			MX7D_PAD_GPIO1_IO12__GPIO1_IO12	0x59
			MX7D_PAD_GPIO1_IO13__GPIO1_IO13	0x59
		>;
	};

	pinctrl_tsc2046_pendown: tsc2046-pendowngrp {
		fsl,pins = <
			MX7D_PAD_EPDC_BDR1__GPIO2_IO29		0x59
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX7D_PAD_UART1_TX_DATA__UART1_DCE_TX	0x79
			MX7D_PAD_UART1_RX_DATA__UART1_DCE_RX	0x79
		>;
	};

	pinctrl_uart5: uart5grp {
		fsl,pins = <
			MX7D_PAD_SAI1_TX_BCLK__UART5_DCE_TX	0x79
			MX7D_PAD_SAI1_RX_DATA__UART5_DCE_RX	0x79
			MX7D_PAD_SAI1_TX_SYNC__UART5_DCE_CTS	0x79
			MX7D_PAD_SAI1_TX_DATA__UART5_DCE_RTS	0x79
		>;
	};

	pinctrl_uart6: uart6grp {
		fsl,pins = <
			MX7D_PAD_ECSPI1_MOSI__UART6_DCE_TX	0x79
			MX7D_PAD_ECSPI1_SCLK__UART6_DCE_RX	0x79
			MX7D_PAD_ECSPI1_SS0__UART6_DCE_CTS	0x79
			MX7D_PAD_ECSPI1_MISO__UART6_DCE_RTS	0x79
		>;
	};

	pinctrl_usdhc1_gpio: usdhc1-gpiogrp {
		fsl,pins = <
			MX7D_PAD_SD1_CD_B__GPIO5_IO0		0x59 /* CD */
			MX7D_PAD_SD1_WP__GPIO5_IO1		0x59 /* WP */
			MX7D_PAD_SD1_RESET_B__GPIO5_IO2		0x59 /* vmmc */
			MX7D_PAD_GPIO1_IO08__SD1_VSELECT	0x59 /* VSELECT */
		>;
	};

	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <
			MX7D_PAD_SD1_CMD__SD1_CMD		0x59
			MX7D_PAD_SD1_CLK__SD1_CLK		0x19
			MX7D_PAD_SD1_DATA0__SD1_DATA0		0x59
			MX7D_PAD_SD1_DATA1__SD1_DATA1		0x59
			MX7D_PAD_SD1_DATA2__SD1_DATA2		0x59
			MX7D_PAD_SD1_DATA3__SD1_DATA3		0x59
		>;
	};

	pinctrl_usdhc1_100mhz: usdhc1-100mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD1_CMD__SD1_CMD		0x5a
			MX7D_PAD_SD1_CLK__SD1_CLK		0x1a
			MX7D_PAD_SD1_DATA0__SD1_DATA0		0x5a
			MX7D_PAD_SD1_DATA1__SD1_DATA1		0x5a
			MX7D_PAD_SD1_DATA2__SD1_DATA2		0x5a
			MX7D_PAD_SD1_DATA3__SD1_DATA3		0x5a
		>;
	};

	pinctrl_usdhc1_200mhz: usdhc1-200mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD1_CMD__SD1_CMD		0x5b
			MX7D_PAD_SD1_CLK__SD1_CLK		0x1b
			MX7D_PAD_SD1_DATA0__SD1_DATA0		0x5b
			MX7D_PAD_SD1_DATA1__SD1_DATA1		0x5b
			MX7D_PAD_SD1_DATA2__SD1_DATA2		0x5b
			MX7D_PAD_SD1_DATA3__SD1_DATA3		0x5b
		>;
	};

	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <
			MX7D_PAD_SD2_CMD__SD2_CMD		0x59
			MX7D_PAD_SD2_CLK__SD2_CLK		0x19
			MX7D_PAD_SD2_DATA0__SD2_DATA0		0x59
			MX7D_PAD_SD2_DATA1__SD2_DATA1		0x59
			MX7D_PAD_SD2_DATA2__SD2_DATA2		0x59
			MX7D_PAD_SD2_DATA3__SD2_DATA3		0x59
		>;
	};

	pinctrl_usdhc2_100mhz: usdhc2-100mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD2_CMD__SD2_CMD		0x5a
			MX7D_PAD_SD2_CLK__SD2_CLK		0x1a
			MX7D_PAD_SD2_DATA0__SD2_DATA0		0x5a
			MX7D_PAD_SD2_DATA1__SD2_DATA1		0x5a
			MX7D_PAD_SD2_DATA2__SD2_DATA2		0x5a
			MX7D_PAD_SD2_DATA3__SD2_DATA3		0x5a
		>;
	};

	pinctrl_usdhc2_200mhz: usdhc2-200mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD2_CMD__SD2_CMD		0x5b
			MX7D_PAD_SD2_CLK__SD2_CLK		0x1b
			MX7D_PAD_SD2_DATA0__SD2_DATA0		0x5b
			MX7D_PAD_SD2_DATA1__SD2_DATA1		0x5b
			MX7D_PAD_SD2_DATA2__SD2_DATA2		0x5b
			MX7D_PAD_SD2_DATA3__SD2_DATA3		0x5b
		>;
	};


	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX7D_PAD_SD3_CMD__SD3_CMD		0x59
			MX7D_PAD_SD3_CLK__SD3_CLK		0x19
			MX7D_PAD_SD3_DATA0__SD3_DATA0		0x59
			MX7D_PAD_SD3_DATA1__SD3_DATA1		0x59
			MX7D_PAD_SD3_DATA2__SD3_DATA2		0x59
			MX7D_PAD_SD3_DATA3__SD3_DATA3		0x59
			MX7D_PAD_SD3_DATA4__SD3_DATA4		0x59
			MX7D_PAD_SD3_DATA5__SD3_DATA5		0x59
			MX7D_PAD_SD3_DATA6__SD3_DATA6		0x59
			MX7D_PAD_SD3_DATA7__SD3_DATA7		0x59
			MX7D_PAD_SD3_STROBE__SD3_STROBE		0x19
		>;
	};

	pinctrl_usdhc3_100mhz: usdhc3-100mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD3_CMD__SD3_CMD		0x5a
			MX7D_PAD_SD3_CLK__SD3_CLK		0x1a
			MX7D_PAD_SD3_DATA0__SD3_DATA0		0x5a
			MX7D_PAD_SD3_DATA1__SD3_DATA1		0x5a
			MX7D_PAD_SD3_DATA2__SD3_DATA2		0x5a
			MX7D_PAD_SD3_DATA3__SD3_DATA3		0x5a
			MX7D_PAD_SD3_DATA4__SD3_DATA4		0x5a
			MX7D_PAD_SD3_DATA5__SD3_DATA5		0x5a
			MX7D_PAD_SD3_DATA6__SD3_DATA6		0x5a
			MX7D_PAD_SD3_DATA7__SD3_DATA7		0x5a
			MX7D_PAD_SD3_STROBE__SD3_STROBE		0x1a
		>;
	};

	pinctrl_usdhc3_200mhz: usdhc3-200mhz-grp {
		fsl,pins = <
			MX7D_PAD_SD3_CMD__SD3_CMD		0x5b
			MX7D_PAD_SD3_CLK__SD3_CLK		0x1b
			MX7D_PAD_SD3_DATA0__SD3_DATA0		0x5b
			MX7D_PAD_SD3_DATA1__SD3_DATA1		0x5b
			MX7D_PAD_SD3_DATA2__SD3_DATA2		0x5b
			MX7D_PAD_SD3_DATA3__SD3_DATA3		0x5b
			MX7D_PAD_SD3_DATA4__SD3_DATA4		0x5b
			MX7D_PAD_SD3_DATA5__SD3_DATA5		0x5b
			MX7D_PAD_SD3_DATA6__SD3_DATA6		0x5b
			MX7D_PAD_SD3_DATA7__SD3_DATA7		0x5b
			MX7D_PAD_SD3_STROBE__SD3_STROBE		0x1b
		>;
	};
};

&pwm1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>;
	status = "okay";
};

&iomuxc_lpsr {
	pinctrl_wdog: wdoggrp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO00__WDOG1_WDOG_B		0x74
		>;
	};

	pinctrl_pwm1: pwm1grp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO01__PWM1_OUT		0x30
		>;
	};

	pinctrl_usb_otg2_vbus_reg: usbotg2vbusreggrp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO07__GPIO1_IO7	  0x14
		>;
	};

	pinctrl_sai3_mclk: sai3-mclk-grp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO03__SAI3_MCLK	0x1f
		>;
	};
};
