// SPDX-License-Identifier: GPL-2.0 OR X11
/*
 * Device Tree Include file for TQ-Systems TQMa7x boards with full mounted PCB.
 *
 * Copyright (C) 2016 TQ-Systems GmbH
 * Author: Markus Niebel <Markus.Niebel@tq-group.com>
 * Copyright (C) 2019 Bruno Thomsen <bruno.thomsen@gmail.com>
 */

/ {
	memory@80000000 {
		device_type = "memory";
		/* 512 MB - default configuration */
		reg = <0x80000000 0x20000000>;
	};
};

&cpu0 {
	cpu-supply = <&sw1a_reg>;
};

&gpio2 {
	/* Configured as pullup by QSPI pin group */
	qspi-reset-hog {
		gpio-hog;
		gpios = <4 GPIO_ACTIVE_LOW>;
		input;
		line-name = "qspi-reset";
	};
};

&i2c1 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_i2c1>;
	pinctrl-1 = <&pinctrl_i2c1_recovery>;
	scl-gpios = <&gpio4 8 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio4 9 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	clock-frequency = <100000>;
	status = "okay";

	pfuze3000: pmic@8 {
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_pmic1>;
		compatible = "fsl,pfuze3000";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1a {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			/* use sw1c_reg to align with pfuze100/pfuze200 */
			sw1c_reg: sw1b {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1850000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3 {
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1650000>;
				regulator-boot-on;
				regulator-always-on;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vldo1 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen2_reg: vldo2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
				regulator-always-on;
			};

			vgen3_reg: vccsd {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen4_reg: v33 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vldo3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vldo4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};

	/* LM75A temperature sensor, TQMa7x 01xx */
	lm75a: temperature-sensor@48 {
		compatible = "national,lm75a";
		reg = <0x48>;
		vs-supply = <&vgen4_reg>;
	};

	/* NXP SE97BTP with temperature sensor + eeprom, TQMa7x 02xx */
	se97b: temperature-sensor@1e {
		compatible = "nxp,se97b", "jedec,jc-42.4-temp";
		reg = <0x1e>;
	};

	/* ST M24C64 */
	m24c64: eeprom@50 {
		compatible = "atmel,24c64";
		read-only;
		reg = <0x50>;
		pagesize = <32>;
		vcc-supply = <&vgen4_reg>;
		status = "okay";
	};

	at24c02: eeprom@56 {
		compatible = "nxp,se97b", "atmel,24c02";
		reg = <0x56>;
		pagesize = <16>;
		vcc-supply = <&vgen4_reg>;
		status = "okay";
	};

	ds1339: rtc@68 {
		compatible = "dallas,ds1339";
		reg = <0x68>;
	};
};

&iomuxc {
	pinctrl_i2c1: i2c1grp {
		fsl,pins =
			<MX7D_PAD_I2C1_SDA__I2C1_SDA	0x40000078>,
			<MX7D_PAD_I2C1_SCL__I2C1_SCL	0x40000078>;
	};

	pinctrl_i2c1_recovery: i2c1recoverygrp {
		fsl,pins =
			<MX7D_PAD_I2C1_SDA__GPIO4_IO9	0x40000078>,
			<MX7D_PAD_I2C1_SCL__GPIO4_IO8	0x40000078>;
	};

	pinctrl_pmic1: pmic1grp {
		fsl,pins =
			<MX7D_PAD_SD2_RESET_B__GPIO5_IO11	0x4000005C>;
	};

	pinctrl_qspi: qspigrp {
		fsl,pins =
			<MX7D_PAD_EPDC_DATA00__QSPI_A_DATA0	0x5A>,
			<MX7D_PAD_EPDC_DATA01__QSPI_A_DATA1	0x5A>,
			<MX7D_PAD_EPDC_DATA02__QSPI_A_DATA2	0x5A>,
			<MX7D_PAD_EPDC_DATA03__QSPI_A_DATA3	0x5A>,
			<MX7D_PAD_EPDC_DATA05__QSPI_A_SCLK	0x11>,
			<MX7D_PAD_EPDC_DATA06__QSPI_A_SS0_B	0x54>,
			<MX7D_PAD_EPDC_DATA07__QSPI_A_SS1_B	0x54>;
	};

	pinctrl_qspi_reset: qspi_resetgrp {
		fsl,pins =
			/* #QSPI_RESET */
			<MX7D_PAD_EPDC_DATA04__GPIO2_IO4	0x52>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins =
			<MX7D_PAD_SD3_CMD__SD3_CMD		0x59>,
			<MX7D_PAD_SD3_CLK__SD3_CLK		0x56>,
			<MX7D_PAD_SD3_DATA0__SD3_DATA0		0x59>,
			<MX7D_PAD_SD3_DATA1__SD3_DATA1		0x59>,
			<MX7D_PAD_SD3_DATA2__SD3_DATA2		0x59>,
			<MX7D_PAD_SD3_DATA3__SD3_DATA3		0x59>,
			<MX7D_PAD_SD3_DATA4__SD3_DATA4		0x59>,
			<MX7D_PAD_SD3_DATA5__SD3_DATA5		0x59>,
			<MX7D_PAD_SD3_DATA6__SD3_DATA6		0x59>,
			<MX7D_PAD_SD3_DATA7__SD3_DATA7		0x59>,
			<MX7D_PAD_SD3_STROBE__SD3_STROBE	0x19>;
	};

	pinctrl_usdhc3_100mhz: usdhc3_100mhzgrp {
		fsl,pins =
			<MX7D_PAD_SD3_CMD__SD3_CMD               0x5a>,
			<MX7D_PAD_SD3_CLK__SD3_CLK               0x51>,
			<MX7D_PAD_SD3_DATA0__SD3_DATA0           0x5a>,
			<MX7D_PAD_SD3_DATA1__SD3_DATA1           0x5a>,
			<MX7D_PAD_SD3_DATA2__SD3_DATA2           0x5a>,
			<MX7D_PAD_SD3_DATA3__SD3_DATA3           0x5a>,
			<MX7D_PAD_SD3_DATA4__SD3_DATA4           0x5a>,
			<MX7D_PAD_SD3_DATA5__SD3_DATA5           0x5a>,
			<MX7D_PAD_SD3_DATA6__SD3_DATA6           0x5a>,
			<MX7D_PAD_SD3_DATA7__SD3_DATA7           0x5a>,
			<MX7D_PAD_SD3_STROBE__SD3_STROBE         0x1a>;
	};

	pinctrl_usdhc3_200mhz: usdhc3_200mhzgrp {
		fsl,pins =
			<MX7D_PAD_SD3_CMD__SD3_CMD               0x5b>,
			<MX7D_PAD_SD3_CLK__SD3_CLK               0x51>,
			<MX7D_PAD_SD3_DATA0__SD3_DATA0           0x5b>,
			<MX7D_PAD_SD3_DATA1__SD3_DATA1           0x5b>,
			<MX7D_PAD_SD3_DATA2__SD3_DATA2           0x5b>,
			<MX7D_PAD_SD3_DATA3__SD3_DATA3           0x5b>,
			<MX7D_PAD_SD3_DATA4__SD3_DATA4           0x5b>,
			<MX7D_PAD_SD3_DATA5__SD3_DATA5           0x5b>,
			<MX7D_PAD_SD3_DATA6__SD3_DATA6           0x5b>,
			<MX7D_PAD_SD3_DATA7__SD3_DATA7           0x5b>,
			<MX7D_PAD_SD3_STROBE__SD3_STROBE         0x1b>;
	};
};

&iomuxc_lpsr {
	pinctrl_wdog1: wdog1grp {
		fsl,pins =
			<MX7D_PAD_LPSR_GPIO1_IO00__WDOG1_WDOG_B	0x30>;
	};
};

&qspi {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_qspi &pinctrl_qspi_reset>;
	status = "okay";

	flash0: flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <29000000>;
		spi-rx-bus-width = <4>;
		spi-tx-bus-width = <4>;
	};
};

&usdhc3 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc3>;
	pinctrl-1 = <&pinctrl_usdhc3_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc3_200mhz>;
	assigned-clocks = <&clks IMX7D_USDHC3_ROOT_CLK>;
	assigned-clock-rates = <400000000>;
	bus-width = <8>;
	non-removable;
	no-sd;
	no-sdio;
	vmmc-supply = <&vgen4_reg>;
	vqmmc-supply = <&sw2_reg>;
	status = "okay";
};

&wdog1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_wdog1>;
	/*
	 * Errata e10574:
	 * WDOG reset needs to run with WDOG_RESET_B signal enabled.
	 * X1-51 (WDOG1#) signal needs carrier board handling to reset
	 * TQMa7 on X1-22 (RESET_IN#).
	 */
	fsl,ext-reset-output;
	status = "okay";
};
