Binding for TI DaVinci Power Sleep Controller (PSC)

The PSC provides power management, clock gating and reset functionality. It is
primarily used for clocking.

Required properties:
- compatible: shall be one of:
	- "ti,da850-psc0" for PSC0 on DA850/OMAP-L138/AM18XX
	- "ti,da850-psc1" for PSC1 on DA850/OMAP-L138/AM18XX
- reg: physical base address and size of the controller's register area
- #clock-cells: from common clock binding; shall be set to 1
- #power-domain-cells: from generic power domain binding; shall be set to 1.
- clocks: phandles to clocks corresponding to the clock-names property
- clock-names: list of parent clock names - depends on compatible value
	- for "ti,da850-psc0", shall be "pll0_sysclk1", "pll0_sysclk2",
	  "pll0_sysclk4", "pll0_sysclk6", "async1"
	- for "ti,da850-psc1", shall be "pll0_sysclk2", "pll0_sysclk4", "async3"

Optional properties:
- #reset-cells: from reset binding; shall be set to 1 - only applicable when
  at least one local domain provides a local reset.

Consumers:

	Clock, power domain and reset consumers shall use the local power domain
	module ID (LPSC) as the index corresponding to the clock cell. Refer to
	the device-specific datasheet to find these numbers. NB: Most local
	domains	only provide a clock/power domain and not a reset.

Examples:

	psc0: clock-controller@10000 {
		compatible = "ti,da850-psc0";
		reg = <0x10000 0x1000>;
		#clock-cells = <1>;
		#power-domain-cells = <1>;
		#reset-cells = <1>;
		clocks = <&pll0_sysclk 1>, <&pll0_sysclk 2>,
			 <&pll0_sysclk 4>, <&pll0_sysclk 6>, <&async1_clk>;
		clock_names = "pll0_sysclk1", "pll0_sysclk2",
			      "pll0_sysclk4", "pll0_sysclk6", "async1";
	};
	psc1: clock-controller@227000 {
		compatible = "ti,da850-psc1";
		reg = <0x227000 0x1000>;
		#clock-cells = <1>;
		#power-domain-cells = <1>;
		clocks = <&pll0_sysclk 2>, <&pll0_sysclk 4>, <&async3_clk>;
		clock_names = "pll0_sysclk2", "pll0_sysclk4", "async3";
	};

	/* consumer */
	dsp: dsp@11800000 {
		compatible = "ti,da850-dsp";
		reg = <0x11800000 0x40000>,
		      <0x11e00000 0x8000>,
		      <0x11f00000 0x8000>,
		      <0x01c14044 0x4>,
		      <0x01c14174 0x8>;
		reg-names = "l2sram", "l1pram", "l1dram", "host1cfg", "chipsig";
		interrupt-parent = <&intc>;
		interrupts = <28>;
		clocks = <&psc0 15>;
		power-domains = <&psc0 15>;
		resets = <&psc0 15>;
	};

Also see:
- Documentation/devicetree/bindings/clock/clock-bindings.txt
- Documentation/devicetree/bindings/power/power_domain.txt
- Documentation/devicetree/bindings/reset/reset.txt
