Configuration:

You can pass the following kernel command line options to sm501 videoframebuffer:

	sm501fb.bpp=	SM501 Display driver:
			Specify bits-per-pixel if not specified by 'mode'

	sm501fb.mode=	SM501 Display driver:
			Specify resolution as
			"<xres>x<yres>[-<bpp>][@<refresh>]"
