.. -*- coding: utf-8; mode: rst -*-

.. _V4L2-SDR-FMT-CU16LE:

****************************
V4L2_SDR_FMT_CU16LE ('CU16')
****************************


Complex unsigned 16-bit little endian IQ sample


Description
===========

This format contains sequence of complex number samples. Each complex
number consist two parts, called In-phase and Quadrature (IQ). Both I
and Q are represented as a 16 bit unsigned little endian number. I value
comes first and Q value after that.

**Byte Order.**
Each cell is one byte.


.. flat-table::
    :header-rows:  0
    :stub-columns: 0

    * - start + 0:
      - I'\ :sub:`0[7:0]`
      - I'\ :sub:`0[15:8]`
    * - start + 2:
      - Q'\ :sub:`0[7:0]`
      - Q'\ :sub:`0[15:8]`
