What:		/sys/bus/platform/devices/INT3407:00/dptf_power/charger_type
Date:		Jul, 2016
KernelVersion:	v4.10
Contact:	linux-acpi@vger.kernel.org
Description:
		(RO) The charger type - Traditional, Hybrid or NVDC.

What:		/sys/bus/platform/devices/INT3407:00/dptf_power/adapter_rating_mw
Date:		Jul, 2016
KernelVersion:	v4.10
Contact:	linux-acpi@vger.kernel.org
Description:
		(RO) Adapter rating in milliwatts (the maximum Adapter power).
		Must be 0 if no AC Adaptor is plugged in.

What:		/sys/bus/platform/devices/INT3407:00/dptf_power/max_platform_power_mw
Date:		Jul, 2016
KernelVersion:	v4.10
Contact:	linux-acpi@vger.kernel.org
Description:
		(RO) Maximum platform power that can be supported by the battery
		in milliwatts.

What:		/sys/bus/platform/devices/INT3407:00/dptf_power/platform_power_source
Date:		Jul, 2016
KernelVersion:	v4.10
Contact:	linux-acpi@vger.kernel.org
Description:
		(RO) Display the platform power source
		0x00 = DC
		0x01 = AC
		0x02 = USB
		0x03 = Wireless Charger

What:		/sys/bus/platform/devices/INT3407:00/dptf_power/battery_steady_power
Date:		Jul, 2016
KernelVersion:	v4.10
Contact:	linux-acpi@vger.kernel.org
Description:
		(RO) The maximum sustained power for battery in milliwatts.
