Omnivision OV5647 raw image sensor
---------------------------------

OV5647 is a raw image sensor with MIPI CSI-2 and CCP2 image data interfaces
and CCI (I2C compatible) control bus.

Required properties:

- compatible		: "ovti,ov5647".
- reg			: I2C slave address of the sensor.
- clocks		: Reference to the xclk clock.

The common video interfaces bindings (see video-interfaces.txt) should be
used to specify link to the image data receiver. The OV5647 device
node should contain one 'port' child node with an 'endpoint' subnode.

Endpoint node mandatory properties:

- remote-endpoint: A phandle to the bus receiver's endpoint node.

Example:

	i2c@2000 {
		...
		ov: camera@36 {
			compatible = "ovti,ov5647";
			reg = <0x36>;
			clocks = <&camera_clk>;
			port {
				camera_1: endpoint {
					remote-endpoint = <&csi1_ep1>;
				};
			};
		};
	};
