THS8134 and THS8135 Video DAC
-----------------------------

This is the binding for Texas Instruments THS8134, THS8134A, THS8134B and
THS8135 Video DAC bridges.

Required properties:

- compatible: Must be one of
  "ti,ths8134"
  "ti,ths8134a," "ti,ths8134"
  "ti,ths8134b", "ti,ths8134"
  "ti,ths8135"

Required nodes:

This device has two video ports. Their connections are modelled using the OF
graph bindings specified in Documentation/devicetree/bindings/graph.txt.

- Video port 0 for RGB input
- Video port 1 for VGA output

Example
-------

vga-bridge {
	compatible = "ti,ths8135";
	#address-cells = <1>;
	#size-cells = <0>;

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;

			vga_bridge_in: endpoint {
				remote-endpoint = <&lcdc_out_vga>;
			};
		};

		port@1 {
			reg = <1>;

			vga_bridge_out: endpoint {
				remote-endpoint = <&vga_con_in>;
			};
		};
	};
};
