Realtek platforms device tree bindings
--------------------------------------


RTD1295 SoC
===========

Required root node properties:

 - compatible :  must contain "realtek,rtd1295"


Root node property compatible must contain, depending on board:

 - MeLE V9: "mele,v9"
 - ProBox2 AVA: "probox2,ava"
 - Zidoo X9S: "zidoo,x9s"


Example:

    compatible = "zidoo,x9s", "realtek,rtd1295";
