Rocktech Display Ltd. RK070ER9427 800(RGB)x480 TFT LCD panel

This binding is compatible with the simple-panel binding, which is specified
in simple-panel.txt in this directory.

Required properties:
- compatible: should be "rocktech,rk070er9427"

Optional properties:
- backlight: phandle of the backlight device attached to the panel

Optional nodes:
- Video port for LCD panel input.

Example:
	panel {
		compatible = "rocktech,rk070er9427";
		backlight = <&backlight_lcd>;

		port {
			lcd_panel_in: endpoint {
				remote-endpoint = <&lcd_display_out>;
			};
		};
	};
