Qualcomm Video Clock & Reset Controller Binding
-----------------------------------------------

Required properties :
- compatible : shall contain "qcom,sdm845-videocc"
- reg : shall contain base register location and length
- #clock-cells : from common clock binding, shall contain 1.
- #power-domain-cells : from generic power domain binding, shall contain 1.

Optional properties :
- #reset-cells : from common reset binding, shall contain 1.

Example:
	videocc: clock-controller@ab00000 {
		compatible = "qcom,sdm845-videocc";
		reg = <0xab00000 0x10000>;
		#clock-cells = <1>;
		#power-domain-cells = <1>;
	};
