Panasonic 10" WUXGA TFT LCD panel

Required properties:
- compatible: should be "panasonic,vvx10f034n00"
- reg: DSI virtual channel of the peripheral
- power-supply: phandle of the regulator that provides the supply voltage

Optional properties:
- backlight: phandle of the backlight device attached to the panel

Example:

	mdss_dsi@fd922800 {
		panel@0 {
			compatible = "panasonic,vvx10f034n00";
			reg = <0>;
			power-supply = <&vreg_vsp>;
			backlight = <&lp8566_wled>;
		};
	};
