Sony CXD2880 DVB-T2/T tuner + demodulator driver SPI adapter

Required properties:
- compatible: Should be "sony,cxd2880".
- reg: SPI chip select number for the device.
- spi-max-frequency: Maximum bus speed, should be set to <55000000> (55MHz).

Example:

cxd2880@0 {
	compatible = "sony,cxd2880";
	reg = <0>; /* CE0 */
	spi-max-frequency = <55000000>; /* 55MHz */
};
