* Thermal Monitoring Unit (TMU) on Freescale QorIQ SoCs

Required properties:
- compatible : Must include "fsl,qoriq-tmu". The version of the device is
	determined by the TMU IP Block Revision Register (IPBRR0) at
	offset 0x0BF8.
	Table of correspondences between IPBRR0 values and example  chips:
		Value           Device
		----------      -----
		0x01900102      T1040
- reg : Address range of TMU registers.
- interrupts : Contains the interrupt for TMU.
- fsl,tmu-range : The values to be programmed into TTRnCR, as specified by
	the SoC reference manual. The first cell is TTR0CR, the second is
	TTR1CR, etc.
- fsl,tmu-calibration : A list of cell pairs containing temperature
	calibration data, as specified by the SoC reference manual.
	The first cell of each pair is the value to be written to TTCFGR,
	and the second is the value to be written to TSCFGR.
- #thermal-sensor-cells : Must be 1. The sensor specifier is the monitoring
	site ID, and represents the "n" in TRITSRn and TRATSRn.

Optional property:
- little-endian : If present, the TMU registers are little endian. If absent,
	the default is big endian.

Example:

tmu@f0000 {
	compatible = "fsl,qoriq-tmu";
	reg = <0xf0000 0x1000>;
	interrupts = <18 2 0 0>;
	fsl,tmu-range = <0x000a0000 0x00090026 0x0008004a 0x0001006a>;
	fsl,tmu-calibration = <0x00000000 0x00000025
			       0x00000001 0x00000028
			       0x00000002 0x0000002d
			       0x00000003 0x00000031
			       0x00000004 0x00000036
			       0x00000005 0x0000003a
			       0x00000006 0x00000040
			       0x00000007 0x00000044
			       0x00000008 0x0000004a
			       0x00000009 0x0000004f
			       0x0000000a 0x00000054

			       0x00010000 0x0000000d
			       0x00010001 0x00000013
			       0x00010002 0x00000019
			       0x00010003 0x0000001f
			       0x00010004 0x00000025
			       0x00010005 0x0000002d
			       0x00010006 0x00000033
			       0x00010007 0x00000043
			       0x00010008 0x0000004b
			       0x00010009 0x00000053

			       0x00020000 0x00000010
			       0x00020001 0x00000017
			       0x00020002 0x0000001f
			       0x00020003 0x00000029
			       0x00020004 0x00000031
			       0x00020005 0x0000003c
			       0x00020006 0x00000042
			       0x00020007 0x0000004d
			       0x00020008 0x00000056

			       0x00030000 0x00000012
			       0x00030001 0x0000001d>;
	#thermal-sensor-cells = <1>;
};
