Parallel to LVDS Encoder
------------------------

This binding supports the parallel to LVDS encoders that don't require any
configuration.

LVDS is a physical layer specification defined in ANSI/TIA/EIA-644-A. Multiple
incompatible data link layers have been used over time to transmit image data
to LVDS panels. This binding targets devices compatible with the following
specifications only.

[JEIDA] "Digital Interface Standards for Monitor", JEIDA-59-1999, February
1999 (Version 1.0), Japan Electronic Industry Development Association (JEIDA)
[LDI] "Open LVDS Display Interface", May 1999 (Version 0.95), National
Semiconductor
[VESA] "VESA Notebook Panel Standard", October 2007 (Version 1.0), Video
Electronics Standards Association (VESA)

Those devices have been marketed under the FPD-Link and FlatLink brand names
among others.


Required properties:

- compatible: Must be "lvds-encoder"

Required nodes:

This device has two video ports. Their connections are modeled using the OF
graph bindings specified in Documentation/devicetree/bindings/graph.txt.

- Video port 0 for parallel input
- Video port 1 for LVDS output


Example
-------

lvds-encoder {
	compatible = "lvds-encoder";
	#address-cells = <1>;
	#size-cells = <0>;

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;

			lvds_enc_in: endpoint {
				remote-endpoint = <&display_out_rgb>;
			};
		};

		port@1 {
			reg = <1>;

			lvds_enc_out: endpoint {
				remote-endpoint = <&lvds_panel_in>;
			};
		};
	};
};
