Innolux P097PFG 9.7" 1536x2048 TFT LCD panel

Required properties:
- compatible: should be "innolux,p097pfg"
- reg: DSI virtual channel of the peripheral
- avdd-supply: phandle of the regulator that provides positive voltage
- avee-supply: phandle of the regulator that provides negative voltage
- enable-gpios: panel enable gpio

Optional properties:
- backlight: phandle of the backlight device attached to the panel

Example:

	&mipi_dsi {
		panel {
			compatible = "innolux,p079zca";
			reg = <0>;
			avdd-supply = <...>;
			avee-supply = <...>;
			backlight = <&backlight>;
			enable-gpios = <&gpio1 13 GPIO_ACTIVE_HIGH>;
		};
	};
