Binding for MIPS Cluster Power Controller (CPC).

This binding allows a system to specify where the CPC registers are
located.

Required properties:
compatible : Should be "mti,mips-cpc".
regs: Should describe the address & size of the CPC register region.
