* Tango Thermal

The SMP8758 SoC includes 3 instances of this temperature sensor
(in the CPU, video decoder, and PCIe controller).

Required properties:
- #thermal-sensor-cells: Should be 0 (see thermal.txt)
- compatible: "sigma,smp8758-thermal"
- reg: Address range of the thermal registers

Example:

	cpu_temp: thermal@920100 {
		#thermal-sensor-cells = <0>;
		compatible = "sigma,smp8758-thermal";
		reg = <0x920100 12>;
	};
