Innolux TV123WAM 12.3 inch eDP 2K display panel

This binding is compatible with the simple-panel binding, which is specified
in simple-panel.txt in this directory.

Required properties:
- compatible: should be "innolux,tv123wam"
- power-supply: regulator to provide the supply voltage

Optional properties:
- enable-gpios: GPIO pin to enable or disable the panel
- backlight: phandle of the backlight device attached to the panel

Example:
	panel_edp: panel-edp {
		compatible = "innolux,tv123wam";
		enable-gpios = <&msmgpio 31 GPIO_ACTIVE_LOW>;
		power-supply = <&pm8916_l2>;
		backlight = <&backlight>;
	};
