Broadcom Stingray device tree bindings
------------------------------------------------

Boards with Stingray shall have the following properties:

Required root node property:

Stingray Combo SVK board
compatible = "brcm,bcm958742k", "brcm,stingray";

Stingray SST100 board
compatible = "brcm,bcm958742t", "brcm,stingray";
