Broadcom BCM2835 device tree bindings
-------------------------------------------

Raspberry Pi Model A
Required root node properties:
compatible = "raspberrypi,model-a", "brcm,bcm2835";

Raspberry Pi Model A+
Required root node properties:
compatible = "raspberrypi,model-a-plus", "brcm,bcm2835";

Raspberry Pi Model B
Required root node properties:
compatible = "raspberrypi,model-b", "brcm,bcm2835";

Raspberry Pi Model B (no P5)
early model B with I2C0 rather than I2C1 routed to the expansion header
Required root node properties:
compatible = "raspberrypi,model-b-i2c0", "brcm,bcm2835";

Raspberry Pi Model B rev2
Required root node properties:
compatible = "raspberrypi,model-b-rev2", "brcm,bcm2835";

Raspberry Pi Model B+
Required root node properties:
compatible = "raspberrypi,model-b-plus", "brcm,bcm2835";

Raspberry Pi 2 Model B
Required root node properties:
compatible = "raspberrypi,2-model-b", "brcm,bcm2836";

Raspberry Pi 3 Model B
Required root node properties:
compatible = "raspberrypi,3-model-b", "brcm,bcm2837";

Raspberry Pi 3 Model B+
Required root node properties:
compatible = "raspberrypi,3-model-b-plus", "brcm,bcm2837";

Raspberry Pi Compute Module
Required root node properties:
compatible = "raspberrypi,compute-module", "brcm,bcm2835";

Raspberry Pi Zero
Required root node properties:
compatible = "raspberrypi,model-zero", "brcm,bcm2835";

Raspberry Pi Zero W
Required root node properties:
compatible = "raspberrypi,model-zero-w", "brcm,bcm2835";

Generic BCM2835 board
Required root node properties:
compatible = "brcm,bcm2835";
