STMicroelectronics STM32 Digital Camera Memory Interface (DCMI)

Required properties:
- compatible: "st,stm32-dcmi"
- reg: physical base address and length of the registers set for the device
- interrupts: should contain IRQ line for the DCMI
- resets: reference to a reset controller,
          see Documentation/devicetree/bindings/reset/st,stm32-rcc.txt
- clocks: list of clock specifiers, corresponding to entries in
          the clock-names property
- clock-names: must contain "mclk", which is the DCMI peripherial clock
- pinctrl: the pincontrol settings to configure muxing properly
           for pins that connect to DCMI device.
           See Documentation/devicetree/bindings/pinctrl/st,stm32-pinctrl.txt.
- dmas: phandle to DMA controller node,
        see Documentation/devicetree/bindings/dma/stm32-dma.txt
- dma-names: must contain "tx", which is the transmit channel from DCMI to DMA

DCMI supports a single port node with parallel bus. It should contain one
'port' child node with child 'endpoint' node. Please refer to the bindings
defined in Documentation/devicetree/bindings/media/video-interfaces.txt.

Example:

	dcmi: dcmi@50050000 {
		compatible = "st,stm32-dcmi";
		reg = <0x50050000 0x400>;
		interrupts = <78>;
		resets = <&rcc STM32F4_AHB2_RESET(DCMI)>;
		clocks = <&rcc 0 STM32F4_AHB2_CLOCK(DCMI)>;
		clock-names = "mclk";
		pinctrl-names = "default";
		pinctrl-0 = <&dcmi_pins>;
		dmas = <&dma2 1 1 0x414 0x3>;
		dma-names = "tx";
		port {
			dcmi_0: endpoint {
				remote-endpoint = <...>;
				bus-width = <8>;
				hsync-active = <0>;
				vsync-active = <0>;
				pclk-sample = <1>;
			};
		};
	};
