Sharp Microelectronics 4.3" qHD TFT LCD panel

Required properties:
- compatible: should be "sharp,ls043t1le01-qhd"
- reg: DSI virtual channel of the peripheral
- power-supply: phandle of the regulator that provides the supply voltage

Optional properties:
- backlight: phandle of the backlight device attached to the panel
- reset-gpios: a GPIO spec for the reset pin

Example:

	mdss_dsi@fd922800 {
		panel@0 {
			compatible = "sharp,ls043t1le01-qhd";
			reg = <0>;
			avdd-supply = <&pm8941_l22>;
			backlight = <&pm8941_wled>;
			reset-gpios = <&pm8941_gpios 19 GPIO_ACTIVE_HIGH>;
		};
	};
