JDI model LT070ME05000 1200x1920 7" DSI Panel

Required properties:
- compatible: should be "jdi,lt070me05000"
- vddp-supply: phandle of the regulator that provides the supply voltage
  Power IC supply (3-5V)
- iovcc-supply: phandle of the regulator that provides the supply voltage
  IOVCC , power supply for LCM (1.8V)
- enable-gpios: phandle of gpio for enable line
  LED_EN, LED backlight enable, High active
- reset-gpios: phandle of gpio for reset line
  This should be 8mA, gpio can be configured using mux, pinctrl, pinctrl-names
  XRES, Reset, Low active
- dcdc-en-gpios: phandle of the gpio for power ic line
  Power IC supply enable, High active

Example:

	dsi0: qcom,mdss_dsi@4700000 {
		panel@0 {
			compatible = "jdi,lt070me05000";
			reg = <0>;

			vddp-supply = <&pm8921_l17>;
			iovcc-supply = <&pm8921_lvs7>;

			enable-gpios = <&pm8921_gpio 36 GPIO_ACTIVE_HIGH>;
			reset-gpios = <&tlmm_pinmux 54 GPIO_ACTIVE_LOW>;
			dcdc-en-gpios = <&pm8921_gpio 23 GPIO_ACTIVE_HIGH>;
		};
	};
