AU Optronics Corporation 7.0" FHD (800 x 480) TFT LCD panel

Required properties:
- compatible: should be "auo,g070vvn01"
- backlight: phandle of the backlight device attached to the panel
- power-supply: single regulator to provide the supply voltage

Required nodes:
- port: Parallel port mapping to connect this display

This panel needs single power supply voltage. Its backlight is conntrolled
via PWM signal.

Example:
--------

Example device-tree definition when connected to iMX6Q based board

	lcd_panel: lcd-panel {
		compatible = "auo,g070vvn01";
		backlight = <&backlight_lcd>;
		power-supply = <&reg_display>;

		port {
			lcd_panel_in: endpoint {
				remote-endpoint = <&lcd_display_out>;
			};
		};
	};
