Samsung S6E3HA2 5.7" 1440x2560 AMOLED panel
Samsung S6E3HF2 5.65" 1600x2560 AMOLED panel

Required properties:
  - compatible: should be one of:
    "samsung,s6e3ha2",
    "samsung,s6e3hf2".
  - reg: the virtual channel number of a DSI peripheral
  - vdd3-supply: I/O voltage supply
  - vci-supply: voltage supply for analog circuits
  - reset-gpios: a GPIO spec for the reset pin (active low)
  - enable-gpios: a GPIO spec for the panel enable pin (active high)

Optional properties:
  - te-gpios: a GPIO spec for the tearing effect synchronization signal
    gpio pin (active high)

Example:
&dsi {
	...

	panel@0 {
		compatible = "samsung,s6e3ha2";
		reg = <0>;
		vdd3-supply = <&ldo27_reg>;
		vci-supply = <&ldo28_reg>;
		reset-gpios = <&gpg0 0 GPIO_ACTIVE_LOW>;
		enable-gpios = <&gpf1 5 GPIO_ACTIVE_HIGH>;
		te-gpios = <&gpf1 3 GPIO_ACTIVE_HIGH>;
	};
};
