Sharp 15" LQ150X1LG11 XGA TFT LCD panel

Required properties:
- compatible: should be "sharp,lq150x1lg11"
- power-supply: regulator to provide the VCC supply voltage (3.3 volts)

Optional properties:
- backlight: phandle of the backlight device
- rlud-gpios: a single GPIO for the RL/UD (rotate 180 degrees) pin.
- sellvds-gpios: a single GPIO for the SELLVDS pin.

If rlud-gpios and/or sellvds-gpios are not specified, the RL/UD and/or SELLVDS
pins are assumed to be handled appropriately by the hardware.

Example:

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm 0 100000>;                      /* VBR */

		brightness-levels = <0 20 40 60 80 100>;
		default-brightness-level = <2>;

		power-supply = <&vdd_12v_reg>;               /* VDD */
		enable-gpios = <&gpio 42 GPIO_ACTIVE_HIGH>;  /* XSTABY */
	};

	panel {
		compatible = "sharp,lq150x1lg11";

		power-supply = <&vcc_3v3_reg>;               /* VCC */

		backlight = <&backlight>;
		rlud-gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;    /* RL/UD */
		sellvds-gpios = <&gpio 18 GPIO_ACTIVE_HIGH>; /* SELLVDS */
	};
