* Device tree bindings for TI TPS61050/61052 Boost Converters

The TP61050/TPS61052 is a high-power "white LED driver". The
device provides LED, GPIO and regulator functionalities.

Required properties:
- compatible:		"ti,tps61050" or "ti,tps61052"
- reg:			Specifies the I2C slave address

Example:

i2c0 {
	tps61052@33 {
		compatible = "ti,tps61052";
		reg = <0x33>;
	};
};
