Broadcom BCM4708 device tree bindings
-------------------------------------------

Boards with the BCM4708 SoC shall have the following properties:

Required root node property:

bcm4708
compatible = "brcm,bcm4708";

bcm4709
compatible = "brcm,bcm4709";

bcm53012
compatible = "brcm,bcm53012";
