* Currus Logic CLPS711X Framebuffer

Required properties:
- compatible: Shall contain "cirrus,ep7209-fb".
- reg       : Physical base address and length of the controller's registers +
              location and size of the framebuffer memory.
- clocks    : phandle + clock specifier pair of the FB reference clock.
- display   : phandle to a display node as described in
              Documentation/devicetree/bindings/display/panel/display-timing.txt.
              Additionally, the display node has to define properties:
  - bits-per-pixel: Bits per pixel.
  - ac-prescale   : LCD AC bias frequency. This frequency is the required
                    AC bias frequency for a given manufacturer's LCD plate.
  - cmap-invert   : Invert the color levels (Optional).

Optional properties:
- lcd-supply: Regulator for LCD supply voltage.

Example:
	fb: fb@800002c0 {
		compatible = "cirrus,ep7312-fb", "cirrus,ep7209-fb";
		reg = <0x800002c0 0xd44>, <0x60000000 0xc000>;
		clocks = <&clks 2>;
		lcd-supply = <&reg5v0>;
		display = <&display>;
	};

	display: display {
		model = "320x240x4";
		native-mode = <&timing0>;
		bits-per-pixel = <4>;
		ac-prescale = <17>;

		display-timings {
			timing0: 320x240 {
				hactive = <320>;
				hback-porch = <0>;
				hfront-porch = <0>;
				hsync-len = <0>;
				vactive = <240>;
				vback-porch = <0>;
				vfront-porch = <0>;
				vsync-len = <0>;
				clock-frequency = <6500000>;
			};
		};
	};
