NVIDIA Tegra124 SoC EMC (external memory controller)
====================================================

Required properties :
- compatible : Should be "nvidia,tegra124-emc".
- reg : physical base address and length of the controller's registers.
- nvidia,memory-controller : phandle of the MC driver.

The node should contain a "emc-timings" subnode for each supported RAM type
(see field RAM_CODE in register PMC_STRAPPING_OPT_A), with its unit address
being its RAM_CODE.

Required properties for "emc-timings" nodes :
- nvidia,ram-code : Should contain the value of RAM_CODE this timing set is
used for.

Each "emc-timings" node should contain a "timing" subnode for every supported
EMC clock rate. The "timing" subnodes should have the clock rate in Hz as
their unit address.

Required properties for "timing" nodes :
- clock-frequency : Should contain the memory clock rate in Hz.
- The following properties contain EMC timing characterization values
(specified in the board documentation) :
  - nvidia,emc-auto-cal-config : EMC_AUTO_CAL_CONFIG
  - nvidia,emc-auto-cal-config2 : EMC_AUTO_CAL_CONFIG2
  - nvidia,emc-auto-cal-config3 : EMC_AUTO_CAL_CONFIG3
  - nvidia,emc-auto-cal-interval : EMC_AUTO_CAL_INTERVAL
  - nvidia,emc-bgbias-ctl0 : EMC_BGBIAS_CTL0
  - nvidia,emc-cfg : EMC_CFG
  - nvidia,emc-cfg-2 : EMC_CFG_2
  - nvidia,emc-ctt-term-ctrl : EMC_CTT_TERM_CTRL
  - nvidia,emc-mode-1 : Mode Register 1
  - nvidia,emc-mode-2 : Mode Register 2
  - nvidia,emc-mode-4 : Mode Register 4
  - nvidia,emc-mode-reset : Mode Register 0
  - nvidia,emc-mrs-wait-cnt : EMC_MRS_WAIT_CNT
  - nvidia,emc-sel-dpd-ctrl : EMC_SEL_DPD_CTRL
  - nvidia,emc-xm2dqspadctrl2 : EMC_XM2DQSPADCTRL2
  - nvidia,emc-zcal-cnt-long : EMC_ZCAL_WAIT_CNT after clock change
  - nvidia,emc-zcal-interval : EMC_ZCAL_INTERVAL
- nvidia,emc-configuration : EMC timing characterization data. These are the
registers (see section "15.6.2 EMC Registers" in the TRM) whose values need to
be specified, according to the board documentation:

	EMC_RC
	EMC_RFC
	EMC_RFC_SLR
	EMC_RAS
	EMC_RP
	EMC_R2W
	EMC_W2R
	EMC_R2P
	EMC_W2P
	EMC_RD_RCD
	EMC_WR_RCD
	EMC_RRD
	EMC_REXT
	EMC_WEXT
	EMC_WDV
	EMC_WDV_MASK
	EMC_QUSE
	EMC_QUSE_WIDTH
	EMC_IBDLY
	EMC_EINPUT
	EMC_EINPUT_DURATION
	EMC_PUTERM_EXTRA
	EMC_PUTERM_WIDTH
	EMC_PUTERM_ADJ
	EMC_CDB_CNTL_1
	EMC_CDB_CNTL_2
	EMC_CDB_CNTL_3
	EMC_QRST
	EMC_QSAFE
	EMC_RDV
	EMC_RDV_MASK
	EMC_REFRESH
	EMC_BURST_REFRESH_NUM
	EMC_PRE_REFRESH_REQ_CNT
	EMC_PDEX2WR
	EMC_PDEX2RD
	EMC_PCHG2PDEN
	EMC_ACT2PDEN
	EMC_AR2PDEN
	EMC_RW2PDEN
	EMC_TXSR
	EMC_TXSRDLL
	EMC_TCKE
	EMC_TCKESR
	EMC_TPD
	EMC_TFAW
	EMC_TRPAB
	EMC_TCLKSTABLE
	EMC_TCLKSTOP
	EMC_TREFBW
	EMC_FBIO_CFG6
	EMC_ODT_WRITE
	EMC_ODT_READ
	EMC_FBIO_CFG5
	EMC_CFG_DIG_DLL
	EMC_CFG_DIG_DLL_PERIOD
	EMC_DLL_XFORM_DQS0
	EMC_DLL_XFORM_DQS1
	EMC_DLL_XFORM_DQS2
	EMC_DLL_XFORM_DQS3
	EMC_DLL_XFORM_DQS4
	EMC_DLL_XFORM_DQS5
	EMC_DLL_XFORM_DQS6
	EMC_DLL_XFORM_DQS7
	EMC_DLL_XFORM_DQS8
	EMC_DLL_XFORM_DQS9
	EMC_DLL_XFORM_DQS10
	EMC_DLL_XFORM_DQS11
	EMC_DLL_XFORM_DQS12
	EMC_DLL_XFORM_DQS13
	EMC_DLL_XFORM_DQS14
	EMC_DLL_XFORM_DQS15
	EMC_DLL_XFORM_QUSE0
	EMC_DLL_XFORM_QUSE1
	EMC_DLL_XFORM_QUSE2
	EMC_DLL_XFORM_QUSE3
	EMC_DLL_XFORM_QUSE4
	EMC_DLL_XFORM_QUSE5
	EMC_DLL_XFORM_QUSE6
	EMC_DLL_XFORM_QUSE7
	EMC_DLL_XFORM_ADDR0
	EMC_DLL_XFORM_ADDR1
	EMC_DLL_XFORM_ADDR2
	EMC_DLL_XFORM_ADDR3
	EMC_DLL_XFORM_ADDR4
	EMC_DLL_XFORM_ADDR5
	EMC_DLL_XFORM_QUSE8
	EMC_DLL_XFORM_QUSE9
	EMC_DLL_XFORM_QUSE10
	EMC_DLL_XFORM_QUSE11
	EMC_DLL_XFORM_QUSE12
	EMC_DLL_XFORM_QUSE13
	EMC_DLL_XFORM_QUSE14
	EMC_DLL_XFORM_QUSE15
	EMC_DLI_TRIM_TXDQS0
	EMC_DLI_TRIM_TXDQS1
	EMC_DLI_TRIM_TXDQS2
	EMC_DLI_TRIM_TXDQS3
	EMC_DLI_TRIM_TXDQS4
	EMC_DLI_TRIM_TXDQS5
	EMC_DLI_TRIM_TXDQS6
	EMC_DLI_TRIM_TXDQS7
	EMC_DLI_TRIM_TXDQS8
	EMC_DLI_TRIM_TXDQS9
	EMC_DLI_TRIM_TXDQS10
	EMC_DLI_TRIM_TXDQS11
	EMC_DLI_TRIM_TXDQS12
	EMC_DLI_TRIM_TXDQS13
	EMC_DLI_TRIM_TXDQS14
	EMC_DLI_TRIM_TXDQS15
	EMC_DLL_XFORM_DQ0
	EMC_DLL_XFORM_DQ1
	EMC_DLL_XFORM_DQ2
	EMC_DLL_XFORM_DQ3
	EMC_DLL_XFORM_DQ4
	EMC_DLL_XFORM_DQ5
	EMC_DLL_XFORM_DQ6
	EMC_DLL_XFORM_DQ7
	EMC_XM2CMDPADCTRL
	EMC_XM2CMDPADCTRL4
	EMC_XM2CMDPADCTRL5
	EMC_XM2DQPADCTRL2
	EMC_XM2DQPADCTRL3
	EMC_XM2CLKPADCTRL
	EMC_XM2CLKPADCTRL2
	EMC_XM2COMPPADCTRL
	EMC_XM2VTTGENPADCTRL
	EMC_XM2VTTGENPADCTRL2
	EMC_XM2VTTGENPADCTRL3
	EMC_XM2DQSPADCTRL3
	EMC_XM2DQSPADCTRL4
	EMC_XM2DQSPADCTRL5
	EMC_XM2DQSPADCTRL6
	EMC_DSR_VTTGEN_DRV
	EMC_TXDSRVTTGEN
	EMC_FBIO_SPARE
	EMC_ZCAL_WAIT_CNT
	EMC_MRS_WAIT_CNT2
	EMC_CTT
	EMC_CTT_DURATION
	EMC_CFG_PIPE
	EMC_DYN_SELF_REF_CONTROL
	EMC_QPOP

Example SoC include file:

/ {
	emc@7001b000 {
		compatible = "nvidia,tegra124-emc";
		reg = <0x0 0x7001b000 0x0 0x1000>;

		nvidia,memory-controller = <&mc>;
	};
};

Example board file:

/ {
	emc@7001b000 {
		emc-timings-3 {
			nvidia,ram-code = <3>;

			timing-12750000 {
				clock-frequency = <12750000>;

				nvidia,emc-zcal-cnt-long = <0x00000042>;
				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-ctt-term-ctrl = <0x00000802>;
				nvidia,emc-cfg = <0x73240000>;
				nvidia,emc-cfg-2 = <0x000008c5>;
				nvidia,emc-sel-dpd-ctrl = <0x00040128>;
				nvidia,emc-bgbias-ctl0 = <0x00000008>;
				nvidia,emc-auto-cal-config = <0xa1430000>;
				nvidia,emc-auto-cal-config2 = <0x00000000>;
				nvidia,emc-auto-cal-config3 = <0x00000000>;
				nvidia,emc-mode-reset = <0x80001221>;
				nvidia,emc-mode-1 = <0x80100003>;
				nvidia,emc-mode-2 = <0x80200008>;
				nvidia,emc-mode-4 = <0x00000000>;

				nvidia,emc-configuration = <
					0x00000000 /* EMC_RC */
					0x00000003 /* EMC_RFC */
					0x00000000 /* EMC_RFC_SLR */
					0x00000000 /* EMC_RAS */
					0x00000000 /* EMC_RP */
					0x00000004 /* EMC_R2W */
					0x0000000a /* EMC_W2R */
					0x00000003 /* EMC_R2P */
					0x0000000b /* EMC_W2P */
					0x00000000 /* EMC_RD_RCD */
					0x00000000 /* EMC_WR_RCD */
					0x00000003 /* EMC_RRD */
					0x00000003 /* EMC_REXT */
					0x00000000 /* EMC_WEXT */
					0x00000006 /* EMC_WDV */
					0x00000006 /* EMC_WDV_MASK */
					0x00000006 /* EMC_QUSE */
					0x00000002 /* EMC_QUSE_WIDTH */
					0x00000000 /* EMC_IBDLY */
					0x00000005 /* EMC_EINPUT */
					0x00000005 /* EMC_EINPUT_DURATION */
					0x00010000 /* EMC_PUTERM_EXTRA */
					0x00000003 /* EMC_PUTERM_WIDTH */
					0x00000000 /* EMC_PUTERM_ADJ */
					0x00000000 /* EMC_CDB_CNTL_1 */
					0x00000000 /* EMC_CDB_CNTL_2 */
					0x00000000 /* EMC_CDB_CNTL_3 */
					0x00000004 /* EMC_QRST */
					0x0000000c /* EMC_QSAFE */
					0x0000000d /* EMC_RDV */
					0x0000000f /* EMC_RDV_MASK */
					0x00000060 /* EMC_REFRESH */
					0x00000000 /* EMC_BURST_REFRESH_NUM */
					0x00000018 /* EMC_PRE_REFRESH_REQ_CNT */
					0x00000002 /* EMC_PDEX2WR */
					0x00000002 /* EMC_PDEX2RD */
					0x00000001 /* EMC_PCHG2PDEN */
					0x00000000 /* EMC_ACT2PDEN */
					0x00000007 /* EMC_AR2PDEN */
					0x0000000f /* EMC_RW2PDEN */
					0x00000005 /* EMC_TXSR */
					0x00000005 /* EMC_TXSRDLL */
					0x00000004 /* EMC_TCKE */
					0x00000005 /* EMC_TCKESR */
					0x00000004 /* EMC_TPD */
					0x00000000 /* EMC_TFAW */
					0x00000000 /* EMC_TRPAB */
					0x00000005 /* EMC_TCLKSTABLE */
					0x00000005 /* EMC_TCLKSTOP */
					0x00000064 /* EMC_TREFBW */
					0x00000000 /* EMC_FBIO_CFG6 */
					0x00000000 /* EMC_ODT_WRITE */
					0x00000000 /* EMC_ODT_READ */
					0x106aa298 /* EMC_FBIO_CFG5 */
					0x002c00a0 /* EMC_CFG_DIG_DLL */
					0x00008000 /* EMC_CFG_DIG_DLL_PERIOD */
					0x00064000 /* EMC_DLL_XFORM_DQS0 */
					0x00064000 /* EMC_DLL_XFORM_DQS1 */
					0x00064000 /* EMC_DLL_XFORM_DQS2 */
					0x00064000 /* EMC_DLL_XFORM_DQS3 */
					0x00064000 /* EMC_DLL_XFORM_DQS4 */
					0x00064000 /* EMC_DLL_XFORM_DQS5 */
					0x00064000 /* EMC_DLL_XFORM_DQS6 */
					0x00064000 /* EMC_DLL_XFORM_DQS7 */
					0x00064000 /* EMC_DLL_XFORM_DQS8 */
					0x00064000 /* EMC_DLL_XFORM_DQS9 */
					0x00064000 /* EMC_DLL_XFORM_DQS10 */
					0x00064000 /* EMC_DLL_XFORM_DQS11 */
					0x00064000 /* EMC_DLL_XFORM_DQS12 */
					0x00064000 /* EMC_DLL_XFORM_DQS13 */
					0x00064000 /* EMC_DLL_XFORM_DQS14 */
					0x00064000 /* EMC_DLL_XFORM_DQS15 */
					0x00000000 /* EMC_DLL_XFORM_QUSE0 */
					0x00000000 /* EMC_DLL_XFORM_QUSE1 */
					0x00000000 /* EMC_DLL_XFORM_QUSE2 */
					0x00000000 /* EMC_DLL_XFORM_QUSE3 */
					0x00000000 /* EMC_DLL_XFORM_QUSE4 */
					0x00000000 /* EMC_DLL_XFORM_QUSE5 */
					0x00000000 /* EMC_DLL_XFORM_QUSE6 */
					0x00000000 /* EMC_DLL_XFORM_QUSE7 */
					0x00000000 /* EMC_DLL_XFORM_ADDR0 */
					0x00000000 /* EMC_DLL_XFORM_ADDR1 */
					0x00000000 /* EMC_DLL_XFORM_ADDR2 */
					0x00000000 /* EMC_DLL_XFORM_ADDR3 */
					0x00000000 /* EMC_DLL_XFORM_ADDR4 */
					0x00000000 /* EMC_DLL_XFORM_ADDR5 */
					0x00000000 /* EMC_DLL_XFORM_QUSE8 */
					0x00000000 /* EMC_DLL_XFORM_QUSE9 */
					0x00000000 /* EMC_DLL_XFORM_QUSE10 */
					0x00000000 /* EMC_DLL_XFORM_QUSE11 */
					0x00000000 /* EMC_DLL_XFORM_QUSE12 */
					0x00000000 /* EMC_DLL_XFORM_QUSE13 */
					0x00000000 /* EMC_DLL_XFORM_QUSE14 */
					0x00000000 /* EMC_DLL_XFORM_QUSE15 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS0 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS1 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS2 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS3 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS4 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS5 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS6 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS7 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS8 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS9 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS10 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS11 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS12 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS13 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS14 */
					0x00000000 /* EMC_DLI_TRIM_TXDQS15 */
					0x000fc000 /* EMC_DLL_XFORM_DQ0 */
					0x000fc000 /* EMC_DLL_XFORM_DQ1 */
					0x000fc000 /* EMC_DLL_XFORM_DQ2 */
					0x000fc000 /* EMC_DLL_XFORM_DQ3 */
					0x0000fc00 /* EMC_DLL_XFORM_DQ4 */
					0x0000fc00 /* EMC_DLL_XFORM_DQ5 */
					0x0000fc00 /* EMC_DLL_XFORM_DQ6 */
					0x0000fc00 /* EMC_DLL_XFORM_DQ7 */
					0x10000280 /* EMC_XM2CMDPADCTRL */
					0x00000000 /* EMC_XM2CMDPADCTRL4 */
					0x00111111 /* EMC_XM2CMDPADCTRL5 */
					0x00000000 /* EMC_XM2DQPADCTRL2 */
					0x00000000 /* EMC_XM2DQPADCTRL3 */
					0x77ffc081 /* EMC_XM2CLKPADCTRL */
					0x00000e0e /* EMC_XM2CLKPADCTRL2 */
					0x81f1f108 /* EMC_XM2COMPPADCTRL */
					0x07070004 /* EMC_XM2VTTGENPADCTRL */
					0x0000003f /* EMC_XM2VTTGENPADCTRL2 */
					0x016eeeee /* EMC_XM2VTTGENPADCTRL3 */
					0x51451400 /* EMC_XM2DQSPADCTRL3 */
					0x00514514 /* EMC_XM2DQSPADCTRL4 */
					0x00514514 /* EMC_XM2DQSPADCTRL5 */
					0x51451400 /* EMC_XM2DQSPADCTRL6 */
					0x0000003f /* EMC_DSR_VTTGEN_DRV */
					0x00000007 /* EMC_TXDSRVTTGEN */
					0x00000000 /* EMC_FBIO_SPARE */
					0x00000042 /* EMC_ZCAL_WAIT_CNT */
					0x000e000e /* EMC_MRS_WAIT_CNT2 */
					0x00000000 /* EMC_CTT */
					0x00000003 /* EMC_CTT_DURATION */
					0x0000f2f3 /* EMC_CFG_PIPE */
					0x800001c5 /* EMC_DYN_SELF_REF_CONTROL */
					0x0000000a /* EMC_QPOP */
				>;
			};
		};
	};
};
