Platform DesignWare HS OTG USB 2.0 controller
-----------------------------------------------------

Required properties:
- compatible : One of:
  - brcm,bcm2835-usb: The DWC2 USB controller instance in the BCM2835 SoC.
  - hisilicon,hi6220-usb: The DWC2 USB controller instance in the hi6220 SoC.
  - rockchip,rk3066-usb: The DWC2 USB controller instance in the rk3066 Soc;
  - "rockchip,rk3188-usb", "rockchip,rk3066-usb", "snps,dwc2": for rk3188 Soc;
  - "rockchip,rk3288-usb", "rockchip,rk3066-usb", "snps,dwc2": for rk3288 Soc;
  - "lantiq,arx100-usb": The DWC2 USB controller instance in Lantiq ARX SoCs;
  - "lantiq,xrx200-usb": The DWC2 USB controller instance in Lantiq XRX SoCs;
  - "amlogic,meson8-usb": The DWC2 USB controller instance in Amlogic Meson8 SoCs;
  - "amlogic,meson8b-usb": The DWC2 USB controller instance in Amlogic Meson8b SoCs;
  - "amlogic,meson-gxbb-usb": The DWC2 USB controller instance in Amlogic S905 SoCs;
  - "amcc,dwc-otg": The DWC2 USB controller instance in AMCC Canyonlands 460EX SoCs;
  - snps,dwc2: A generic DWC2 USB controller with default parameters.
  - "st,stm32f4x9-fsotg": The DWC2 USB FS/HS controller instance in STM32F4x9 SoCs
  configured in FS mode;
  - "st,stm32f4x9-hsotg": The DWC2 USB HS controller instance in STM32F4x9 SoCs
  configured in HS mode;
  - "st,stm32f7-hsotg": The DWC2 USB HS controller instance in STM32F7 SoCs
    configured in HS mode;
- reg : Should contain 1 register range (address and length)
- interrupts : Should contain 1 interrupt
- clocks: clock provider specifier
- clock-names: shall be "otg"
Refer to clk/clock-bindings.txt for generic clock consumer properties

Optional properties:
- phys: phy provider specifier
- phy-names: shall be "usb2-phy"
Refer to phy/phy-bindings.txt for generic phy consumer properties
- dr_mode: shall be one of "host", "peripheral" and "otg"
  Refer to usb/generic.txt
- g-rx-fifo-size: size of rx fifo size in gadget mode.
- g-np-tx-fifo-size: size of non-periodic tx fifo size in gadget mode.
- g-tx-fifo-size: size of periodic tx fifo per endpoint (except ep0) in gadget mode.

Deprecated properties:
- g-use-dma: gadget DMA mode is automatically detected

Example:

        usb@101c0000 {
                compatible = "ralink,rt3050-usb, snps,dwc2";
                reg = <0x101c0000 40000>;
                interrupts = <18>;
		clocks = <&usb_otg_ahb_clk>;
		clock-names = "otg";
		phys = <&usbphy>;
		phy-names = "usb2-phy";
        };
