TMP108 temperature sensor
-------------------------

This device supports I2C only.

Requires node properties:
- compatible : "ti,tmp108"
- reg : the I2C address of the device. This is 0x48, 0x49, 0x4a, or 0x4b.

Example:
	tmp108@48 {
		compatible = "ti,tmp108";
		reg = <0x48>;
	};
