Amlogic Meson SoC Reset Controller
=======================================

Please also refer to reset.txt in this directory for common reset
controller binding usage.

Required properties:
- compatible: Should be "amlogic,meson8b-reset", "amlogic,meson-gxbb-reset" or
	"amlogic,meson-axg-reset".
- reg: should contain the register address base
- #reset-cells: 1, see below

example:

reset: reset-controller {
	compatible = "amlogic,meson-gxbb-reset";
	reg = <0x0 0x04404 0x0 0x20>;
	#reset-cells = <1>;
};
