Broadcom Northstar Plus device tree bindings
--------------------------------------------

Broadcom Northstar Plus family of SoCs are used for switching control
and management applications as well as residential router/gateway
applications. The SoC features dual core Cortex A9 ARM CPUs, integrating
several peripheral interfaces including multiple Gigabit Ethernet PHYs,
DDR3 memory, PCIE Gen-2, USB 2.0 and USB 3.0, serial and NAND flash,
SATA and several other IO controllers.

Boards with Northstar Plus SoCs shall have the following properties:

Required root node property:

BCM58522
compatible = "brcm,bcm58522", "brcm,nsp";

BCM58525
compatible = "brcm,bcm58525", "brcm,nsp";

BCM58535
compatible = "brcm,bcm58535", "brcm,nsp";

BCM58622
compatible = "brcm,bcm58622", "brcm,nsp";

BCM58623
compatible = "brcm,bcm58623", "brcm,nsp";

BCM58625
compatible = "brcm,bcm58625", "brcm,nsp";

BCM88312
compatible = "brcm,bcm88312", "brcm,nsp";
