Qualcomm MSM8916 A53 PLL Binding
--------------------------------
The A53 PLL on MSM8916 platforms is the main CPU PLL used used for frequencies
above 1GHz.

Required properties :
- compatible : Shall contain only one of the following:

		"qcom,msm8916-a53pll"

- reg : shall contain base register location and length

- #clock-cells : must be set to <0>

Example:

	a53pll: clock@b016000 {
		compatible = "qcom,msm8916-a53pll";
		reg = <0xb016000 0x40>;
		#clock-cells = <0>;
	};

