MediaTek PWM controller

Required properties:
 - compatible: should be "mediatek,<name>-pwm":
   - "mediatek,mt2712-pwm": found on mt2712 SoC.
   - "mediatek,mt7622-pwm": found on mt7622 SoC.
   - "mediatek,mt7623-pwm": found on mt7623 SoC.
   - "mediatek,mt7628-pwm": found on mt7628 SoC.
 - reg: physical base address and length of the controller's registers.
 - #pwm-cells: must be 2. See pwm.txt in this directory for a description of
   the cell format.
 - clocks: phandle and clock specifier of the PWM reference clock.
 - clock-names: must contain the following, except for MT7628 which
                has no clocks
   - "top": the top clock generator
   - "main": clock used by the PWM core
   - "pwm1-8": the eight per PWM clocks for mt2712
   - "pwm1-6": the six per PWM clocks for mt7622
   - "pwm1-5": the five per PWM clocks for mt7623
 - pinctrl-names: Must contain a "default" entry.
 - pinctrl-0: One property must exist for each entry in pinctrl-names.
   See pinctrl/pinctrl-bindings.txt for details of the property values.

Example:
	pwm0: pwm@11006000 {
		compatible = "mediatek,mt7623-pwm";
		reg = <0 0x11006000 0 0x1000>;
		#pwm-cells = <2>;
		clocks = <&topckgen CLK_TOP_PWM_SEL>,
			 <&pericfg CLK_PERI_PWM>,
			 <&pericfg CLK_PERI_PWM1>,
			 <&pericfg CLK_PERI_PWM2>,
			 <&pericfg CLK_PERI_PWM3>,
			 <&pericfg CLK_PERI_PWM4>,
			 <&pericfg CLK_PERI_PWM5>;
		clock-names = "top", "main", "pwm1", "pwm2",
			      "pwm3", "pwm4", "pwm5";
		pinctrl-names = "default";
		pinctrl-0 = <&pwm0_pins>;
	};
