* Powerventure Semiconductor PV88060 Voltage Regulator

Required properties:
- compatible: "pvs,pv88060".
- reg: I2C slave address, usually 0x49.
- interrupts: the interrupt outputs of the controller
- regulators: A node that houses a sub-node for each regulator within the
  device. Each sub-node is identified using the node's name, with valid
  values listed below. The content of each sub-node is defined by the
  standard binding for regulators; see regulator.txt.
  BUCK1, LDO1, LDO2, LDO3, LDO4, LDO5, LDO6, LDO7, SW1, SW2, SW3, SW4,
  SW5, and SW6.

Optional properties:
- Any optional property defined in regulator.txt

Example

	pmic: pv88060@49 {
		compatible = "pvs,pv88060";
		reg = <0x49>;
		interrupt-parent = <&gpio>;
		interrupts = <24 24>;

		regulators {
			BUCK1 {
				regulator-name = "buck1";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <4387500>;
				regulator-min-microamp 	= <1496000>;
				regulator-max-microamp 	= <4189000>;
				regulator-boot-on;
			};

			LDO1 {
				regulator-name = "ldo1";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO2 {
				regulator-name = "ldo2";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO3 {
				regulator-name = "ldo3";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO4 {
				regulator-name = "ldo4";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO5 {
				regulator-name = "ldo5";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO6 {
				regulator-name = "ldo6";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			LDO7 {
				regulator-name = "ldo7";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <3350000>;
				regulator-boot-on;
			};

			SW1 {
				regulator-name = "sw1";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
			};

			SW2 {
				regulator-name = "sw2";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-boot-on;
			};

			SW3 {
				regulator-name = "sw3";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-boot-on;
			};

			SW4 {
				regulator-name = "sw4";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-boot-on;
			};

			SW5 {
				regulator-name = "sw5";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-boot-on;
			};

			SW6 {
				regulator-name = "sw6";
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
			};
		};
	};