Broadcom North Star 2 (NS2) device tree bindings
------------------------------------------------

Boards with NS2 shall have the following properties:

Required root node property:

NS2 SVK board
compatible = "brcm,ns2-svk", "brcm,ns2";
