Sharp LQ035Q7DB03 3.5" QVGA TFT LCD panel

Required properties:
- compatible: should be "sharp,lq035q7db03"
- power-supply: phandle of the regulator that provides the supply voltage

Optional properties:
- enable-gpios: GPIO pin to enable or disable the panel
- backlight: phandle of the backlight device attached to the panel

This binding is compatible with the simple-panel binding, which is specified
in simple-panel.txt in this directory.
