Qualcomm Multimedia Clock & Reset Controller Binding
----------------------------------------------------

Required properties :
- compatible : shall contain only one of the following:

			"qcom,mmcc-apq8064"
			"qcom,mmcc-apq8084"
			"qcom,mmcc-msm8660"
			"qcom,mmcc-msm8960"
			"qcom,mmcc-msm8974"
			"qcom,mmcc-msm8996"

- reg : shall contain base register location and length
- #clock-cells : shall contain 1
- #reset-cells : shall contain 1

Optional properties :
- #power-domain-cells : shall contain 1

Example:
	clock-controller@4000000 {
		compatible = "qcom,mmcc-msm8960";
		reg = <0x4000000 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
		#power-domain-cells = <1>;
	};
