* MediaTek mt76xx devices

This node provides properties for configuring the MediaTek mt76xx wireless
device. The node is expected to be specified as a child node of the PCI
controller to which the wireless chip is connected.

Optional properties:

- mac-address: See ethernet.txt in the parent directory
- local-mac-address: See ethernet.txt in the parent directory
- ieee80211-freq-limit: See ieee80211.txt
- mediatek,mtd-eeprom: Specify a MTD partition + offset containing EEPROM data

Optional nodes:
- led: Properties for a connected LED
  Optional properties:
    - led-sources: See Documentation/devicetree/bindings/leds/common.txt

&pcie {
	pcie0 {
		wifi@0,0 {
			compatible = "mediatek,mt76";
			reg = <0x0000 0 0 0 0>;
			ieee80211-freq-limit = <5000000 6000000>;
			mediatek,mtd-eeprom = <&factory 0x8000>;

			led {
				led-sources = <2>;
			};
		};
	};
};
