STMicroelectronics STM32MP1 Peripheral Reset Controller
=======================================================

The RCC IP is both a reset and a clock controller.

Please see Documentation/devicetree/bindings/clock/st,stm32mp1-rcc.txt
