* Freescale Inter IC (I2C) and High Speed Inter IC (HS-I2C) for i.MX

Required properties:
- compatible :
  - "fsl,imx1-i2c" for I2C compatible with the one integrated on i.MX1 SoC
  - "fsl,imx21-i2c" for I2C compatible with the one integrated on i.MX21 SoC
  - "fsl,vf610-i2c" for I2C compatible with the one integrated on Vybrid vf610 SoC
- reg : Should contain I2C/HS-I2C registers location and length
- interrupts : Should contain I2C/HS-I2C interrupt
- clocks : Should contain the I2C/HS-I2C clock specifier

Optional properties:
- clock-frequency : Constains desired I2C/HS-I2C bus clock frequency in Hz.
  The absence of the property indicates the default frequency 100 kHz.
- dmas: A list of two dma specifiers, one for each entry in dma-names.
- dma-names: should contain "tx" and "rx".
- scl-gpios: specify the gpio related to SCL pin
- sda-gpios: specify the gpio related to SDA pin
- pinctrl: add extra pinctrl to configure i2c pins to gpio function for i2c
  bus recovery, call it "gpio" state

Examples:

i2c@83fc4000 { /* I2C2 on i.MX51 */
	compatible = "fsl,imx51-i2c", "fsl,imx21-i2c";
	reg = <0x83fc4000 0x4000>;
	interrupts = <63>;
};

i2c@70038000 { /* HS-I2C on i.MX51 */
	compatible = "fsl,imx51-i2c", "fsl,imx21-i2c";
	reg = <0x70038000 0x4000>;
	interrupts = <64>;
	clock-frequency = <400000>;
};

i2c0: i2c@40066000 { /* i2c0 on vf610 */
	compatible = "fsl,vf610-i2c";
	reg = <0x40066000 0x1000>;
	interrupts =<0 71 0x04>;
	dmas = <&edma0 0 50>,
		<&edma0 0 51>;
	dma-names = "rx","tx";
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_i2c1>;
	pinctrl-1 = <&pinctrl_i2c1_gpio>;
	scl-gpios = <&gpio5 26 GPIO_ACTIVE_HIGH>;
	sda-gpios = <&gpio5 27 GPIO_ACTIVE_HIGH>;
};
