Samsung S6E63J0X03 1.63" 320x320 AMOLED panel (interface: MIPI-DSI command mode)

Required properties:
  - compatible: "samsung,s6e63j0x03"
  - reg: the virtual channel number of a DSI peripheral
  - vdd3-supply: I/O voltage supply
  - vci-supply: voltage supply for analog circuits
  - reset-gpios: a GPIO spec for the reset pin (active low)
  - te-gpios: a GPIO spec for the tearing effect synchronization signal
    gpio pin (active high)

Example:
&dsi {
	...

	panel@0 {
		compatible = "samsung,s6e63j0x03";
		reg = <0>;
		vdd3-supply = <&ldo16_reg>;
		vci-supply = <&ldo20_reg>;
		reset-gpios = <&gpe0 1 GPIO_ACTIVE_LOW>;
		te-gpios = <&gpx0 6 GPIO_ACTIVE_HIGH>;
	};
};
