United Radiant Technology UMSH-8596MD-xT 7.0" WVGA TFT LCD panel

Supported are LVDS versions (-11T, -19T) and parallel ones
(-T, -1T, -7T, -20T).

Required properties:
- compatible: should be one of:
  "urt,umsh-8596md-t",
  "urt,umsh-8596md-1t",
  "urt,umsh-8596md-7t",
  "urt,umsh-8596md-11t",
  "urt,umsh-8596md-19t",
  "urt,umsh-8596md-20t".

This binding is compatible with the simple-panel binding, which is specified
in simple-panel.txt in this directory.
