Copyright (C) 2017-2019 by Vadim Yanitskiy <axilirator@gmail.com>
License GPLv2+: GNU GPL version 2 or later <http://gnu.org/licenses/gpl.html>
This is free software: you are free to change and redistribute it.
There is NO WARRANTY, to the extent permitted by law.

[INFO] transceiver.py:157 Init transceiver 'BTS@127.0.0.1:5700'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5702 <-> R:127.0.0.1:5802)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5701 <-> R:127.0.0.1:5801)
[INFO] transceiver.py:157 Init transceiver 'MS@127.0.0.1:6700'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:6702 <-> R:127.0.0.1:6802)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:6701 <-> R:127.0.0.1:6801)
[INFO] transceiver.py:157 Init transceiver 'TRX1@127.0.0.1:5700/1'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5704 <-> R:127.0.0.1:5804)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5703 <-> R:127.0.0.1:5803)
[INFO] transceiver.py:157 Init transceiver 'TRX2@127.0.0.1:5700/2'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5706 <-> R:127.0.0.1:5806)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5705 <-> R:127.0.0.1:5805)
[INFO] transceiver.py:157 Init transceiver 'TRX3@127.0.0.1:5700/3'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5708 <-> R:127.0.0.1:5808)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5707 <-> R:127.0.0.1:5807)
[INFO] fake_trx.py:426 Init complete
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 102
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=104 tn=7 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=130 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=131 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=123 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=123 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=124 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=153 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=148 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=104 tn=7 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=105 tn=7 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=107): ver=1 fn=106 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=128 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=127 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=125 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=125 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=125 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=126 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=0 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=1 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=2 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=3 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=4 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=5 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=6 bl=148 pwr=0), but transceiver is not running => dropping...
[WARNING] transceiver.py:287 (BTS@127.0.0.1:5700) RX TRXD message (ver=1 fn=137 tn=7 bl=148 pwr=0), but transceiver is not running => dropping...
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[INFO] transceiver.py:276 Stopping clock generator
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX1@127.0.0.1:5700/1) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX1@127.0.0.1:5700/1) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX1@127.0.0.1:5700/1) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX2@127.0.0.1:5700/2) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX2@127.0.0.1:5700/2) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX2@127.0.0.1:5700/2) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (TRX3@127.0.0.1:5700/3) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:131 (TRX3@127.0.0.1:5700/3) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:215 (TRX3@127.0.0.1:5700/3) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:97 (BTS@127.0.0.1:5700) Recv POWERON CMD
[INFO] ctrl_if_trx.py:109 (BTS@127.0.0.1:5700) Starting transceiver...
[INFO] transceiver.py:273 Starting clock generator
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETRXGAIN
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETSLOT
[DEBUG] clck_gen.py:128 IND CLOCK 0
[DEBUG] clck_gen.py:128 IND CLOCK 102
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=105): ver=1 fn=104 tn=7 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=0 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=1 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=2 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=3 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=4 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=5 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=6 bl=148 pwr=0
[WARNING] transceiver.py:330 (BTS@127.0.0.1:5700) Stale TRXD message (fn=106): ver=1 fn=105 tn=7 bl=148 pwr=0
[DEBUG] fake_trx.py:273 (BTS@127.0.0.1:5700) Recv FAKE_TOA cmd
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD NOHANDOVER
[DEBUG] fake_trx.py:292 (BTS@127.0.0.1:5700) Recv FAKE_RSSI cmd
[DEBUG] fake_trx.py:317 (BTS@127.0.0.1:5700) Recv FAKE_CI cmd
[DEBUG] clck_gen.py:128 IND CLOCK 204
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] clck_gen.py:128 IND CLOCK 306
[DEBUG] clck_gen.py:128 IND CLOCK 408
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] clck_gen.py:128 IND CLOCK 510
[DEBUG] clck_gen.py:128 IND CLOCK 612
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX1@127.0.0.1:5700/1) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX2@127.0.0.1:5700/2) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:207 (TRX3@127.0.0.1:5700/3) Recv SETPOWER cmd
[DEBUG] clck_gen.py:128 IND CLOCK 714
