09:29:57.138389 13818 C5G_Tests.ttcn:324 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating'.
09:29:58.183543 13818 C5G_Tests.ttcn:324 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating' was executed successfully (exit status: 0).
09:29:58.183808 13818 C5G_Tests.ttcn:324 Test case TC_periodic_registration_updating started.
09:29:58.183979 13818 C5G_Tests.ttcn:324 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_periodic_registration_updating.
09:29:58.184173 13818 C5G_Tests.ttcn:324 Port NGAP_UNIT[0] was started.
09:29:58.184235 13818 C5G_Tests.ttcn:324 Port NGAP_PROC[0] was started.
09:29:58.184284 13818 C5G_Tests.ttcn:324 Port TEID0 was started.
09:29:58.184334 13818 C5G_Tests.ttcn:324 Component type C5G_Tests.MTC_CT was initialized.
09:29:58.184389 13818 C5G_Tests.ttcn:191 Start timer g_Tguard: 30 s
09:29:58.184452 13818 C5G_Tests.ttcn:192 Altstep as_Tguard was activated as default, id 1
09:29:58.184512 13818 C5G_Tests.ttcn:183 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:29:58.191067 14048 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:58.191106 14048 - TTCN-3 Parallel Test Component started on 809ffe4822d8. Component reference: GTP1U_EM(12), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
09:29:58.191127 14048 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:58.191167 14048 - Connected to MC.
09:29:58.191187 14048 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_periodic_registration_updating.
09:29:58.191223 13818 C5G_Tests.ttcn:183 PTC was created. Component reference: 12, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:29:58.191235 13818 C5G_Tests.ttcn:184 Mapping port GTP1U_EM(12):GTP1U to system:GTP1U.
09:29:58.193422 14048 - Port GTP1U was started.
09:29:58.193517 14048 - Port TEID0 was started.
09:29:58.193566 14048 - Port CLIENT was started.
09:29:58.193614 14048 - Port CLIENT_PROC was started.
09:29:58.193662 14048 - Port UECUPS was started.
09:29:58.193708 14048 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
09:29:58.193854 14048 - Port GTP1U was mapped to system:GTP1U.
09:29:58.193971 13818 C5G_Tests.ttcn:184 Map operation of GTP1U_EM(12):GTP1U to system:GTP1U finished.
09:29:58.194034 13818 C5G_Tests.ttcn:185 Connecting ports GTP1U_EM(12):TEID0 and mtc:TEID0.
09:29:58.194593 13818 C5G_Tests.ttcn:185 Port TEID0 is waiting for connection from GTP1U_EM(12):TEID0 on UNIX pathname /tmp/ttcn3-portconn-7c6ca674.
09:29:58.194710 14048 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
09:29:58.194807 13818 C5G_Tests.ttcn:185 Port TEID0 has accepted the connection from GTP1U_EM(12):TEID0.
09:29:58.194873 13818 C5G_Tests.ttcn:185 Connect operation on GTP1U_EM(12):TEID0 and mtc:TEID0 finished.
09:29:58.194929 13818 C5G_Tests.ttcn:186 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(12).
09:29:58.195039 13818 C5G_Tests.ttcn:186 Function was started.
09:29:58.195285 13818 C5G_Tests.ttcn:161 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:29:58.195328 14048 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
09:29:58.196063 14048 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 14.196055: srand48(724622012).
09:29:58.196149 14048 Osmocom_Types.ttcn:65 Function rnd() returned 0.130332.
09:29:58.196353 14048 Osmocom_Types.ttcn:65 Function rnd() returned 0.586161.
09:29:58.196609 14048 GTPv1U_Emulation.ttcnpp:214 Mapping port GTP1U_EM(12):UECUPS to system:UECUPS.
09:29:58.196734 14048 GTPv1U_Emulation.ttcnpp:214 Port UECUPS was mapped to system:UECUPS.
09:29:58.196839 14048 GTPv1U_Emulation.ttcnpp:214 Map operation of GTP1U_EM(12):UECUPS to system:UECUPS finished.
09:29:58.197694 14048 GTPv1U_Emulation.ttcnpp:215 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
09:29:58.198298 14048 GTPv1U_Emulation.ttcnpp:215 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:29:58.201279 14048 GTPv1U_Emulation.ttcnpp:190 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
09:29:58.201590 14048 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
09:29:58.201872 14048 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
09:29:58.202188 14048 GTPv1U_Emulation.ttcnpp:190 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
09:29:58.202702 14048 GTPv1U_Emulation.ttcnpp:191 Start timer T: 30 s
09:29:58.203334 14049 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:58.203602 14049 - TTCN-3 Parallel Test Component started on 809ffe4822d8. Component reference: TC_periodic_registration_updating-NGAP0(13), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0. Version: 11.1.0.
09:29:58.203731 14048 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:58.203761 14049 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:58.204008 14049 - Connected to MC.
09:29:58.204048 14048 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
09:29:58.204178 14049 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_periodic_registration_updating.
09:29:58.204259 13818 C5G_Tests.ttcn:161 PTC was created. Component reference: 13, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:29:58.204341 13818 C5G_Tests.ttcn:162 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:29:58.204356 14048 GTPv1U_Emulation.ttcnpp:194 Matching on port UECUPS succeeded:  matched
09:29:58.204481 14048 GTPv1U_Emulation.ttcnpp:194 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:58.204561 14048 GTPv1U_Emulation.ttcnpp:194 Message with id 1 was extracted from the queue of UECUPS.
09:29:58.204927 14048 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
09:29:58.205088 14048 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
09:29:58.205419 14048 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
09:29:58.205585 14048 GTPv1U_Emulation.ttcnpp:192 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:29:58.205802 14048 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS succeeded:  matched
09:29:58.205882 14048 GTPv1U_Emulation.ttcnpp:193 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:29:58.205952 14048 GTPv1U_Emulation.ttcnpp:193 Message with id 2 was extracted from the queue of UECUPS.
09:29:58.206117 14048 GTPv1U_Emulation.ttcnpp:225 Altstep as_uecups_ind was activated as default, id 1
09:29:58.207716 14049 - Port NGAP was started.
09:29:58.207808 14049 - Port NGAP_CLIENT was started.
09:29:58.207862 14049 - Port NGAP_PROC was started.
09:29:58.207913 14049 - Port NGAP_UNIT was started.
09:29:58.207964 14049 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:29:58.208082 14049 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:29:58.208289 13818 C5G_Tests.ttcn:162 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:29:58.208370 13818 C5G_Tests.ttcn:163 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0].
09:29:58.209021 13818 C5G_Tests.ttcn:163 Port NGAP_PROC[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-4d54f519.
09:29:58.209223 14049 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
09:29:58.209316 13818 C5G_Tests.ttcn:163 Port NGAP_PROC[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:58.209434 13818 C5G_Tests.ttcn:163 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0] finished.
09:29:58.209491 13818 C5G_Tests.ttcn:164 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0].
09:29:58.209973 13818 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-5c4dec08.
09:29:58.210146 14049 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
09:29:58.210235 13818 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:29:58.210352 13818 C5G_Tests.ttcn:164 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
09:29:58.210406 13818 C5G_Tests.ttcn:165 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0") on component TC_periodic_registration_updating-NGAP0(13).
09:29:58.210675 13818 C5G_Tests.ttcn:165 Function was started.
09:29:58.210940 14049 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0").
09:29:58.213078 14049 NGAP_Emulation.ttcn:452 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:29:58.213297 14049 NGAP_Emulation.ttcn:452 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:29:58.214098 14049 NGAP_Emulation.ttcn:457 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
09:29:58.214654 14049 NGAP_Emulation.ttcn:457 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:29:58.216984 14049 NGAP_Emulation.ttcn:469 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:29:58.217203 13818 C5G_Tests.ttcn:166 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:29:58.217278 13818 C5G_Tests.ttcn:166 Matching on port NGAP_UNIT[0] succeeded:  matched
09:29:58.217340 13818 C5G_Tests.ttcn:166 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:29:58.217398 13818 C5G_Tests.ttcn:166 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
09:29:58.217903 13818 C5G_Tests.ttcn:268 Sent on NGAP_UNIT[0] to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
09:29:58.218018 13818 C5G_Tests.ttcn:269 Start timer T: 5 s
09:29:58.221093 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:58.224345 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:58.224738 14049 NGAP_Emulation.ttcn:542 Matching on port NGAP_UNIT succeeded:  matched
09:29:58.224813 14049 NGAP_Emulation.ttcn:542 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:58.224857 14049 NGAP_Emulation.ttcn:542 Message with id 1 was extracted from the queue of NGAP_UNIT.
09:29:58.227765 14049 NGAP_Emulation.ttcn:544 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.228513 14049 NGAP_Emulation.ttcn:544 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
09:29:58.228995 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:29:58.229063 14049 NGAP_Emulation.ttcn:600 Matching on port NGAP succeeded:  matched
09:29:58.229090 14049 NGAP_Emulation.ttcn:600 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:58.229109 14049 NGAP_Emulation.ttcn:600 Message with id 1 was extracted from the queue of NGAP.
09:29:58.229190 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
09:29:58.230148 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:58.230205 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.230226 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:58.230242 14049 NGAP_Emulation.ttcn:548 Message with id 2 was extracted from the queue of NGAP.
09:29:58.230315 14049 C5G_Tests.ttcn:128 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.230529 13818 C5G_Tests.ttcn:270 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:58.230558 13818 C5G_Tests.ttcn:271 Matching on port NGAP_UNIT[0] succeeded:  matched
09:29:58.230573 13818 C5G_Tests.ttcn:271 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:58.230588 13818 C5G_Tests.ttcn:271 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
09:29:58.230599 13818 C5G_Tests.ttcn:272 setverdict(pass): none -> pass
09:29:58.230637 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.002416.
09:29:58.230651 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.025681.
09:29:58.230662 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.898613.
09:29:58.230672 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.682232.
09:29:58.230682 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.930926.
09:29:58.230692 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.098929.
09:29:58.230702 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.404402.
09:29:58.230711 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.551736.
09:29:58.230721 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.928809.
09:29:58.230731 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.718720.
09:29:58.230741 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.783785.
09:29:58.230751 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.304753.
09:29:58.230761 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.580324.
09:29:58.230770 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.857388.
09:29:58.230780 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.627131.
09:29:58.230790 13818 Osmocom_Types.ttcn:65 Function rnd() returned 0.569489.
09:29:58.230824 13818 C5G_Tests.ttcn:216 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:29:58.233254 14050 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:58.233305 14050 - TTCN-3 Parallel Test Component started on 809ffe4822d8. Component reference: TC_periodic_registration_updating0(14), component type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0. Version: 11.1.0.
09:29:58.233324 14050 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:58.233375 14050 - Connected to MC.
09:29:58.233392 14050 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_periodic_registration_updating.
09:29:58.233461 13818 C5G_Tests.ttcn:216 PTC was created. Component reference: 14, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:29:58.233478 13818 C5G_Tests.ttcn:218 Connecting ports TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:29:58.233643 14049 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT is waiting for connection from TC_periodic_registration_updating0(14):NGAP on UNIX pathname /tmp/ttcn3-portconn-127da15c.
09:29:58.234555 14050 - Port NGAP was started.
09:29:58.234582 14050 - Port NGAP_PROC was started.
09:29:58.234595 14050 - Port GTP1U[0] was started.
09:29:58.234608 14050 - Port GTP1U[1] was started.
09:29:58.234621 14050 - Port GTP1U[2] was started.
09:29:58.234634 14050 - Port GTP1U[3] was started.
09:29:58.234647 14050 - Port GTP1U_PROC[0] was started.
09:29:58.234660 14050 - Port GTP1U_PROC[1] was started.
09:29:58.234673 14050 - Port GTP1U_PROC[2] was started.
09:29:58.234686 14050 - Port GTP1U_PROC[3] was started.
09:29:58.234698 14050 - Component type ConnHdlr.ConnHdlr was initialized.
09:29:58.234740 14050 - Port NGAP has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT using transport type UNIX.
09:29:58.234771 14049 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT has accepted the connection from TC_periodic_registration_updating0(14):NGAP.
09:29:58.234827 13818 C5G_Tests.ttcn:218 Connect operation on TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT finished.
09:29:58.234844 13818 C5G_Tests.ttcn:219 Connecting ports TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:58.234976 14049 NGAP_Emulation.ttcn:485 Port NGAP_PROC is waiting for connection from TC_periodic_registration_updating0(14):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-867ae15.
09:29:58.235008 14050 - Port NGAP_PROC has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_PROC using transport type UNIX.
09:29:58.235034 14049 NGAP_Emulation.ttcn:485 Port NGAP_PROC has accepted the connection from TC_periodic_registration_updating0(14):NGAP_PROC.
09:29:58.235049 13818 C5G_Tests.ttcn:219 Connect operation on TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC finished.
09:29:58.235065 13818 C5G_Tests.ttcn:222 Connecting ports TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT.
09:29:58.235210 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT is waiting for connection from TC_periodic_registration_updating0(14):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-1325d238.
09:29:58.235243 14050 - Port GTP1U[0] has established the connection with GTP1U_EM(12):CLIENT using transport type UNIX.
09:29:58.235285 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT has accepted the connection from TC_periodic_registration_updating0(14):GTP1U[0].
09:29:58.235299 13818 C5G_Tests.ttcn:222 Connect operation on TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT finished.
09:29:58.235317 13818 C5G_Tests.ttcn:223 Connecting ports TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:29:58.235448 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC is waiting for connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-517ea655.
09:29:58.235481 14050 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(12):CLIENT_PROC using transport type UNIX.
09:29:58.235506 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC has accepted the connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:29:58.235521 13818 C5G_Tests.ttcn:223 Connect operation on TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC finished.
09:29:58.235538 13818 C5G_Tests.ttcn:227 Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '0086904597735865'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}) on component TC_periodic_registration_updating0(14).
09:29:58.235616 13818 C5G_Tests.ttcn:227 Function was started.
09:29:58.236450 14050 - Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '0086904597735865'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}).
09:29:58.239814 14050 ConnHdlr.ttcn:539 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:58.240483 14050 ConnHdlr.ttcn:539 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
09:29:58.245712 14050 ConnHdlr.ttcn:544 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:29:58.246980 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:58.247072 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.247103 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.247129 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.247153 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.247447 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.247498 14049 NGAP_Emulation.ttcn:513 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:58.247528 14049 NGAP_Emulation.ttcn:513 Message with id 1 was extracted from the queue of NGAP_CLIENT.
09:29:58.249524 14049 NGAP_Emulation.ttcn:519 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.250061 14049 NGAP_Emulation.ttcn:519 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
09:29:58.254632 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403E000003000A000200020055000200000026002B2A7E00560202000021BE5B5D51E6982F3D04F7C1174C49B8932010D18696D48FEC800052AE713ACAC735A3'O
} id 3
09:29:58.256800 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560202000021BE5B5D51E6982F3D04F7C1174C49B8932010D18696D48FEC800052AE713ACAC735A3'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:29:58.257040 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.257137 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560202000021BE5B5D51E6982F3D04F7C1174C49B8932010D18696D48FEC800052AE713ACAC735A3'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:29:58.257208 14049 NGAP_Emulation.ttcn:548 Message with id 3 was extracted from the queue of NGAP.
09:29:58.257736 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E00560202000021BE5B5D51E6982F3D04F7C1174C49B8932010D18696D48FEC800052AE713ACAC735A3'O
09:29:58.259290 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10111110010110110101110101010001111001101001100000101111001111010000010011110111110000010001011101001100010010011011100010010011'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '11010001100001101001011011010100100011111110110010000000000000000101001010101110011100010011101011001010110001110011010110100011'B
        },
        eapMessage := omit
    }
}
09:29:58.260085 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10111110010110110101110101010001111001101001100000101111001111010000010011110111110000010001011101001100010010011011100010010011'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '11010001100001101001011011010100100011111110110010000000000000000101001010101110011100010011101011001010110001110011010110100011'B
        },
        eapMessage := omit
    }
}
09:29:58.260909 14050 ConnHdlr.ttcn:556 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10111110010110110101110101010001111001101001100000101111001111010000010011110111110000010001011101001100010010011011100010010011'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '11010001100001101001011011010100100011111110110010000000000000000101001010101110011100010011101011001010110001110011010110100011'B
        },
        eapMessage := omit
    }
} id 1
09:29:58.261584 14050 ConnHdlr.ttcn:189 Matching on port NGAP succeeded:  matched
09:29:58.261735 14050 ConnHdlr.ttcn:189 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10111110010110110101110101010001111001101001100000101111001111010000010011110111110000010001011101001100010010011011100010010011'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '11010001100001101001011011010100100011111110110010000000000000000101001010101110011100010011101011001010110001110011010110100011'B
        },
        eapMessage := omit
    }
} id 1
09:29:58.261842 14050 ConnHdlr.ttcn:189 Message with id 1 was extracted from the queue of NGAP.
09:29:58.266960 14050 ConnHdlr.ttcn:234 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '238C44818E9B94A1D471590C366DA3627AAFE87AFB0C11763B34BB6BCB9F6208'O,
        k_nas_enc := '0F260109818E55827A16B8BC42E9A7F8CB5D42D4B6B68109AC51DD08CF764A13'O
    }
}
09:29:58.267208 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '238C44818E9B94A1D471590C366DA3627AAFE87AFB0C11763B34BB6BCB9F6208'O,
        k_nas_enc := '0F260109818E55827A16B8BC42E9A7F8CB5D42D4B6B68109AC51DD08CF764A13'O
    }
} id 2
09:29:58.267330 14050 ConnHdlr.ttcn:238 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00011111010011110100001110011010011001000100101000100100101010011101110100100110010110100010011101011010000110001110111011001100'B
        },
        eapMessage := omit
    }
}
09:29:58.267336 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.267392 14049 NGAP_Emulation.ttcn:487 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '238C44818E9B94A1D471590C366DA3627AAFE87AFB0C11763B34BB6BCB9F6208'O,
        k_nas_enc := '0F260109818E55827A16B8BC42E9A7F8CB5D42D4B6B68109AC51DD08CF764A13'O
    }
} id 2
09:29:58.267430 14049 NGAP_Emulation.ttcn:487 Message with id 2 was extracted from the queue of NGAP_CLIENT.
09:29:58.267736 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00011111010011110100001110011010011001000100101000100100101010011101110100100110010110100010011101011010000110001110111011001100'B
        },
        eapMessage := omit
    }
} id 3
09:29:58.267915 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.267953 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.267984 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.268013 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.268060 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.268141 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.268185 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00011111010011110100001110011010011001000100101000100100101010011101110100100110010110100010011101011010000110001110111011001100'B
        },
        eapMessage := omit
    }
} id 3
09:29:58.268221 14049 NGAP_Emulation.ttcn:522 Message with id 3 was extracted from the queue of NGAP_CLIENT.
09:29:58.268326 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00011111010011110100001110011010011001000100101000100100101010011101110100100110010110100010011101011010000110001110111011001100'B
        },
        eapMessage := omit
    }
}
09:29:58.268677 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D101F4F439A644A24A9DD265A275A18EECC'O
09:29:58.270149 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D101F4F439A644A24A9DD265A275A18EECC'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.270394 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403C000004000A0002000200550002000000260016157E00572D101F4F439A644A24A9DD265A275A18EECC0079400F4099F907000000000099F907000001'O
}
09:29:58.277293 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044027000003000A0002000200550002000000260014137E03EF3F2BA0007E005D0102028040E1360102'O
} id 4
09:29:58.277526 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03EF3F2BA0007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:29:58.277657 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.277732 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03EF3F2BA0007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:29:58.277803 14049 NGAP_Emulation.ttcn:548 Message with id 4 was extracted from the queue of NGAP.
09:29:58.277876 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E03EF3F2BA0007E005D0102028040E1360102'O
09:29:58.277974 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := 'EF3F2BA0'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0102028040E1360102'O
    }
}
09:29:58.280123 14049 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0102028040E1360102'O
09:29:58.280705 14049 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:29:58.281275 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:29:58.281883 14050 ConnHdlr.ttcn:557 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:29:58.282471 14050 ConnHdlr.ttcn:250 Matching on port NGAP succeeded:  matched
09:29:58.282580 14050 ConnHdlr.ttcn:250 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:29:58.282649 14050 ConnHdlr.ttcn:250 Message with id 2 was extracted from the queue of NGAP.
09:29:58.282779 14050 ConnHdlr.ttcn:255 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
09:29:58.282904 14050 ConnHdlr.ttcn:260 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
09:29:58.282939 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:29:58.283099 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:29:58.283174 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:29:58.283238 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.283292 14049 NGAP_Emulation.ttcn:499 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:29:58.283329 14050 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:58.283348 14049 NGAP_Emulation.ttcn:499 Message with id 4 was extracted from the queue of NGAP_CLIENT.
09:29:58.283515 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:29:58.283559 14050 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004129000D0199F9072143000100000000002E028040'O
09:29:58.283584 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:29:58.283638 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:29:58.283747 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
09:29:58.283814 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.283866 14049 NGAP_Emulation.ttcn:506 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:29:58.283918 14049 NGAP_Emulation.ttcn:506 Message with id 5 was extracted from the queue of NGAP_CLIENT.
09:29:58.283963 14050 ConnHdlr.ttcn:271 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '0086904597735865'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:29:58.284291 14050 NGAP_Emulation.ttcn:717 Called on NGAP_PROC to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
09:29:58.284459 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '0086904597735865'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:29:58.284708 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.284767 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.284813 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.284858 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.284916 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.284974 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.285035 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '0086904597735865'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:29:58.285091 14049 NGAP_Emulation.ttcn:522 Message with id 6 was extracted from the queue of NGAP_CLIENT.
09:29:58.285212 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '0086904597735865'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:29:58.285445 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090500869045977358657100177E004129000D0199F9072143000100000000002E028040'O
09:29:58.287082 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '6CF7E4CA'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090500869045977358657100177E004129000D0199F9072143000100000000002E028040'O
    }
}
09:29:58.287163 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E046CF7E4CA007E005E7700090500869045977358657100177E004129000D0199F9072143000100000000002E028040'O
09:29:58.287393 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E046CF7E4CA007E005E7700090500869045977358657100177E004129000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.287535 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4057000004000A0002000200550002000000260031307E046CF7E4CA007E005E7700090500869045977358657100177E004129000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
09:29:58.287825 14049 NGAP_Emulation.ttcn:485 Call enqueued on NGAP_PROC from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:29:58.287916 14049 NGAP_Emulation.ttcn:602 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
09:29:58.287958 14049 NGAP_Emulation.ttcn:606 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
09:29:58.288003 14049 NGAP_Emulation.ttcn:610 Matching on port NGAP_PROC succeeded: { } with { } matched
09:29:58.288092 14049 NGAP_Emulation.ttcn:610 Getcall operation on port NGAP_PROC succeeded, call from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:29:58.288141 14049 NGAP_Emulation.ttcn:610 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:29:58.288213 14049 NGAP_Emulation.ttcn:613 Replied on NGAP_PROC to TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2
09:29:58.288399 14050 NGAP_Emulation.ttcn:717 Reply enqueued on NGAP_PROC from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:29:58.288513 14050 NGAP_Emulation.ttcn:718 Matching on port NGAP_PROC succeeded: { } with { } matched value 2 with ? matched
09:29:58.288650 14050 NGAP_Emulation.ttcn:718 Getreply operation on port NGAP_PROC succeeded, reply from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:29:58.288701 14050 NGAP_Emulation.ttcn:718 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:29:58.306265 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044056000005000A000200020055000200000026002F2E7E02DBD79EC4017E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
09:29:58.307683 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02DBD79EC4017E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:29:58.307898 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.308000 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02DBD79EC4017E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:29:58.308063 14049 NGAP_Emulation.ttcn:548 Message with id 5 was extracted from the queue of NGAP.
09:29:58.308146 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02DBD79EC4017E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192'O
09:29:58.308236 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'DBD79EC4'O,
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192'O
    }
}
09:29:58.309869 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000036A54074099F90700000115020101210201005E0192'O
09:29:58.311288 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:58.312359 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:58.313418 14050 ConnHdlr.ttcn:562 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:29:58.314359 14050 ConnHdlr.ttcn:562 Matching on port NGAP succeeded:  matched
09:29:58.314491 14050 ConnHdlr.ttcn:562 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:29:58.314565 14050 ConnHdlr.ttcn:562 Message with id 3 was extracted from the queue of NGAP.
09:29:58.314740 14050 ConnHdlr.ttcn:564 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:58.314882 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:29:58.314973 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.315016 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.315058 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.315099 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.315151 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.315201 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.315249 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:29:58.315297 14049 NGAP_Emulation.ttcn:522 Message with id 7 was extracted from the queue of NGAP_CLIENT.
09:29:58.315368 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:58.315444 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:29:58.316478 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '6310D0F4'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:29:58.316528 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E026310D0F4007E0043'O
09:29:58.316745 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E026310D0F4007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.316870 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E026310D0F4007E00430079400F4099F907000000000099F907000001'O
}
09:29:58.318612 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E028874BCD3027E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
} id 6
09:29:58.318815 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E028874BCD3027E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:29:58.318945 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.319003 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E028874BCD3027E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:29:58.319049 14049 NGAP_Emulation.ttcn:548 Message with id 6 was extracted from the queue of NGAP.
09:29:58.319105 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E028874BCD3027E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
09:29:58.319168 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '8874BCD3'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
    }
}
09:29:58.320299 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
09:29:58.320806 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:58.321297 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:58.321703 14050 ConnHdlr.ttcn:566 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:29:58.322237 14050 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:29:58.322332 14050 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:29:58.322394 14050 ConnHdlr.ttcn:279 Message with id 4 was extracted from the queue of NGAP.
09:29:58.322511 14050 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:58.322644 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:29:58.322760 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.322810 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.322855 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.322899 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.322955 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.323008 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.323061 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:29:58.323113 14049 NGAP_Emulation.ttcn:522 Message with id 8 was extracted from the queue of NGAP_CLIENT.
09:29:58.323131 14050 ConnHdlr.ttcn:578 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:58.323188 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:58.323269 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:29:58.324510 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '1B5B499C'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:29:58.324585 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E021B5B499C007E0055'O
09:29:58.324820 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E021B5B499C007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.324966 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E021B5B499C007E00550079400F4099F907000000000099F907000001'O
}
09:29:58.325741 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:29:58.326192 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.326254 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.326306 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.326372 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.326443 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.326527 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.326629 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:29:58.326699 14049 NGAP_Emulation.ttcn:522 Message with id 9 was extracted from the queue of NGAP_CLIENT.
09:29:58.326772 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000036A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:58.327030 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00412B000BF299F907020040C000036A2E028040'O
09:29:58.328490 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '68D4F4BE'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E00412B000BF299F907020040C000036A2E028040'O
    }
}
09:29:58.328563 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0268D4F4BE007E00412B000BF299F907020040C000036A2E028040'O
09:29:58.328816 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0268D4F4BE007E00412B000BF299F907020040C000036A2E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.328969 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4043000004000A000200020055000200000026001D1C7E0268D4F4BE007E00412B000BF299F907020040C000036A2E0280400079400F4099F907000000000099F907000001'O
}
09:29:58.531819 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000004000A000200020055000200000026002F2E7E0248DD9126037E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192000000020001'O
} id 7
09:29:58.532311 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0248DD9126037E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:29:58.532611 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.532795 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0248DD9126037E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:29:58.533091 14049 NGAP_Emulation.ttcn:548 Message with id 7 was extracted from the queue of NGAP.
09:29:58.533451 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0248DD9126037E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192'O
09:29:58.533812 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '48DD9126'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192'O
    }
}
09:29:58.535471 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C00001CB54074099F90700000115020101210201005E0192'O
09:29:58.535832 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:58.536292 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:58.536743 14050 ConnHdlr.ttcn:590 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:29:58.537243 14050 ConnHdlr.ttcn:590 Matching on port NGAP succeeded:  matched
09:29:58.537380 14050 ConnHdlr.ttcn:590 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:29:58.537468 14050 ConnHdlr.ttcn:590 Message with id 5 was extracted from the queue of NGAP.
09:29:58.537594 14050 ConnHdlr.ttcn:592 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:58.537824 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:29:58.538015 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.538112 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.538199 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.538252 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.538359 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.538432 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.538498 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:29:58.538561 14049 NGAP_Emulation.ttcn:522 Message with id 10 was extracted from the queue of NGAP_CLIENT.
09:29:58.538655 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:58.538740 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:29:58.540147 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '6310D0F4'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:29:58.540237 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E026310D0F4007E0043'O
09:29:58.540510 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E026310D0F4007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.540724 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E026310D0F4007E00430079400F4099F907000000000099F907000001'O
}
09:29:58.543508 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E029E148CF2047E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
} id 8
09:29:58.543701 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E029E148CF2047E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:58.543818 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.543900 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E029E148CF2047E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:58.543961 14049 NGAP_Emulation.ttcn:548 Message with id 8 was extracted from the queue of NGAP.
09:29:58.544039 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E029E148CF2047E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
09:29:58.544124 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '9E148CF2'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
    }
}
09:29:58.545728 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752215190928500490100'O
09:29:58.545993 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:58.546230 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:58.546452 14050 ConnHdlr.ttcn:594 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:29:58.546695 14050 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:29:58.546793 14050 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '85'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:29:58.546860 14050 ConnHdlr.ttcn:279 Message with id 6 was extracted from the queue of NGAP.
09:29:58.546940 14050 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:58.547047 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:29:58.547116 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.547179 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.547228 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.547277 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.547337 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.547396 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.547454 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:29:58.547510 14049 NGAP_Emulation.ttcn:522 Message with id 11 was extracted from the queue of NGAP_CLIENT.
09:29:58.547574 14050 ConnHdlr.ttcn:608 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        }
    }
}
09:29:58.547586 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:58.547656 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:29:58.549042 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '1B5B499C'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:29:58.549114 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E021B5B499C007E0055'O
09:29:58.549324 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E021B5B499C007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.549474 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E021B5B499C007E00550079400F4099F907000000000099F907000001'O
}
09:29:58.549805 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        }
    }
} id 12
09:29:58.549949 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.550020 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.550078 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.550318 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.550510 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:58.550687 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.550829 14049 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        }
    }
} id 12
09:29:58.550944 14049 NGAP_Emulation.ttcn:522 Message with id 12 was extracted from the queue of NGAP_CLIENT.
09:29:58.551074 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00001CB'O
        }
    }
}
09:29:58.551294 14049 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C00001CB'O
09:29:58.552593 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '2EC07C5F'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C00001CB'O
    }
}
09:29:58.552732 14049 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E022EC07C5F007E004531000BF299F907020040C00001CB'O
09:29:58.552938 14049 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E022EC07C5F007E004531000BF299F907020040C00001CB'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.553087 14049 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403F000004000A0002000200550002000000260019187E022EC07C5F007E004531000BF299F907020040C00001CB0079400F4099F907000000000099F907000001'O
}
09:29:58.769472 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401E000003000A000200020055000200000026000B0A7E02F486937E057E0046'O
} id 9
09:29:58.769851 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F486937E057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:29:58.770062 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.770142 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F486937E057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:29:58.770206 14049 NGAP_Emulation.ttcn:548 Message with id 9 was extracted from the queue of NGAP.
09:29:58.770291 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02F486937E057E0046'O
09:29:58.770379 14049 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'F486937E'O,
        sequenceNumber := '05'O,
        plainNASMessage := '7E0046'O
    }
}
09:29:58.771808 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
09:29:58.771904 14049 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:29:58.772017 14049 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:29:58.772229 14050 ConnHdlr.ttcn:610 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:29:58.772273 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900100000020072000400020000000F400148'O
} id 10
09:29:58.772471 14050 ConnHdlr.ttcn:610 Matching on port NGAP succeeded:  matched
09:29:58.772551 14050 ConnHdlr.ttcn:610 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:29:58.772617 14050 ConnHdlr.ttcn:610 Message with id 7 was extracted from the queue of NGAP.
09:29:58.773558 14049 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:29:58.773681 14049 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:58.773755 14049 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:29:58.773826 14049 NGAP_Emulation.ttcn:548 Message with id 10 was extracted from the queue of NGAP.
09:29:58.774033 14049 NGAP_Emulation.ttcn:587 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.775764 14050 ConnHdlr.ttcn:611 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:58.776876 14050 ConnHdlr.ttcn:624 Matching on port NGAP succeeded:  matched
09:29:58.776970 14050 ConnHdlr.ttcn:624 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:58.777036 14050 ConnHdlr.ttcn:624 Message with id 8 was extracted from the queue of NGAP.
09:29:58.779654 14050 ConnHdlr.ttcn:625 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.780193 14050 - Function f_init_handler finished. PTC terminates.
09:29:58.780265 14050 - Terminating component type ConnHdlr.ConnHdlr.
09:29:58.780320 14050 - Removing unterminated connection between port NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:29:58.780415 14049 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:29:58.780418 14050 - Port NGAP was stopped.
09:29:58.780473 14050 - Removing unterminated connection between port NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:58.780601 14049 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.780675 14050 - Port NGAP_PROC was stopped.
09:29:58.780683 14049 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.780736 14049 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.780760 14050 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(12):CLIENT.
09:29:58.780788 14049 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:58.780843 14050 - Port GTP1U[0] was stopped.
09:29:58.780893 14050 - Port GTP1U[1] was stopped.
09:29:58.780942 14050 - Port GTP1U[2] was stopped.
09:29:58.780971 14048 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT to TC_periodic_registration_updating0(14):GTP1U[0] was closed unexpectedly by the peer.
09:29:58.780991 14050 - Port GTP1U[3] was stopped.
09:29:58.781039 14050 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:29:58.781116 14050 - Port GTP1U_PROC[0] was stopped.
09:29:58.781152 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT was disconnected from TC_periodic_registration_updating0(14):GTP1U[0].
09:29:58.781165 14050 - Port GTP1U_PROC[1] was stopped.
09:29:58.781227 14050 - Port GTP1U_PROC[2] was stopped.
09:29:58.781275 14050 - Port GTP1U_PROC[3] was stopped.
09:29:58.781350 14049 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:29:58.781386 14048 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT_PROC to TC_periodic_registration_updating0(14):GTP1U_PROC[0] was closed unexpectedly by the peer.
09:29:58.781437 14050 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_periodic_registration_updating.
09:29:58.781491 14049 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
09:29:58.781498 14050 - Final verdict of PTC: none
09:29:58.781521 14048 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC was disconnected from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:29:58.781612 13818 C5G_Tests.ttcn:331 PTC with component reference 14 is done.
09:29:58.781626 14049 NGAP_Emulation.ttcn:535 Matching on port NGAP_CLIENT succeeded:  matched
09:29:58.781715 14049 NGAP_Emulation.ttcn:535 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:29:58.781787 13818 C5G_Tests.ttcn:331 Terminating component type C5G_Tests.MTC_CT.
09:29:58.781844 14050 - Disconnected from MC.
09:29:58.781961 14049 NGAP_Emulation.ttcn:535 Message with id 13 was extracted from the queue of NGAP_CLIENT.
09:29:58.781964 13818 C5G_Tests.ttcn:331 Default with id 1 (altstep as_Tguard) was deactivated.
09:29:58.781972 14050 - TTCN-3 Parallel Test Component finished.
09:29:58.782045 13818 C5G_Tests.ttcn:331 Stop timer g_Tguard: 30 s
09:29:58.782205 13818 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_UNIT[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:29:58.782411 13818 C5G_Tests.ttcn:331 Port NGAP_UNIT[0] was stopped.
09:29:58.782632 13818 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_PROC[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:58.782719 13818 C5G_Tests.ttcn:331 Port NGAP_PROC[0] was stopped.
09:29:58.782814 13818 C5G_Tests.ttcn:331 Removing unterminated connection between port TEID0 and GTP1U_EM(12):TEID0.
09:29:58.782892 13818 C5G_Tests.ttcn:331 Port TEID0 was stopped.
09:29:58.782946 14048 GTPv1U_Emulation.ttcnpp:265 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
09:29:58.782987 13818 C5G_Tests.ttcn:331 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:58.783053 13818 C5G_Tests.ttcn:331 Waiting for PTCs to finish.
09:29:58.783103 14048 GTPv1U_Emulation.ttcnpp:265 Port TEID0 was disconnected from mtc:TEID0.
09:29:58.783258 14049 NGAP_Emulation.ttcn:538 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:58.783316 14048 GTPv1U_Emulation.ttcnpp:265 Kill was requested from MC.
09:29:58.783416 14048 GTPv1U_Emulation.ttcnpp:265 Terminating test component execution.
09:29:58.783543 14049 NGAP_Emulation.ttcn:538 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290022000003000A400200020055400200000079400F4099F907000000000099F907000001'O
}
09:29:58.784473 14049 NGAP_Emulation.ttcn:485 Connection of port NGAP_CLIENT to TC_periodic_registration_updating0(14):NGAP was closed unexpectedly by the peer.
09:29:58.784595 14049 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT was disconnected from TC_periodic_registration_updating0(14):NGAP.
09:29:58.784741 14049 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to TC_periodic_registration_updating0(14):NGAP_PROC was closed unexpectedly by the peer.
09:29:58.784860 14049 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from TC_periodic_registration_updating0(14):NGAP_PROC.
09:29:58.784945 14049 NGAP_Emulation.ttcn:485 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
09:29:58.785043 14049 NGAP_Emulation.ttcn:485 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
09:29:58.785123 14049 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
09:29:58.785184 14049 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
09:29:58.785265 14049 NGAP_Emulation.ttcn:485 Kill was requested from MC.
09:29:58.785321 14049 NGAP_Emulation.ttcn:485 Terminating test component execution.
09:29:58.785481 14048 - Function main was stopped. PTC terminates.
09:29:58.785696 14048 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
09:29:58.785859 14048 - Default with id 1 (altstep as_uecups_ind) was deactivated.
09:29:58.785992 14048 - Removing unterminated mapping between port GTP1U and system:GTP1U.
09:29:58.786142 14049 - Function main was stopped. PTC terminates.
09:29:58.786164 14048 - Port GTP1U was unmapped from system:GTP1U.
09:29:58.786262 14049 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:29:58.786370 14048 - Port GTP1U was stopped.
09:29:58.786446 14049 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:29:58.786505 14048 - Port TEID0 was stopped.
09:29:58.786668 14048 - Port CLIENT was stopped.
09:29:58.786745 14048 - Port CLIENT_PROC was stopped.
09:29:58.786816 14048 - Removing unterminated mapping between port UECUPS and system:UECUPS.
09:29:58.787075 14049 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:29:58.787149 14049 - Port NGAP was stopped.
09:29:58.787206 14049 - Port NGAP_CLIENT was stopped.
09:29:58.787506 14049 - Port NGAP_PROC was stopped.
09:29:58.787687 14049 - Port NGAP_UNIT was stopped.
09:29:58.787745 14048 - Port UECUPS was unmapped from system:UECUPS.
09:29:58.787816 14048 - Port UECUPS was stopped.
09:29:58.787853 14049 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:58.787940 14048 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:58.788004 14049 - Final verdict of PTC: none
09:29:58.788012 14048 - Final verdict of PTC: none
09:29:58.788210 14048 - Disconnected from MC.
09:29:58.788273 14048 - TTCN-3 Parallel Test Component finished.
09:29:58.788281 14049 - Disconnected from MC.
09:29:58.788301 13818 C5G_Tests.ttcn:331 Setting final verdict of the test case.
09:29:58.788375 14049 - TTCN-3 Parallel Test Component finished.
09:29:58.788416 13818 C5G_Tests.ttcn:331 Local verdict of MTC: pass
09:29:58.788537 13818 C5G_Tests.ttcn:331 Local verdict of PTC GTP1U_EM(12): none (pass -> pass)
09:29:58.788618 13818 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating-NGAP0(13): none (pass -> pass)
09:29:58.788726 13818 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating0(14): none (pass -> pass)
09:29:58.788842 13818 C5G_Tests.ttcn:331 Test case TC_periodic_registration_updating finished. Verdict: pass
09:29:58.789108 13818 C5G_Tests.ttcn:331 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass'.
09:30:00.859577 13818 C5G_Tests.ttcn:331 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass' was executed successfully (exit status: 0).
09:30:00.859857 13818 C5G_Tests.ttcn:339 Switching to log file `C5G_Tests-TC_ue_context_release_no_pdu_session-809ffe4822d8-mtc-13818.log'
