[1;36m20260505160324692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP[0x5120000066a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP[0x512000006820]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP[0x5120000069a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP[0x512000006b20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP[0x512000006ca0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000006fa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000072a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000075a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000078a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000007ba0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000007ea0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000081a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000084a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP[0x512000008620]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x5120000087a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x512000008920]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP[0x512000008aa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP[0x512000008c20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP[0x512000008da0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP[0x512000008f20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP[0x5120000090a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000093a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000096a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000099a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000009ca0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000009fa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000a2a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000a5a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000a8a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP[0x51200000aa20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x51200000aba0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x51200000ad20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP[0x51200000aea0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP[0x51200000b020]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP[0x51200000b1a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP[0x51200000b320]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP[0x51200000b4a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000b7a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000baa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000bda0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x51200000ffa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000102a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000105a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000108a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000010ba0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP[0x512000010d20]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x512000010ea0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324697 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x512000011020]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP[0x5120000111a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP[0x512000011320]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP[0x5120000114a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP[0x512000011620]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP[0x5120000117a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000011aa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000011da0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000120a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000123a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000126a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x5120000129a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000012ca0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP[0x512000012fa0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP[0x512000013120]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x5120000132a0]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
[1;36m20260505160324699 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP[0x512000013420]{DISABLED_NOTINSTALLED}: Allocated (fsm.c:457)[0;m
% VTY node 'asp' without a '[no] shutdown' command at the end is deprecated, please make sure you update your cfg file for future compatibility.
20260505160324700 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m Available via telnet 127.0.0.1 4242 (telnet_interface.c:88)
[38;5;23m20260505160324700 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) enabling ipaccess BSC mode on 0.0.0.0 with OML 3002 and RSL 3003 TCP ports (ipaccess.c:1025)[0;m
[38;5;33m20260505160324700 [1;33mDLCTRL[0;m[38;5;33m [1;33mNOTICE[0;m[38;5;33m CTRL at 127.0.0.1 4249 (control_if.c:1026)[0;m
[38;5;51m20260505160324700 [1;33mDLMGCP[0;m[38;5;51m [1;33mNOTICE[0;m[38;5;51m MGW(mgw) MGCP client: using endpoint domain '@mgw' (mgcp_client.c:945)[0;m
[1;36m20260505160324701 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m MGW pool with 1 pool members configured, (ignoring MGW configuration in VTY node 'msc'). (osmo_bsc_main.c:869)[0;m
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) To auto-configure msc, adding address 'addr-dyn-msc-default' to cs7 instance 0 address-book implicitly (osmo_bsc_sigtran.c:729)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m Initializing SCCP connection for A/m3ua on cs7 instance 0 (osmo_bsc_sigtran.c:817)
[38;5;45m20260505160324701 [1;31mDLSCCP[0;m[38;5;45m [1;31mERROR[0;m[38;5;45m SS7 instance 0: no primary point-code set, using default point-code (sccp_instance.c:637)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: Using SS7 instance 0, pc:0.23.3 (sccp_instance.c:643)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: Creating AS instance (sccp_instance.c:650)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: Using AS instance as-clnt-A-0-m3ua (sccp_instance.c:661)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: Creating default route (sccp_instance.c:667)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: ASP asp-clnt-msc-0 for m3ua is not associated with any AS, using it (sccp_instance.c:693)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m A-0-m3ua: Using ASP instance asp-clnt-msc-0 (sccp_instance.c:772)[0;m
[38;5;43m20260505160324701 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: Creating SCCP instance (ss7_instance.c:218)[0;m
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) A-0-m3ua: local (BSC) SCCP address: RI=SSN_PC,PC=0.23.3,SSN=BSSAP (osmo_bsc_sigtran.c:870)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) A-0-m3ua: remote (MSC) SCCP address: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_sigtran.c:872)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) A-0-m3ua: binding SCCP user (osmo_bsc_sigtran.c:877)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) A-0-m3ua: local (BSC) SCCP address: RI=SSN_PC,PC=0.23.3,SSN=BSSAP (osmo_bsc_sigtran.c:870)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) A-0-m3ua: remote (MSC) SCCP address: RI=SSN_PC,PC=0.0.2,SSN=BSSAP (osmo_bsc_sigtran.c:872)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) A-0-m3ua: user already bound for this SCCP instance (osmo_bsc_sigtran.c:877)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) A-0-m3ua: local (BSC) SCCP address: RI=SSN_PC,PC=0.23.3,SSN=BSSAP (osmo_bsc_sigtran.c:870)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) A-0-m3ua: remote (MSC) SCCP address: RI=SSN_PC,PC=0.0.3,SSN=BSSAP (osmo_bsc_sigtran.c:872)
20260505160324701 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) A-0-m3ua: user already bound for this SCCP instance (osmo_bsc_sigtran.c:877)
20260505160324701 [1;33mDLCS[0;m [1;33mNOTICE[0;m Initializing SCCP connection for Lb/m3ua on cs7 instance 0 (lb.c:607)
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m Lb-0-m3ua: Using SS7 instance 0, pc:0.23.3 (sccp_instance.c:643)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m Lb-0-m3ua: Using AS instance as-clnt-A-0-m3ua (sccp_instance.c:661)[0;m
[38;5;45m20260505160324701 [1;33mDLSCCP[0;m[38;5;45m [1;33mNOTICE[0;m[38;5;45m Lb-0-m3ua: Using ASP instance asp-clnt-msc-0 (sccp_instance.c:772)[0;m
20260505160324701 [1;33mDLCS[0;m [1;33mNOTICE[0;m Lb: Lb-0-m3ua smlc: local (BSC) SCCP address: RI=SSN_PC,PC=0.23.3,SSN=BSC_BSSAP_LE (lb.c:642)
20260505160324701 [1;33mDLCS[0;m [1;33mNOTICE[0;m Lb: Lb-0-m3ua smlc: remote (SMLC) SCCP address: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:644)
[38;5;49m20260505160324701 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Received NOTIFY Type State Change:AS Inactive () (m3ua.c:720)[0;m
20260505160324702 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) now available: N-PCSTATE ind: pc=2=0.0.2 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160324702 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) now available: N-PCSTATE ind: pc=3=0.0.3 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160324702 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
[38;5;49m20260505160324702 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Received NOTIFY Type State Change:AS Active () (m3ua.c:720)[0;m
[38;5;49m20260505160324702 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(RFC4666 4.5.1) for 0.23.1/0, 0.0.2/0, 0.0.3/0, 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160324702 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
[38;5;43m20260505160324702 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=2=0.0.2,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
[38;5;43m20260505160324702 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=3=0.0.3,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
[38;5;43m20260505160324702 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
[38;5;49m20260505160324703 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160324704 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160324704 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160324704 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
20260505160326214 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_chan_act_to_vamos (logging_vty.c:1266)
20260505160326225 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160326226 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160326226 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160326230 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160326231 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160326231 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160326452 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160326452 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160326452 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160326483 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160326483 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160326483 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[38;5;49m20260505160326707 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160326708 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160326708 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
[1;36m20260505160329099 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329099 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329099 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329100 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329101 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160329102 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329102 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160329103 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329103 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329104 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329105 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329105 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329105 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329105 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160329105 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329106 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329106 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329107 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329107 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329108 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329108 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329109 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329109 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329109 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329109 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329110 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329110 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329110 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329111 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329111 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329111 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329112 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329112 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329112 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329113 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329113 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329114 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160329115 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329115 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329115 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160329115 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160329115 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329116 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329117 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329118 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329118 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329118 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329119 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329120 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329120 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329120 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329121 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329122 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329122 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329122 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse1)[0x51200000aa20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329316 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x51200000ad20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x51200000ad20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x51200000ad20]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse1)[0x51200000aa20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse1)[0x51200000aa20]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160329317 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329318 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329319 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329319 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329319 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x512000008aa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160329320 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329320 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329321 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160329322 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell1)[0x512000008da0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329322 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse1)[0x51200000aa20]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329323 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329324 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160329324 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160329324 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160329324 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329324 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329324 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x51200000ad20]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329324 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse1)[0x51200000aa20]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329325 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329326 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329327 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329328 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329329 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329329 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329329 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329329 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329330 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329331 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329331 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160329331 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x51200000aba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329332 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329332 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329333 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160329333 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329333 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329334 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329335 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160329335 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329336 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329336 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329336 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329337 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329338 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts1-trx0)[0x512000008f20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=1,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts1)[0x512000008c20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329339 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts1-trx0)[0x5120000090a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329340 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts0)[0x5120000093a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts1)[0x5120000096a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329341 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts2)[0x5120000099a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts3)[0x512000009ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329342 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts4)[0x512000009fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts5)[0x51200000a2a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts6)[0x51200000a5a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329343 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts1-trx0-ts7)[0x51200000a8a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse2)[0x512000010d20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000011020]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000011020]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000011020]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse2)[0x512000010d20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse2)[0x512000010d20]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329553 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x51200000aea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160329554 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell2)[0x51200000b1a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160329554 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse2)[0x512000010d20]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329554 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160329555 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160329555 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160329555 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160329555 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329555 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329555 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000011020]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160329555 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse2)[0x512000010d20]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329556 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329557 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160329558 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x512000010ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160329559 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329559 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329560 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329560 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160329561 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329561 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329562 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts2-trx0)[0x51200000b320]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=2,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160329563 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts2)[0x51200000b020]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts2-trx0)[0x51200000b4a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329564 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts0)[0x51200000b7a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts1)[0x51200000baa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts2)[0x51200000bda0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts3)[0x51200000ffa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329565 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts4)[0x5120000102a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts5)[0x5120000105a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts6)[0x5120000108a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160329566 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts2-trx0-ts7)[0x512000010ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;35m20260505160330200 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160331212 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_chan_act_to_vamos() start (logging_vty.c:1266)
[38;5;49m20260505160331232 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160331233 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;32m20260505160332214 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x512000014aa0]{UNUSED}: (type=NONE) attempt from VTY to activate lchan (bts=0,trx=0,ts=1,ss=0) with codec fr (bsc_vty.c:1603)[0;m
[1;32m20260505160332215 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x512000014aa0]{WAIT_ACTIV_ACK}: (type=TCH_F) Timing Advance IE shall be present, but the actual value is not known => assuming 0 (abis_rsl.c:709)[0;m
[1;32m20260505160332230 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x512000014aa0]{WAIT_ACTIV_ACK}: (type=TCH_F) lchan ACTIVATE_FOR_VTY is now active (lchan_fsm.c:1102)[0;m
[1;32m20260505160332230 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x512000014aa0]{ESTABLISHED}: (type=TCH_F) lchan ACTIVATE_FOR_VTY fully established (lchan_fsm.c:321)[0;m
[1;32m20260505160333235 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x512000014aa0]{ESTABLISHED}: (type=TCH_F) attempt from VTY to release lchan (bts=0,trx=0,ts=1,ss=0) (bsc_vty.c:1673)[0;m
[38;5;23m20260505160333255 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160333255 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160333255 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160333255 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160333255 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160333260 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160333260 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160333260 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160333260 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333261 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160333262 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160333263 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160333263 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160333263 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160333263 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160333263 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160333263 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160333263 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
[38;5;49m20260505160336234 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160336234 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160336292 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160336293 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160336293 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160336293 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160336294 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160336294 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160336294 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160336294 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160336295 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336296 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160336297 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160336714 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160338265 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
20260505160338676 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160338677 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160338677 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160338680 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160338681 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160338906 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160338906 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160338906 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160338932 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160338932 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160338932 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[38;5;49m20260505160338938 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160338938 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160338938 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
[1;35m20260505160339817 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160340923 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_mode_modify_to_vamos_fr() start (logging_vty.c:1266)
20260505160342304 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000021820]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160343681 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160343682 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160343743 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160343744 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160343744 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160345360 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160345563 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160345568 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160345571 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160347564 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;23m20260505160347581 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160347581 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160347581 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160347581 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160347581 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160347582 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160347582 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160347582 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160347582 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160347582 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160347583 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160347583 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160347583 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160347583 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160347583 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[38;5;49m20260505160347583 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160347583 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160347583 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160347583 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160347583 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160348684 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160348685 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160350635 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160350636 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160350636 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160350637 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160350637 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160350637 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350638 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160350639 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160352588 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160352588 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
20260505160352912 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160352913 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160352913 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160352917 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160352917 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160353140 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160353140 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160353140 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
[38;5;49m20260505160353156 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160353156 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160353156 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
20260505160353156 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160353156 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160353156 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[1;35m20260505160354005 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160355116 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_mode_modify_to_vamos_hr() start (logging_vty.c:1266)
20260505160356493 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x5120000255a0]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160357920 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160357920 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160357962 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160357962 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160357963 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160359548 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160359754 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160359758 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160359759 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160401760 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;23m20260505160401788 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160401788 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160401788 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160401788 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160401789 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160401793 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160401793 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160401794 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160401794 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160401794 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160401795 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160401796 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160401796 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160401796 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160401796 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160401796 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160401796 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160401796 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160401796 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160401796 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160401796 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160401796 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160401796 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160401796 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160401796 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[38;5;49m20260505160402922 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160402922 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404848 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160404849 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160404849 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160404850 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404850 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160404851 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160404851 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160404851 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404851 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404852 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404853 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160404854 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160404854 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160404854 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160406800 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160406801 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
20260505160407171 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160407172 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160407174 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160407176 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160407176 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160407394 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160407394 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160407394 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160407420 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160407420 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160407420 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[38;5;49m20260505160407435 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160407435 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160407435 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
[1;35m20260505160408284 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160409389 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_assign_to_secondary_lchan_fr() start (logging_vty.c:1266)
[38;5;49m20260505160409703 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160409703 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.2/0 (xua_snm.c:499)[0;m
20260505160410719 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000029320]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160412179 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160412179 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160412242 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160412242 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160412243 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
[1;32m20260505160413731 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-0)[0x5120000270a0]{ESTABLISHED}: (type=TCH_F) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=2,ss=shadow0) (to VAMOS mode) (bsc_vty.c:2185)[0;m
[1;32m20260505160413731 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-2-TCH_F-shadow0)[0x5120000276a0]{UNUSED}: (type=TCH_F) VTY requests re-assignment of (bts=0,trx=0,ts=1,ss=0) to this lchan (to VAMOS mode) TSC 4/2 (bsc_vty.c:2187)[0;m
20260505160413819 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000029320]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[1;32m20260505160416853 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-2-TCH_F-shadow0)[0x5120000276a0]{ESTABLISHED}: (type=TCH_F) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=3,ss=0) (bsc_vty.c:2185)[0;m
[1;32m20260505160416853 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-3-TCH_F-0)[0x5120000279a0]{UNUSED}: (type=TCH_F) VTY requests re-assignment of (bts=0,trx=0,ts=2,ss=shadow0) to this lchan TSC -1/-1 (bsc_vty.c:2187)[0;m
20260505160416934 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000029320]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160417180 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160417180 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160419963 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160420167 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160420172 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160420174 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160422167 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;49m20260505160422180 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160422180 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160423188 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160423189 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160423189 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160423189 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160423189 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;23m20260505160423189 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160423189 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160423189 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160423189 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160423189 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160423194 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160423195 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160423195 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160423195 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423196 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160423197 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160423198 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160423198 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160423198 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160423199 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160423199 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160426237 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160426238 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160426238 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160426238 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160426239 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160426239 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160426239 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426240 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426241 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426242 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426243 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426244 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160426245 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160427182 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160427182 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160428192 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160428201 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
20260505160428605 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160428606 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160428608 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160428610 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160428611 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160428834 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160428834 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160428834 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
[38;5;49m20260505160428846 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160428846 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160428846 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
20260505160428847 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160428847 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160428847 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[1;35m20260505160429727 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160430825 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_assign_to_secondary_lchan_hr() start (logging_vty.c:1266)
20260505160432159 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200002d6a0]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160433612 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160433613 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160433665 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160433665 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160433665 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
[1;32m20260505160435180 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-5-TCH_H-0)[0x51200002c620]{ESTABLISHED}: (type=TCH_H) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=6,ss=shadow0) (to VAMOS mode) (bsc_vty.c:2185)[0;m
[1;32m20260505160435180 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-6-TCH_H-shadow0)[0x51200002cf20]{UNUSED}: (type=TCH_H) VTY requests re-assignment of (bts=0,trx=0,ts=5,ss=0) to this lchan (to VAMOS mode) TSC 4/2 (bsc_vty.c:2187)[0;m
20260505160435268 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200002d6a0]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[1;32m20260505160438306 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-6-TCH_H-shadow0)[0x51200002cf20]{ESTABLISHED}: (type=TCH_H) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=6,ss=1) (bsc_vty.c:2185)[0;m
[1;32m20260505160438306 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-6-TCH_H-1)[0x51200002cda0]{UNUSED}: (type=TCH_H) VTY requests re-assignment of (bts=0,trx=0,ts=6,ss=shadow0) to this lchan TSC -1/-1 (bsc_vty.c:2187)[0;m
20260505160438364 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200002d6a0]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160438613 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160438613 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160441390 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160441599 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160441607 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160441610 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160443602 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;49m20260505160443615 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160443615 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;23m20260505160444631 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160444631 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160444631 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160444631 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160444631 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160444636 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160444636 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160444636 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160444636 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444636 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160444637 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160444637 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160444637 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160444637 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160444637 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160444637 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160444637 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160444637 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160444637 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160444637 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160447692 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447692 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160447693 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447693 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160447694 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160447694 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160447694 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447694 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447695 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160447696 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160448615 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160448615 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160449641 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160449641 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
20260505160450007 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160450008 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160450009 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160450011 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160450011 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160450232 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160450232 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160450232 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
[38;5;49m20260505160450254 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160450255 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160450255 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
20260505160450259 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160450259 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160450259 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[1;35m20260505160451102 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160452211 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_vamos_multiplex_tch_f_tch_f() start (logging_vty.c:1266)
20260505160453580 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200001d920]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160454704 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160454704 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160455013 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160455013 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160455062 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160455062 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160455063 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160457608 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): f_est_lchan_and_mode_modify_to_vamos done (logging_vty.c:1266)
20260505160457841 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200001eb20]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160500013 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160500013 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;32m20260505160500846 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-2-TCH_F-0)[0x51200002fc20]{ESTABLISHED}: (type=TCH_F) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=1,ss=shadow0) (to VAMOS mode) (bsc_vty.c:2185)[0;m
[1;32m20260505160500846 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-1-TCH_F-shadow0)[0x51200002f920]{UNUSED}: (type=TCH_F) VTY requests re-assignment of (bts=0,trx=0,ts=2,ss=0) to this lchan (to VAMOS mode) TSC 4/2 (bsc_vty.c:2187)[0;m
20260505160500905 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200001eb20]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
20260505160504937 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160504938 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160504950 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160504953 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160504955 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160504956 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160504956 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160504956 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
[38;5;49m20260505160505016 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160505017 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160506952 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
20260505160506953 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;23m20260505160506976 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160506976 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160506977 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160506977 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160506977 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160506981 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160506981 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160506982 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160506982 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160506982 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160506982 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160506982 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160506983 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160506983 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160506983 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160506983 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160506983 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160506983 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160506983 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[38;5;49m20260505160510017 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160510017 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510030 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160510031 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160510031 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510031 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160510032 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160510032 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160510032 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510032 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510033 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160510034 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160511986 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160511987 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
20260505160512345 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160512345 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=1) VTY requests BSSMAP RESET (bsc_vty.c:3616)
20260505160512345 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=2) VTY requests BSSMAP RESET (bsc_vty.c:3616)
[38;5;49m20260505160512349 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160512349 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160512571 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.1/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160512571 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160512571 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now available: N-PCSTATE ind: pc=185=0.23.1 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (osmo_bsc_sigtran.c:319)
20260505160512585 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) RESET ACK from MSC: RI=SSN_PC,PC=0.23.1,SSN=BSSAP (osmo_bsc_bssap.c:84)
20260505160512585 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160512585 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is up (a_reset.c:45)
[38;5;49m20260505160512600 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DAVA() for 0.23.6/0 (xua_snm.c:532)[0;m
[38;5;43m20260505160512600 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=unavailable) changed to status 'available' (ss7_route.c:465)[0;m
20260505160512600 [1;33mDLCS[0;m [1;33mNOTICE[0;m now available: N-PCSTATE ind: pc=190=0.23.6 sp_status=ACCESSIBLE remote_sccp_status=AVAILABLE (lb.c:267)
[1;35m20260505160513461 [1;33mDRSL[0;m[1;35m [1;33mNOTICE[0;m[1;35m (bts=0,trx=0) bootstrapping RSL on ARFCN 871 using MCC-MNC 001-01 LAC=1 CID=0 BSIC=10 (osmo_bsc_main.c:320)[0;m
20260505160514569 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): TC_vamos_multiplex_tch_h_tch_h_tch_h_tch_h() start (logging_vty.c:1266)
20260505160515906 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200000ec20]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160517351 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160517351 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160517398 [1;33mDLCS[0;m [1;33mNOTICE[0;m RESET from SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:120)
20260505160517398 [1;33mDRESET[0;m [1;33mNOTICE[0;m Sending RESET ACK to SMLC: RI=SSN_PC,PC=0.23.6,SSN=SMLC_BSSAP (lb.c:80)
20260505160517398 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{CONNECTED}: link up (bssmap_reset.c:83)
20260505160518961 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): f_est_lchan_and_mode_modify_to_vamos done (logging_vty.c:1266)
20260505160519268 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200000fe20]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[1;32m20260505160522291 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-5-TCH_H-1)[0x51200000dd20]{ESTABLISHED}: (type=TCH_H) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=5,ss=shadow0) (to VAMOS mode) (bsc_vty.c:2185)[0;m
[1;32m20260505160522291 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-5-TCH_H-shadow0)[0x51200000dea0]{UNUSED}: (type=TCH_H) VTY requests re-assignment of (bts=0,trx=0,ts=5,ss=1) to this lchan (to VAMOS mode) TSC 4/2 (bsc_vty.c:2187)[0;m
[38;5;49m20260505160522352 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160522352 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
20260505160522389 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x51200000fe20]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
20260505160525768 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000031420]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160527351 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160527352 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160528823 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): f_est_lchan_and_mode_modify_to_vamos done (logging_vty.c:1266)
20260505160529130 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000032620]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[1;32m20260505160532151 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-6-TCH_H-0)[0x51200000e1a0]{ESTABLISHED}: (type=TCH_H) VTY requests re-assignment of this lchan to (bts=0,trx=0,ts=5,ss=shadow1) (to VAMOS mode) (bsc_vty.c:2185)[0;m
[1;32m20260505160532151 [1;33mDCHAN[0;m[1;32m [1;33mNOTICE[0;m[1;32m lchan(0-0-5-TCH_H-shadow1)[0x51200000e020]{UNUSED}: (type=TCH_H) VTY requests re-assignment of (bts=0,trx=0,ts=6,ss=0) to this lchan (to VAMOS mode) TSC 4/2 (bsc_vty.c:2187)[0;m
20260505160532215 [1;33mDLCLS[0;m [1;33mNOTICE[0;m LCLS[0x512000032620]{NO_LCLS}: No GCR set, ignoring APPLY_CFG_CSC (osmo_bsc_lcls.c:388)
[38;5;49m20260505160532354 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160532355 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
20260505160535249 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160535249 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160535251 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160535252 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): MSC instructs BSC to clear channel (logging_vty.c:1266)
20260505160535453 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160535455 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160535457 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160535458 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got BSSMAP Clear Complete (logging_vty.c:1266)
20260505160535459 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160535461 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160535461 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160535464 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160535464 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160535466 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
20260505160535468 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RR Release (logging_vty.c:1266)
20260505160535469 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL Deact SACCH (logging_vty.c:1266)
[38;5;49m20260505160537358 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160537359 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
20260505160537455 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
20260505160537456 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
20260505160537457 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
20260505160537457 [1;33mDLGLOBAL[0;m [1;33mNOTICE[0;m TTCN3 f_logp(): Got RSL RF Chan Rel, sending Rel Ack (logging_vty.c:1266)
[38;5;23m20260505160537486 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m SRVCONN(ts-0-2-RSL,ipa-unit-1234/0/0,r=127.0.0.1:10000<->l=127.0.0.1:3003) connection closed with client (stream_srv.c:779)[0;m
[38;5;23m20260505160537486 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1TS(0:2) failed reading from socket: 0 (ipaccess.c:562)[0;m
[38;5;23m20260505160537487 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;23m20260505160537487 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0) Dropping OML link: link down (bts_ipaccess_nanobts.c:543)[0;m
[38;5;27m20260505160537487 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OML link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160537493 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m E1L(0) Signalling link down (bts_ipaccess_nanobts.c:778)[0;m
[38;5;27m20260505160537494 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 OSMO link (osmo_bsc_main.c:487)[0;m
[38;5;23m20260505160537494 [1;33mDLINP[0;m[38;5;23m [1;33mNOTICE[0;m[38;5;23m (bts=0,trx=0) Dropping RSL link: OML link drop (bts_ipaccess_nanobts.c:514)[0;m
[38;5;27m20260505160537494 [1;31mDLMI[0;m[38;5;27m [1;31mERROR[0;m[38;5;27m (bts=0,trx=0) Lost E1 RSL link (osmo_bsc_main.c:487)[0;m
[1;36m20260505160537495 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:565)[0;m
[1;36m20260505160537495 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bb_transc_fsm.c:371)[0;m
[1;36m20260505160537495 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:566)[0;m
[1;36m20260505160537495 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_rcarrier_fsm.c:373)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537496 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:569)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_channel_fsm.c:297)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:573)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_fsm.c:363)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:574)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_cell_fsm.c:351)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:576)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{ENABLED}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_bts_sm_fsm.c:252)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:577)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nse_fsm.c:324)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event OML_DOWN (bts_ipaccess_nanobts.c:579)[0;m
[1;36m20260505160537497 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: State change to DISABLED_NOTINSTALLED (no timeout) (nm_gprs_nsvc_fsm.c:353)[0;m
[38;5;49m20260505160537498 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160537498 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=185=0.23.1,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160537498 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) now unreachable: N-PCSTATE ind: pc=185=0.23.1 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (osmo_bsc_sigtran.c:311)
20260505160537498 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(msc-0)[0x512000013d20]{DISCONNECTED}: link lost (bssmap_reset.c:91)
20260505160537498 [1;33mDMSC[0;m [1;33mNOTICE[0;m (msc=0) BSSMAP association is down (a_reset.c:54)
[38;5;49m20260505160537499 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA() for 0.23.6/0 (xua_snm.c:499)[0;m
[38;5;43m20260505160537499 [1;33mDLSS7[0;m[38;5;43m [1;33mNOTICE[0;m[38;5;43m 0: RT(dpc=190=0.23.6,mask=0x3fff=7.255.7,prio=5,via=as-clnt-A-0-m3ua,st=available) changed to status 'unavailable' (ss7_route.c:465)[0;m
20260505160537499 [1;33mDLCS[0;m [1;33mNOTICE[0;m now unreachable: N-PCSTATE ind: pc=190=0.23.6 sp_status=INACCESSIBLE remote_sccp_status=UNAVAILABLE_UNKNOWN (lb.c:259)
20260505160537499 [1;33mDRESET[0;m [1;33mNOTICE[0;m bssmap_reset(Lb)[0x5120000141a0]{DISCONNECTED}: link lost (bssmap_reset.c:91)
[38;5;49m20260505160539706 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160539706 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(Response to DAUD) for 0.0.2/0 (xua_snm.c:499)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_sm_fsm.c:96)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_cell_fsm.c:82)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nsvc_fsm.c:83)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_gprs_nse_fsm.c:81)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bts_fsm.c:86)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540547 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:157)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_SM_OP(bts_sm)[0x5120000066a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_sm_fsm.c:184)[0;m
[1;36m20260505160540548 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'CS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS5' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS6' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS7' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=GPRS-CELL(f1) INST=(00,00,ff): GPRS Coding Scheme 'MCS9' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:358)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_CELL_OP(gprs-cell0)[0x5120000069a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:181)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:354)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'GPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'EGPRS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'HOPPING' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CBCH' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ETWS_PN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'PAGING_COORDINATION' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'IPV6_NSVC' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'CCN' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VAMOS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'ABIS_OSMO_PCU' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'BCCH_PWR_RED' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'DYN_TS_SDCCH8' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'OSMUX' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VBS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'VGCS' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS001' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Get Attributes Response: feature 'TWTS002' is supported (abis_nm.c:599)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Max Timing Advance: 63 (bts_ipaccess_nanobts_omlattr.c:63)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): ARI reported sw[0/2]: osmobts is 1.11.0.23-b4ff.202605042029~asan (abis_nm.c:652)[0;m
[1;36m20260505160540548 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BTS(01) INST=(00,ff,ff): Reported variant: osmo-bts-omldummy (abis_nm.c:534)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc1)[0x512000008920]{DISABLED_DEPENDENCY}: Received Event FEATURE_NEGOTIATED (nm_bts_fsm.c:163)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSE_OP(nse0)[0x512000008620]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:177)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:363)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_rcarrier_fsm.c:96)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_NOTINSTALLED}: State change to DISABLED_OFFLINE (no timeout) (nm_bb_transc_fsm.c:99)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540548 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event SW_ACT_REP (bts_ipaccess_nanobts.c:232)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_NOTINSTALLED}: State change to DISABLED_DEPENDENCY (no timeout) (nm_channel_fsm.c:78)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:300)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_GPRS_NSVC_OP(nsvc0)[0x5120000087a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:185)[0;m
[1;36m20260505160540549 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Attribute SW Configuration is unreported (abis_nm.c:557)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'P-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'E-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'R-GSM' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'DCS-1800' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band 'PCS-1900' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '850' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '480' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=RADIO-CARRIER(02) INST=(00,00,ff): Freq. band '450' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:319)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160540549 [1;31mDNM[0;m[1;36m [1;31mERROR[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Attribute Manufacturer Dependent State is unreported (abis_nm.c:557)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/1' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/3' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Ciphering algorithm 'A5/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/H' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'BCCH+SDCCH/4+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'SDCCH/8+CBCH' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel type 'TCH/F or PDCH/F' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR1/FS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR2/EFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'FR3/AFS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR1/HS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'HR3/AHS' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD NT 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1200/75 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 600 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 1k2 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 2.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 4.8 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 9.6 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): Channel mode 'CSD T 14.4 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RTP Feature 'Intermediate Rate 64 kbit/s' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'Dynamic PDCH Activation' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): RSL Feature 'RTP Payload Type 2' is supported (bts_ipaccess_nanobts_omlattr.c:69)[0;m
[1;36m20260505160540549 [1;33mDNM[0;m[1;36m [1;33mNOTICE[0;m[1;36m OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ARI reported sw[0/1]: TRX_PHY_VERSION is Unknown (abis_nm.c:652)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event GET_ATTR_REP (bts_ipaccess_nanobts.c:284)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540549 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event SET_ATTR_ACK (bts_ipaccess_nanobts.c:337)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:173)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_RCARRIER_OP(bts0-trx0)[0x512000006b20]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_rcarrier_fsm.c:259)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m (bts=0,trx=0) IPA RSL CONNECT IP=0.0.0.0 PORT=3003 STREAM=0x00 (abis_nm.c:3088)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:161)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BTS_OP(bts0)[0x512000006820]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bts_fsm.c:264)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event RSL_CONNECT_ACK (bts_ipaccess_nanobts.c:382)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:165)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_BB_TRANSC_OP(bts0-trx0)[0x512000006ca0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_bb_transc_fsm.c:271)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540550 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_DEPENDENCY}: State change to DISABLED_OFFLINE (no timeout) (nm_channel_fsm.c:162)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts0)[0x512000006fa0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts1)[0x5120000072a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts2)[0x5120000075a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts3)[0x5120000078a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts4)[0x512000007ba0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts5)[0x512000007ea0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts6)[0x5120000081a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event OPSTART_ACK (bts_ipaccess_nanobts.c:250)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: Received Event STATE_CHG_REP (bts_ipaccess_nanobts.c:169)[0;m
[1;36m20260505160540551 [1;32mDNM[0;m[1;36m [1;32mINFO[0;m[1;36m NM_CHAN_OP(bts0-trx0-ts7)[0x5120000084a0]{DISABLED_OFFLINE}: State change to ENABLED (no timeout) (nm_channel_fsm.c:204)[0;m
[38;5;49m20260505160542359 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.3/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160542359 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.0.2/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160542502 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.1/0 (xua_snm.c:499)[0;m
[38;5;49m20260505160542502 [1;33mDLM3UA[0;m[38;5;49m [1;33mNOTICE[0;m[38;5;49m 0: ASP(asp-clnt-msc-0) Rx DUNA(transfer prohibited (inaccessible SP)) for 0.23.6/0 (xua_snm.c:499)[0;m
